; ** COPYRIGHT (C) 2007 Realtek CORPORATION
;
; Realtek RTL8169/8110 Family PCI Gigabit Ethernet NIC
; Realtek RTL8168/8111 Family PCI-E Gigabit Ethernet NIC
; Realtek RTL8101 Family PCI-E Fast Ethernet NIC
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
DriverVer   = 06/07/2007,6.194.0607.2007
CatalogFile.NT = netrtx32.cat

[Manufacturer]
%Realtek%     = Realtek, NTx86

[ControlFlags]
ExcludeFromSelect     = *


[Realtek.NTx86]
; 8169 Cardbus Jumbo 7k
%RTL8169Cb7k.DeviceDesc%  = RTL8169Cb7k.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03351154
; 8169 S-32
%SMC9452TX.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_EE221113

; 8169
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&REV_10
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10EC8169
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_14329230
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_14320105
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1432&DEV_9230&SUBSYS_14329604
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_14EAED01
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1371734E
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10BD3202
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10BD3102
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1186&DEV_4300&SUBSYS_11864300
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11864301
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1385311A
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_13855200
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_1737&DEV_1032&SUBSYS_17370024
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_16EC&DEV_0116&SUBSYS_16EC0116
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_187E330B
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1259C113
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1259C112
; 8169 OEM IDs
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00361025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006A1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006E1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00711025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00731025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007D1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007E1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007F1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00791025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009A1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009B1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009F1025 ;acer
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102D147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1032147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1039147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1045147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106C147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106D147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106E147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_180A147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2208147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240A147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_46051961 ;AMOI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F7A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F8A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F9A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03FAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0405A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0406A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_040CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_041CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0449A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_044AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0460A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0461A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0462A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0477A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A0A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A1A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A2A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CBA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CCA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CDA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0526A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0528A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_052AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0542A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0543A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0563A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_057CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0583A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0589A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0600A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0601A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0602A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0604A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_060EA0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_202F161F ;Arima
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10A61043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11E51043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11F51043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81CB104D ;ASUS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0121631 ;ASUS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23031565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23041565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_032B1154 ;Buffalo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03351154 ;Buffalo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F446270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2793270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_272B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_273B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F644270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7842270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7860270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_376C1462 ;CHANNEL
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00031854 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02951558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02971558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03751558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04501558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04511558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04521558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04761558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04801558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A01558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05201558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05601558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05711558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05721558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_06601558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001214C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001714C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3085103C ;Compal
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FF001179 ;Compal
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A15BD ;DFI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F271019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F471019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F521019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F561019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F661019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F671019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B111019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18651019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18731019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18741019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18531019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18031019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B081019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B101019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81691019 ;ECS
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_90221695 ;Epox
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_28211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60011509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60021509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60031509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60041509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60051509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60061509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60071509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60081509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60091509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60101509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60111509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60121509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60131509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60141509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60151509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60161509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60191509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_601F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60251509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60271509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60281509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60291509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60301509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60311509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60321509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60331509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60341509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60351509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60361509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80011509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80021509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80031509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80041509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80051509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80101509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80111509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80121509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80131509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80141509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80151509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80161509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80191509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80241509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80251509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80271509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80281509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80291509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_921F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92451509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92461509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92471509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92481509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92491509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92511509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92521509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92671509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92691509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92701509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92731509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92741509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92751509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92761509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92771509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92781509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92791509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C06105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C07105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C08105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C09105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C10105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C11105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C12105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C13105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C14105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C15105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C16105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C17105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C18105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C19105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C20105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C28105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C29105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C30105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C31105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C38105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C41105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C42105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C43105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C45105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C46105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C47105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C48105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C49105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C51105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C52105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C53105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C55105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C56105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C57105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C59105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C60105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C61105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C62105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C63105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C65105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C69105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C70105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C71105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C72105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C73105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C74105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C75105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C80105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C97105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C98105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C99105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF0105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF1105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF2105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF3105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF4105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10911734 ;FSC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE001458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE011458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0091631 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2A17103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_301F103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3022103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3023103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3081103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308F103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3091103C ;HP
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00071170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000A1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000B1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00201170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500417FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500517FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500617FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500D17FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10EC16F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_811016F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_383617AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1854 ;LG
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_011616EC ;Liteon_USR
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01241071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01711071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80501071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_83171071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80661071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0081631 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00A1631 ;Mitac
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003C1462 ;MS-7003
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006C1462 ;MS-7006
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_008C1462 ;MS-7008
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MS-1016
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02411462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_028C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_033C1462 ;MS-7033
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_062C1462 ;MS-7062
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_094C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_097C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_101C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_108C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11501462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_131C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_133C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_139C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_143C1462 ;MS-7143
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_151C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_166C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_173C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_176C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_177C1462 ;MS-7177
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_183C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_191C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_194C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_19601462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_197C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_204C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_208C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_209C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_210C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_211C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_215C1462 ;MS-7215
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_222C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_223C1462 ;MS-7223
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_229C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_232C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_235C1462 ;MS-7235
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_236C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240C1462 ;MS-7240
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_241C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_242C1462 ;MS-7242
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_248C1462 ;MS-7248
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_251C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_254C1462 ;MS-7254
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_258C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_267C1462 ;MS-7254
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_275C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_279C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_327C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_702C1462 ;MS-6702
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_70941462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_72111462 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_728C1462 ;MS-6728
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_758C1462 ;MS-6758
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_771C1462 ;MS-6771
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_788C1462 ;MS-6788
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_799C1462 ;MS-6799
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0071631 ;MSI
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0081631 ;MS-7168
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0111631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82B61033 ;NEC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_88461033 ;NEC
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_833810F7 ;Panasonic
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0746152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0729152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0730152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058A17FF ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058B17FF ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107D1734 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00B1631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00D1631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0111631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0181631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100817AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A17AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3BE617AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_31558452 ;Topstar
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_5003148C ;TUL
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020B14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020F14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_021214FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107C1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10AC1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10B01734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_51081584 ;Uniwill
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_97101584 ;Uniwill
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_109417C0 ;Wistron


; 8168
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
; 8168B OEM IDs
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1071147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1072147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1073147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1074147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B ;ABIT
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01071025 ;acer
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025 ;acer
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B ;acer
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0631A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0640A0A0 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F ;Arima
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F ;Arima
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F ;Arima
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C ;ASUS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058D17FF ;BENQ
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462 ;CHANNEL
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462 ;CHANNEL
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_369C1462 ;CHANNEL
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462 ;CHANNEL
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940 ;Channel
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05211558 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05911558 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_09021558 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0 ;Compal
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0 ;Compal
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033 ;Compal
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179 ;Compal
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179 ;Compal
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81681019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90A21019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_97501019 ;ECS
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90361695 ;Epox
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60251509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60291509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_602A1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60301509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60311509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60321509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60331509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60341509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60351509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60361509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60371509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60381509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60391509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603A1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603B1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603C1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603D1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603E1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_603F1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60401509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60411509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60421509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60431509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60441509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60451509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60461509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60471509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60481509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60491509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80201509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80211509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80221509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80231509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80241509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80251509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80261509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80271509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80281509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80291509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802A1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802B1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802D1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802E1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_802F1509 ;FIC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734 ;FSC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B ;GATEWAY
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458 ;Gigabyte
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C ;HP
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_00401170 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF ;Inventec
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6068086 ;Intel
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086 ;Intel
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3 ;JETWAY
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01171854 ;LGE
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01181854 ;LGE
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01191854 ;LGE
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854 ;LGE
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47001071 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47011071 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01111462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01211462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01311462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01611462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02211462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02411462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02911462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03211462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_034A1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03611462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03911462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03411462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03711462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_040D1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_04711462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05311462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05711462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33371462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33411462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_359C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_373D1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3EF91462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43141462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43241462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43271462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63701462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80111854 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80161854 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80171854 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462 ;MSI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_18548011 ;MSI_SI
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033 ;NEC
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_056017FF ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD ;Sharp
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1179FF10 ;Toshiba
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11071734 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90761584 ;Uniwill
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF ;XPLORE




; 8101
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC
; 8101E OEM IDs
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B ;ABIT
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B ;ABIT
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025 ;acer
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0 ;AOPEN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F ;Arima
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F ;Arima
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F ;Arima
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462 ;CHANNEL
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462 ;CHANNEL
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462 ;CHANNEL
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940 ;Channel
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179 ;Compal
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179 ;Compal
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81361019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90A01019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90A11019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90A21019 ;ECS
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90371695 ;Epox
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60251509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60291509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602A1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60301509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60311509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60321509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60331509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60341509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60351509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60361509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60371509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60381509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60391509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603A1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603B1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603C1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603D1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603E1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60401509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60411509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60421509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60431509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60441509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60451509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60461509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60471509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60481509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60491509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801A1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801C1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801D1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801B1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801E1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_801F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80201509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80211509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80221509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80231509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80241509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80251509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80261509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80271509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80281509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80291509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802A1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802B1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802C1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802D1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802E1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_802F1509 ;FIC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11071734 ;FSC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11081734 ;FSC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_110A1734 ;FSC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B ;FOXCONN
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B ;Gateway
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA ;GIGABYTE
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3 ;JETWAY
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01151854 ;LGE
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01161854 ;LGE
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD ;MiTAC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_359C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462 ;MSI
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271631 ;NEC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631 ;NEC
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD ;Sharp
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD ;Sharp
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_9015104D ;SONY
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1179FF10 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_97001584 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0 ;Wistron



; 8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC
; 8167 OEM IDs
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009A1025;Acer
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009B1025;Acer
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009F1025;Acer
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1077147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107D147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1080147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1082147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1083147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1087147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1088147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108D147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1423147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1425147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_180A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1C2A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240C147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_13451043;ASUS
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_820D1043;ASUS
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_376C1462;CHANNEL
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_81671019;ECS
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_81691019;ECS
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_90381695;Epox
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60041509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60081509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601C1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601E1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601F1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601F1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60211509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60221509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60231509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60241509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60251509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60271509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60291509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_602A1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_602B1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_602C1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_602D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60301509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60311509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60321509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60331509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60341509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60351509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60361509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60371509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60381509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60391509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603A1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603B1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603C1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603E1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_603F1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60401509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60411509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60421509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60431509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60441509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60451509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60461509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60471509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60481509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60491509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604A1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604B1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604C1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604E1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_604F1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80021509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_801A1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_801B1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80201509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80211509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80221509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80231509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80241509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80251509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80261509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80271509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80281509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80291509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802A1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802B1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802C1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802E1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_802F1509;FIC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C06105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C07105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C08105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C09105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C0F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C10105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C11105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C12105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C13105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C14105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C15105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C16105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C17105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C18105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C19105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C1F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C20105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C21105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C22105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C23105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C24105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C25105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C26105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C27105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C28105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C29105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C2F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C30105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C31105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C32105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C33105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C34105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C35105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C36105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C37105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C38105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C39105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C3F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C41105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C42105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C43105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C44105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C45105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C46105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C47105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C48105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C49105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C51105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C52105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C53105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C54105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C55105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C56105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C57105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C58105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C59105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C5F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C61105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C62105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C63105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C64105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C65105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C66105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C67105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C68105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C69105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C6B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C6C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C6D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C6E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C6F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C70105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C71105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C72105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C73105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C74105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C79105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C80105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C81105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C82105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C83105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C84105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C85105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C86105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C87105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C88105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C89105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C8D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C90105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C91105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C92105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C93105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C94105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C95105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C96105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C97105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C98105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C99105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA0105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA1105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA2105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA3105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA4105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA5105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA6105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA7105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CA8105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAA105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAC105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAD105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAE105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CAF105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC5105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC6105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC7105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC8105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC9105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCA105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCC105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCD105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCE105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCF105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CE8105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CE9105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CEA105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CEB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF0105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF1105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF2105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF3105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF4105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF5105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF6105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF7105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF8105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFA105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFC105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFD105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFE105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CFF105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0D09105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0D19105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0D45105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0D46105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0DF9105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_10D01734;FSC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_302A103C;Gigabyte
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_E0001458;Gigabyte
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_2A37103C;HP
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3022103C;HP
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3023103C;HP
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3024103C;HP
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3028103C;HP
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100717AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100A17AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_383617AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_383A17AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_800D1854;LG
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_80101854;LG
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_197C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_251C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_258C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_263C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_277C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_279C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_280C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_281C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_300C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_305C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_312C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_318C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_33101462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_332C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_333C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_376C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_381C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_70941462;MSI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_18548012;MSI_SI
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_88031033;NEC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_88461033;NEC
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_C0191631;RT_QTA
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_30941297;Shuttle
%RTL8169.DeviceDesc%    = RTL8169.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_008317C0;Wistron

; 8168C
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02




; Realtek
;
; Windows NT specific entry
[RTL8169Cb7k.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, JumboNolimit.reg, s5wol.reg, powersavingautophy.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8168.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, powersavingautopcie.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8136.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, powersavingautopcie.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8168C.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dellsov1.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = OffloadIpv6Lsov2.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 


[RTL8168.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8136.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168C.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168_8136.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


[RTL8169.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8168.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8136.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8168C.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog


;-----------------------------------------------------------------------------
; common base for 10/100/1000 Mb Adapters
;
[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,Ndi\params\AutoDisableGigabit,       ParamDesc,  0, %AutoDisableGigabit%
HKR,Ndi\params\AutoDisableGigabit,       default,    0, "0"
HKR,Ndi\params\AutoDisableGigabit,       type,       0, "enum"
HKR,Ndi\params\AutoDisableGigabit\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoDisableGigabit\enum,  "1",        0, %BatteryRe-Link%
HKR,Ndi\params\AutoDisableGigabit\enum,  "2",        0, %AcBatteryRe-Link%
HKR,,AutoDisableGigabit,0,"0"

HKR,Ndi\params\S3S4WolPowerSaving,       ParamDesc,  0, %S3S4WolPowerSaving%
HKR,Ndi\params\S3S4WolPowerSaving,       default,    0, "0"
HKR,Ndi\params\S3S4WolPowerSaving,       type,       0, "enum"
HKR,Ndi\params\S3S4WolPowerSaving\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S3S4WolPowerSaving\enum,  "1",        0, %Enabled%
HKR,,S3S4WolPowerSaving,0,"0"



[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	   ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	   type,       0, "edit"
HKR,Ndi\params\NetworkAddress,	   default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,	   LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,	   UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,	   Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,	   ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,	   default,    0, "0"
HKR,Ndi\params\*FlowControl,	   type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "1",        0, %Enabled%
HKR,,*FlowControl,0,"0"


[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,	ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,	default,    0, "0"
HKR,Ndi\params\*PriorityVLANTag,	type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,	"0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,	ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,	default,    0, "1"
HKR,Ndi\params\*InterruptModeration,	type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,	"0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,	"1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCardbusJumboFrame,0,"0"


[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[powersavingautophy.reg]
HKR,Ndi\params\AutoLinkDownPhyOff,       ParamDesc,  0, %AutoLinkDownPhyOff%
HKR,Ndi\params\AutoLinkDownPhyOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPhyOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPhyOff,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"1"

;HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
;HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
;HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
;HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
;HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
;HKR,,*LsoV2IPv6,0,"0"

HKR,Ndi\params\*RSS,	ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,	default,    0, "1"
HKR,Ndi\params\*RSS,	type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"0"


[del.reg]
HKR,Ndi\params\JumboFrame
HKR,,JumboFrame

[dellsov1.reg]
HKR,Ndi\params\*LsoV1IPv4
HKR,,*LsoV1IPv4


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "RTL8169"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rtl8169.Service]
DisplayName     = %rtl8169.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlh86.sys
LoadOrderGroup  = NDIS


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[RTL8169.CopyFiles]
Rtlh86.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,Rtlh86.sys,,


[SourceDisksFiles]
Rtlh86.sys = 1,, ; on distribution disk 1


[DestinationDirs]
RTL8169.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Realtek                  = "Realtek"

AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress		 = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit (PowerSaving)"
AutoLinkDownPhyOff       = "Auto Disable PHY (PowerSaving)"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe (PowerSaving)"
S3S4WolPowerSaving       = "Sleep WOL Power Saving"
RSS                      = "Receive Side Scaling"

RTL8169.DeviceDesc       = "Realtek RTL8169/8110 Family PCI Gigabit Ethernet NIC (NDIS 6.0)"
RTL8169Cb7k.DeviceDesc   = "Realtek RTL8169/8110 Family PCI Gigabit Ethernet NIC (NDIS 6.0)"
RTL8168.DeviceDesc       = "Realtek RTL8168B/8111B Family PCI-E Gigabit Ethernet NIC (NDIS 6.0)"
RTL8136.DeviceDesc       = "Realtek RTL8101E Family PCI-E Fast Ethernet NIC (NDIS 6.0)"
RTL8168C.DeviceDesc      = "Realtek RTL8168C/8111C Family PCI-E Gigabit Ethernet NIC (NDIS 6.0)"

SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"


rtl8169.Service.DispName = "Realtek 8169 NT Driver"

DiskDescription 	 = "Realtek Driver Disk 1"


;;;;; InfVer = 1.102
