;*******************************************************************************
; Copyright 2001-2007 Broadcom Corporation.
;
; INF for 32-bit Windows 2K, Windows XP and Windows server 2003
;
; InfVersion   10.62.1.2.C
;
;*******************************************************************************


[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57win32.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer   = 11/30/2007,10.62.1.2

[Manufacturer]
%BRCM% = Broadcom, NTx86.5.1, NTx86.6.0, NTamd64

[ControlFlags]
ExcludeFromSelect = *

[Broadcom.NTamd64]

[Broadcom.NTx86.6.0]
%BCM5700%           =  BCM5700CX.XpInst,         PCI\VEN_14e4&DEV_1644&REV_21
%BCM5700%           =  BCM5700CX.XpInst,         PCI\VEN_14e4&DEV_1644&REV_22
%BCM5700%           =  BCM5700.XpInst,           PCI\VEN_14e4&DEV_1644
%BCM5700FA%         =  BCM5700FA.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%         =  BCM5700FB.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%           =  BCM5701G.XpInst,          PCI\VEN_14e4&DEV_1645
%BCM5701FA%         =  BCM5701FA.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_1646
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16a6
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16C6

; NDIS5.1 Install Device List ---------------------------------------------------
[Broadcom.NTx86.5.1]
%3C1000BT%          =  3C1000BT.XpInst,          PCI\VEN_14e4&DEV_16A6&SUBSYS_110010B7
%3C1000BT%          =  3C1000BT.XpInst,          PCI\VEN_14e4&DEV_16C6&SUBSYS_110010B7
%3C1000T%           =  3C1000T.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100710B7
%3C940BR01%         =  3C940BR01.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_100810B7
%3C996BT%           =  3C996BT.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100610B7
%3C996SX%           =  3C996SX.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100410B7
%3C996T%            =  3C996T.XpInst,            PCI\VEN_14e4&DEV_1644&SUBSYS_100010B7
%3C998SX%           =  3C998SX.XpInst,           PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T.XpInst,            PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T.XpInst,            PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5700%           =  BCM5700CX.XpInst,         PCI\VEN_14e4&DEV_1644&REV_21
%BCM5700%           =  BCM5700CX.XpInst,         PCI\VEN_14e4&DEV_1644&REV_22
%BCM5700%           =  BCM5700.XpInst,           PCI\VEN_14e4&DEV_1644
%BCM5700FA%         =  BCM5700FA.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%         =  BCM5700FB.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%           =  BCM5701G.XpInst,           PCI\VEN_14e4&DEV_1645
%BCM5701FA%         =  BCM5701FA.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_1646
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16a6
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16C6
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_16a7
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_16C7
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW%         =  BCM5703SW.XpInst,         PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%           =  BCM5704G.XpInst,           PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S.XpInst,          PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03331014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705.XpInst,           PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2.XpInst,      PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2.XpInst,      PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,      PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,      PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,      PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M.XpInst,          PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714G.XpInst,           PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780.XpInst,           PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780.XpInst,           PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714G.XpInst,           PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_1669
%BCM5714%           =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03281014
%BCM5714%           =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1679&SUBSYS_03671014
%BCM5714%           =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03861014
%BCM5714%           =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03871014
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_1679
%BCM5714S%          =  BCM5714SWol.XpInst,       PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1
%BCM5722%             =  BCM5750A1G.XpInst,         PCI\VEN_14e4&DEV_165A
%BCM5750A1%         =  BCM5750A1F3MEA.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3E.XpInst,      PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3MEA.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1F3MFD.XpInst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3MFD.XpInst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M.XpInst,        PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750A1SPECIAL.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_108B1734
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_03301014
%BCM5750A1%         =  BCM5750MHALe.XpInst,    PCI\VEN_14e4&DEV_1601&SUBSYS_202017AA
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1G.XpInst,        PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1DMOBILE%         =  BCM5750A1DESTAR.XpInst,      PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1672&SUBSYS_02021028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_02001028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_024A1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.XpInst,      PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1674
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_01f81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_02041028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_02621028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_02631028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_02641028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1674&SUBSYS_02651028

%BCM5906%           =  BCM5906MDESTAR.XpInst,        PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906%           =  BCM5906MDESTAR.XpInst,        PCI\VEN_14e4&DEV_1713&SUBSYS_02091028
%BCM5906%           =  BCM5906MDESTAR.XpInst,        PCI\VEN_14e4&DEV_1713&SUBSYS_02271028

%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750MHALe.XpInst,       PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHALe.XpInst,       PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028

%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_024E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167B&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_021D1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_021E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_02141028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_169B&SUBSYS_02201028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,  PCI\VEN_14e4&DEV_1672&SUBSYS_01f71028
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750A1F.XpInst,       PCI\VEN_14e4&DEV_167E
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750FHAL.XpInst,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1STSP%     =  BCM5750A1STSP.XpInst,     PCI\VEN_14e4&DEV_1659&SUBSYS_3260103c
%BCM5750B0%         =  BCM5750B0MHAL.XpInst,        PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_10
%BCM5750B0F%        =  BCM5750B0MFHAL.XpInst,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_10
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01
%BCM5754%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1672
%BCM5755%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1673
%BCM5755%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167B
%BCM5755%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5750A1.XpInst,    PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5755%           =  BCM5750A1.XpInst,    PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5750A1HALeStar.XpInst,     PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101c17AA
%BCM5755%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA
%BCM5754%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167A&SUBSYS_10fe1734
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5750A1F3E.XpInst,      PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A&SUBSYS_101f17AA
%BCM5787%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169B&SUBSYS_11291734
%BCM5787%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5750A1HALeStar.XpInst,      PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787%           =  BCM5750A1F3E.XpInst,       PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1693
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5750A1MBDFS.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01301025
%BCM5787%           =  BCM5750MHALe.XpInst,       PCI\VEN_14e4&DEV_1693&SUBSYS_203017AA
%BCM5787%           =  BCM5750MHALe.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787%           =  BCM5750MHALe.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_3D7F17AA
%BCM5787%           =  BCM5750A1F3MEA.XpInst,    PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf

%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88621033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88631033
%BCM5787%           =  BCM5750A1F3MMFDCQ29902.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88831033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88921033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88A11033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88A21033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88A51033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88A91033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88B01033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_88B91033

%BCM5787%           =  BCM5750MHALe.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_20D517aa
%BCM5787F%          =  BCM5750A1FeStar.XpInst,        PCI\VEN_14e4&DEV_167F
%BCM5788%           =  BCM5788.XpInst,              PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788F1.XpInst,         PCI\VEN_14e4&DEV_169C&SUBSYS_123c10cf
%BCM5788%           =  BCM5788F1.XpInst,         PCI\VEN_14e4&DEV_169C&SUBSYS_12f710cf
%BCM5788%           =  BCM5788F1MFD.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788F1MFD.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789F1.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169d
%BCM5789%           =  BCM5789F1MFD.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789F1MFD.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789F1MFD.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789F1MFD.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789F1MFD.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169d&SUBSYS_0280107b
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169d&SUBSYS_100517AA
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169d&SUBSYS_060017FF
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_16DD
%BCM5750B0%         =  BCM5750B0M.XpInst,        PCI\VEN_14e4&DEV_16FF
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170E
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170E&SUBSYS_05451014
%BCM5906%           =  BCM5906.XpInst,           PCI\VEN_14e4&DEV_1712
%BCM5906%           =  BCM5906M.XpInst,          PCI\VEN_14e4&DEV_1713
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3D7E17AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906%           =  BCM5906MFJ.XpInst,        PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%OEM1_DEV1%         =  OEM1_DEV1.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_00d11028
%OEM1_DEV1%         =  OEM1_DEV1.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_102814e4
%OEM1_DEV2%         =  OEM1_DEV2.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_01091028
%OEM1_DEV3%         =  OEM1_DEV3.XpInst,         PCI\VEN_14e4&DEV_1644&SUBSYS_010A1028
%OEM1_DEV4%         =  OEM1_DEV4XP.XpInst,       PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV4%         =  OEM1_DEV4XP.XpInst,       PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV4%         =  OEM1_DEV4XP.XpInst,       PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV4%         =  OEM1_DEV4XP.XpInst,       PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028
%OEM1_DEV4%         =  OEM1_DEV4XP.XpInst,       PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028
%OEM1_DEV5%         =  OEM1_DEV5XP.XpInst,       PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5XP.XpInst,       PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%         =  OEM1_DEV5XP.XpInst,       PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5XP.XpInst,       PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01841028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
%OEM1_DEV6%         =  OEM1_DEV6XP.XpInst,       PCI\VEN_14e4&DEV_1653&SUBSYS_86531028

; End of NDIS5.1 Install Device List ---------------------------------------------------


;*******************************************************************************
; 32-bit Windows XP NDIS5.1 Install sections.
;*******************************************************************************
[BCM5700.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5700CX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700CX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5701.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5701G.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701G.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5702.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5702.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5703.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5703G.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703G.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5704.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5704G.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS, DelReg.ParamsC
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704G.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5705.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750A1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1G.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.ParamsC
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1G.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1eStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1eStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1HAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1HAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1HALeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1HALeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5714.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5714G.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic, DelReg.ParamsC
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714G.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5780.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSndJumboCombo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5780.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5714S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5714SWol.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714SWol.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5714SHAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714SHAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750A1STSP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1STSP.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5789.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo , DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5789F1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo , DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789F1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5789F1MFD.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo , DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789F1MFD.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750B0MHAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750B0MHAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750B0MFHAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750B0MFHAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750B0M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750B0M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



;[BCM5750B0MF.XpInst.NTx86]
;Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
;DelReg          = DelReg.Jumbo
;DelReg          = DelReg.ClockControl
;AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
;CopyFiles       = CopyFile.XpSys32
;BusType         = 5

;[BCM5750B0MF.XpInst.NTx86.Services]
;AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750A1SPECIAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xSPECIAL, ParamsCSPECIAL, ParamsWOLeStar, ParamsWireSpeedSPECIAL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1SPECIAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750A1M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1MeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1MeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750A1MBDFS.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1MBDFS.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750MHAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750MHAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750MHALe.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750MHALe.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750A1F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1FeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1FeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750FHAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750FHAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750A1DMOBILE.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, DMobileXP.Params
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1DMOBILE.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1DMESTAR.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, DMobileXP.Params, Estar, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1DMESTAR.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750A1DESTAR.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, DMobileXP.Params, Estar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1DESTAR.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5750A1F3.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750A1F3E.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3E.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750A1F3MFD.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3MFD.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5750A1F3M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1F3MEA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3MEA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5750A1F3MMFD.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3MMFD.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1F3MMFDCQ29902.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM, ParamsCQ29902
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3MMFDCQ29902.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5750A1F3MMFDeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3MMFDeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705F.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705A2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705A2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705A2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705MA2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705MA2F2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2F2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5705MA2F2MFD.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2F2MFD.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5901.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5901.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5901.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5788.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5906.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5906MLEN.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd , DelReg.Wol
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906MLEN.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5906MFJ.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC100, ParamsWOLeStarAuto, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906MFJ.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5906MDESTAR.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, 5906DMobileXP.Params, Estar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906MDESTAR.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[BCM5906M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5788F1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788F1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5788F1MFD.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788F1MFD.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[BCM5700FB.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FB.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5700FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5701FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5703S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5703SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5704S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[BCM5704SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C996T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996T.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


[3C996SX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996SX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C996BT.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996BT.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C998T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C998T.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C998SX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C998SX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C999T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C999T.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C1000T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C1000T.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C940BR01.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C940BR01.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[3C1000BT.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C1000BT.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[OEM1_DEV1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[OEM1_DEV2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[OEM1_DEV3.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV3.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[OEM1_DEV4XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5702.Params, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV4XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog



[OEM1_DEV5XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, OEM1_DEV5.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV5XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog




[OEM1_DEV6XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, OEM1_DEV6.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV6XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

;*******************************************************************************
; End of 32-bit Windows XP NDIS5.1 Install sections.
;*******************************************************************************

; NDIS5 Install Device List ---------------------------------------------------
[Broadcom]
%3C1000BT%          =  3C1000BTA3.Inst,        PCI\VEN_14e4&DEV_16C6&SUBSYS_110010B7
%3C1000BT%          =  3C1000BT.Inst,          PCI\VEN_14e4&DEV_16A6&SUBSYS_110010B7
%3C1000T%           =  3C1000T.Inst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100710B7
%3C940BR01%         =  3C940BR01.Inst,         PCI\VEN_14e4&DEV_1645&SUBSYS_100810B7
%3C996BT%           =  3C996BT.Inst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100610B7
%3C996SX%           =  3C996SX.Inst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100410B7
%3C996T%            =  3C996T.Inst,            PCI\VEN_14e4&DEV_1644&SUBSYS_100010B7
%3C998SX%           =  3C998SX.Inst,           PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T.Inst,            PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T.Inst,            PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5700%           =  BCM5700.Inst,           PCI\VEN_14e4&DEV_1644
%BCM5700FA%         =  BCM5700FA.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%         =  BCM5700FB.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%           =  BCM5701G.Inst,           PCI\VEN_14e4&DEV_1645
%BCM5701FA%         =  BCM5701FA.Inst,         PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%           =  BCM5702A3.Inst,         PCI\VEN_14e4&DEV_16C6
%BCM5702%           =  BCM5702.Inst,           PCI\VEN_14e4&DEV_1646
%BCM5702%           =  BCM5702.Inst,           PCI\VEN_14e4&DEV_16A6
%BCM5703%           =  BCM5703G.Inst,         PCI\VEN_14e4&DEV_16C7
%BCM5703%           =  BCM5703G.Inst,           PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703G.Inst,           PCI\VEN_14e4&DEV_16A7
%BCM5703S%          =  BCM5703SA3.Inst,        PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.Inst,          PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.Inst,          PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703SW%         =  BCM5703SW.Inst,         PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%           =  BCM5704G.Inst,           PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S.Inst,          PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5704SW%         =  BCM5704SW.Inst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03331014
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2.Inst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705.Inst,           PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F.Inst,          PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F.Inst,          PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705F%          =  BCM5705F.Inst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705F%          =  BCM5705F.Inst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2.Inst,      PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2.Inst,      PCI\VEN_14e4&DEV_165e&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2MFD.Inst,      PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2MFD.Inst,      PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2MFD.Inst,      PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2.Inst,        PCI\VEN_14e4&DEV_165e
%BCM5705M%          =  BCM5705MA2.Inst,        PCI\VEN_14e4&DEV_165e&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2.Inst,        PCI\VEN_14e4&DEV_165e&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M.Inst,          PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714G.Inst,           PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714.Inst,           PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780.Inst,           PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780.Inst,           PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714G.Inst,           PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714.Inst,           PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714.Inst,           PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S.Inst,          PCI\VEN_14e4&DEV_1669
%BCM5714S%          =  BCM5714S.Inst,          PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S.Inst,          PCI\VEN_14e4&DEV_1679
%BCM5722%           =  BCM5750A1G.Inst,         PCI\VEN_14e4&DEV_165A
%BCM5714S%          =  BCM5714SWol.Inst,       PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1
%BCM5750A1%         =  BCM5750A1F3E.Inst,      PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3MEA.Inst,      PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3MEA.Inst,      PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3MFD.Inst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3MFD.Inst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1F3MMFDeStar.Inst,      PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3MMFDeStar.Inst,      PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_108B1734
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1600&SUBSYS_03301014
%BCM5750A1%         =  BCM5750MHALe.Inst,      PCI\VEN_14e4&DEV_1601&SUBSYS_202017AA
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1G.Inst,         PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1DMOBILE%         =  BCM5750A1DESTAR.Inst,      PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1672&SUBSYS_02021028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_02001028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_024A1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1672&SUBSYS_01f71028
%BCM5750A1%         =  BCM5750A1MeStar.Inst,      PCI\VEN_14e4&DEV_1674
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_01f81028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_02041028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_02621028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_02631028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_02641028
%BCM5750A1DMOBILE%         =  BCM5750A1DMESTAR.Inst,      PCI\VEN_14e4&DEV_1674&SUBSYS_02651028

%BCM5906%           =  BCM5906MDESTAR.Inst,        PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906%           =  BCM5906MDESTAR.Inst,        PCI\VEN_14e4&DEV_1713&SUBSYS_02091028
%BCM5906%           =  BCM5906MDESTAR.Inst,        PCI\VEN_14e4&DEV_1713&SUBSYS_02271028

%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750A1MeStar.Inst,        PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1MeStar.Inst,        PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M.Inst,        PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750MHALe.Inst,       PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHALe.Inst,       PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_024E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167B&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_021D1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_021E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_167A&SUBSYS_02141028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.Inst,  PCI\VEN_14e4&DEV_169B&SUBSYS_02201028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.Inst,  PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1F%        =  BCM5750A1F.Inst,        PCI\VEN_14e4&DEV_167E
%BCM5750A1F%        =  BCM5750A1F.Inst,        PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F.Inst,        PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750A1F.Inst,        PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750FHAL.Inst,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1STSP%     =  BCM5750A1STSP.Inst,     PCI\VEN_14e4&DEV_1659&SUBSYS_3260103C
%BCM5750B0%          =  BCM5750B0MHAL.Inst,        PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_10
%BCM5750B0F%        =  BCM5750B0MFHAL.Inst,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_10
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_167D&REV_00
%BCM5750%           =  BCM5750.Inst,           PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01
%BCM5754%           =  BCM5750A1MeStar.Inst,        PCI\VEN_14e4&DEV_1672
%BCM5755%           =  BCM5750A1MeStar.Inst,        PCI\VEN_14e4&DEV_1673
%BCM5755%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_167B
%BCM5755%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5750A1.Inst,    PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5755%           =  BCM5750A1.Inst,    PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_101c17AA
%BCM5755%           =  BCM5750A1HALeStar.Inst,      PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA
%BCM5754%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_167A&SUBSYS_10fe1734
%BCM5782%           =  BCM5782.Inst,           PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5782.Inst,           PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5782.Inst,           PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5782.Inst,           PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c
%BCM5786%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5750A1F3E.Inst,      PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5786%           =  BCM5750A1eStar.Inst,      PCI\VEN_14e4&DEV_169A&SUBSYS_101f17AA
%BCM5787%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5750A1eStar.Inst,         PCI\VEN_14e4&DEV_169B&SUBSYS_11291734
%BCM5787%           =  BCM5750A1HALeStar.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5750A1HALeStar.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5750A1HALeStar.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787%           =  BCM5750A1F3E.Inst,        PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5750A1MeStar.Inst,         PCI\VEN_14e4&DEV_1693
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5750A1MBDFS.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_01301025
%BCM5787%           =  BCM5750MHALe.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_203017AA
%BCM5787%           =  BCM5750MHALe.Inst,      PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787%           =  BCM5750MHALe.Inst,      PCI\VEN_14e4&DEV_1693&SUBSYS_3D7F17AA
%BCM5787%           =  BCM5750A1F3MEA.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf
%BCM5787%           =  BCM5750A1F3MMFDCQ29902.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88621033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88631033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A11033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88921033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A21033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A51033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A91033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B01033
%BCM5787%           =  BCM5750A1F3MMFDeStar.Inst,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B91033

%BCM5787%           =  BCM5750MHALe.Inst,         PCI\VEN_14e4&DEV_1693&SUBSYS_20D517aa
%BCM5787F%          =  BCM5750A1FeStar.Inst,        PCI\VEN_14e4&DEV_167F
%BCM5788%           =  BCM5788.Inst,             PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788F1.Inst,         PCI\VEN_14e4&DEV_169c&SUBSYS_123c10cf
%BCM5788%           =  BCM5788F1.Inst,         PCI\VEN_14e4&DEV_169c&SUBSYS_12f710cf
%BCM5788%           =  BCM5788F1MFD.Inst,         PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788F1MFD.Inst,         PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5788%           =  BCM5788.Inst,           PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%           =  BCM5788.Inst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788.Inst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788.Inst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788.Inst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_169d
%BCM5789%           =  BCM5789F1.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5789%           =  BCM5789F1MFD.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789F1MFD.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789F1MFD.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789F1MFD.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789F1MFD.Inst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_169d&SUBSYS_0280107b
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_169d&SUBSYS_100517AA
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_169d&SUBSYS_060017FF
%BCM5789%           =  BCM5789.Inst,           PCI\VEN_14e4&DEV_16DD
%BCM5750B0%         =  BCM5750B0M.Inst,        PCI\VEN_14e4&DEV_16FF
%BCM5901%           =  BCM5901.Inst,           PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901.Inst,           PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901.Inst,           PCI\VEN_14e4&DEV_170e
%BCM5901%           =  BCM5901.Inst,           PCI\VEN_14e4&DEV_170E&SUBSYS_05451014
%BCM5906%           =  BCM5906eStar.Inst,           PCI\VEN_14e4&DEV_1712
%BCM5906%           =  BCM5906MeStar.Inst,          PCI\VEN_14e4&DEV_1713
%BCM5906%           =  BCM5906MLEN.Inst,       PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906%           =  BCM5906MLEN.Inst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3D7E17AA
%BCM5906%           =  BCM5906MLEN.Inst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906%           =  BCM5906MLEN.Inst,       PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906%           =  BCM5906MFJ.Inst,        PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%OEM1_DEV1%         =  OEM1_DEV1.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_00d11028
%OEM1_DEV1%         =  OEM1_DEV1.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_102814e4
%OEM1_DEV2%         =  OEM1_DEV2.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_01091028
%OEM1_DEV3%         =  OEM1_DEV3.Inst,         PCI\VEN_14e4&DEV_1644&SUBSYS_010A1028
%OEM1_DEV4%         =  OEM1_DEV4.Inst,         PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028
%OEM1_DEV5%         =  OEM1_DEV5.Inst,         PCI\VEN_14e4&DEV_165D&SUBSYS_019c1028
%OEM1_DEV5%         =  OEM1_DEV5.Inst,         PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5.Inst,         PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%         =  OEM1_DEV5.Inst,         PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5.Inst,         PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
;%OEM1_DEV6%        =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01841028
;%OEM1_DEV6%        =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
;%OEM1_DEV6%        =  BCM5750A1.Inst,         PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
%OEM1_DEV6%         =  OEM1_DEV6.Inst,         PCI\VEN_14e4&DEV_1653&SUBSYS_86531028
%OEM1_DEV7%         =  OEM1_DEV4.Inst,         PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV7%         =  OEM1_DEV4.Inst,         PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV7%         =  OEM1_DEV4.Inst,         PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV7%         =  OEM1_DEV4.Inst,         PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028




; End of NDIS5 Install Device List -----------------------------------------------

;*******************************************************************************
; 32-bit Windows NDIS5 Win2000 Install sections.
;*******************************************************************************
[BCM5700.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5701.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5701G.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701G.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5702.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5702A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5703.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5703G.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703G.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5703A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5704.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5704G.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS, DelReg.ParamsC
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704G.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5705.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5705A2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705A2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705A2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5782.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5782.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5782.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5788.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5906.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5906eStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906eStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5906MLEN.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.Wol
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906MLEN.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5906MFJ.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC100, ParamsWOLeStarAuto, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906MFJ.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5906MDESTAR.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload
AddReg          = NtAddReg, BCM5788.Params, ParamsNt8021p, ParamsNtW9xMOBILE, ParamsC100, ParamsWOLNS, 5906DMobileXP.Params, eStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906MDESTAR.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5906M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5906MeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906MeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5788F1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788F1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5788F1MFD.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788F1MFD.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog




[BCM5705M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5705MA2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5705MA2F2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2F2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5705MA2F2MFD.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2F2MFD.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog




[BCM5901.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5901.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5901.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5705F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705F.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5700FB.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FB.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5700FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5701FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5703S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5703SA3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SA3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5703SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5704S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5704SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5750.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5789.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5789F1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789F1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5789F1MFD.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789F1MFD.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog





[BCM5750A1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1G.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.ParamsC
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC1G, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1G.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog
[BCM5750A1eStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1eStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1HAL.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1HAL.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1HALeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1HALeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5714.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsJumbo, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5714.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5714G.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic, DelReg.ParamsC
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC1G, ParamsWireSpeed, ParamsJumbo, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5714G.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5780.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5780.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5714S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5714S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5714SWol.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5714SWol.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1STSP.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1STSP.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog




[BCM5750A1M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1MeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1MeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1MBDFS.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1MBDFS.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog




[BCM5750MHAL.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM,  ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750MHAL.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750MHALe.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM,  ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750MHALe.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750B0MHAL.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750B0MHAL.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5750B0MFHAL.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750B0MFHAL.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5750B0M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750B0M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



;[BCM5750B0MF.Inst.NT]
;Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
;DelReg          = DelReg.Jumbo
;AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsM
;CopyFiles       = CopyFile.NtSys
;BusType         = 5

;[BCM5750B0MF.Inst.NT.Services]
;AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5750A1F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1FeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1FeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750FHAL.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750FHAL.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[BCM5750A1DMOBILE.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, DMobile.Params
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1DMOBILE.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1DMESTAR.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xMOBILE, ParamsC, DMobile.Params, ParamsWOLNS, Estar, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1DMESTAR.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1DESTAR.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = NtAddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xMOBILE, ParamsC, DMobile.Params, ParamsWOLNS, Estar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1DESTAR.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1F3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1F3E.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3E.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1F3MFD.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3MFD.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog




[BCM5750A1F3M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[BCM5750A1F3MEA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3MEA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1F3MMFD.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3MMFD.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1F3MMFDCQ29902.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsCQ29902
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3MMFDCQ29902.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5750A1F3MMFDeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3MMFDeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C996T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996T.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C996SX.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996SX.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C996BT.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996BT.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C1000T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000T.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C940BR01.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C940BR01.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C998T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C998T.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C998SX.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C998SX.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C999T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C999T.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C1000BT.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000BT.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[3C1000BTA3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000BTA3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[OEM1_DEV1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[OEM1_DEV2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[OEM1_DEV3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[OEM1_DEV4.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, OEM1_DEV4.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV4.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog



[OEM1_DEV5.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5705M.Params, OEM1_DEV5.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV5.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog


[OEM1_DEV6.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5705.Params, OEM1_DEV6.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV6.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

;*******************************************************************************
; End of 32-bit Windows NDIS5 Win2000 Install sections.
;*******************************************************************************


;*******************************************************************************
; 32-bit Windows Xp common sections.
;*******************************************************************************

[Xp32AddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Xp32EventLog]
AddReg = Xp32AddEventLogReg

[Xp32AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57xp32.sys"
HKR, , TypesSupported  , 0x00010001, 7


[BCM5700.Xp32AddService]
DisplayName    = %BCM5700%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS
Addreg         = bcmPnpInstallReg


;*******************************************************************************
; Windows 2k common sections.
;*******************************************************************************

[NtAddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[NtEventLog]
AddReg = NtAddEventLogReg

[NtAddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57w2k.sys"
HKR, , TypesSupported  , 0x00010001, 7

[BCM5700.AddService]
DisplayName    = %BCM5700%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS
Addreg         = bcmPnpInstallReg

;*******************************************************************************
; Windows 2k and Xp common section.
;*******************************************************************************
[bcmPnpInstallReg]
HKR,,product_version,0,"12.0.0"

;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5700.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "360"
HKR, , TxCoalescingTicks,        0, "360"
HKR, , RxMaxCoalescedFrames,     0, "15"
HKR, , TxMaxCoalescedFrames,     0, "75"


[BCM5701.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5702.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5703.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5704.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5901.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[OEM1_DEV4.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV5.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV6.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[DMobile.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"


[DMobileXP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"

[5906DMobileXP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"

[BCM5782.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[ParamsNt]
HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , %TaskOffload%
HKR, Ndi\Params\TaskOffloadCap,      default,   , "63"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,         , %TaskOffload_None%
HKR, Ndi\Params\TaskOffloadCap\enum, 42,        , %TaskOffload_Rx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 21,        , %TaskOffload_Tx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 63,        , %TaskOffload_Rx_Tx_Chksum%

[ParamsNT8021p]
HKR, Ndi\Params\Enable8021p,      ParamDesc, , %QOS_8021p%
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,         , %QOS_8021p_Disable%
HKR, Ndi\Params\Enable8021p\enum, 1,         , %QOS_8021p_Enable%

[ParamsNtW9x]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"


[ParamsNtW9xFJ]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "0"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"



[ParamsNtW9xMOBILE]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%


[ParamsNtW9xSPECIAL]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%


[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "0"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%



[ParamsWireSpeedSPECIAL]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%


[ParamsC]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsCSPECIAL]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%

[ParamsC100]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsC1G]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 8200,      , %Speed_Duplex_1000Mb_Fd%

[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsWOLeStar]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,         , %WolSpeed_LowestAvail%
HKR, , WolSpeed,                 0, "256"

[ParamsWOLeStarAuto]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,         , %WolSpeed_LowestAvail%
HKR, , WolSpeed,                 0, "0"

[Estar]
HKR, , WolSpeed,                 0, "256"

[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsCQ29902]
HKR, , CQ29902Errata,          0, "0"

[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsLgSnd]
HKR, Ndi\Params\LargeSendOffload,    ParamDesc, , %TaskOffload_LargeSend%
HKR, Ndi\Params\LargeSendOffload,    default,   , "1"
HKR, Ndi\Params\LargeSendOffload,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffload\enum, 0,        , %TaskOffload_LargeSend_Disable%
HKR, Ndi\Params\LargeSendOffload\enum, 1,        , %TaskOffload_LargeSend_Enable%

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

[ParamsFlow]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%


[ParamsLgSndJumboCombo]
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 3,        , %TaskOffload_LargeSend_Disable_JumboEnable4500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 4,        , %TaskOffload_LargeSend_Disable_JumboEnable6000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 5,        , %TaskOffload_LargeSend_Disable_JumboEnable7500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 6,        , %TaskOffload_LargeSend_Disable_JumboEnable9000%

[ParamsWOLMagic]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%


;*******************************************************************************
; DriverInfo section.
;*******************************************************************************

[DriverInfo]
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,BaseDriverFileName,,%BaseDriverFileName%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,BaseDriverFileVersion,,%BaseDriverFileVersion%



;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType

[DelReg.Wol]
HKR, Ndi\Params\WolSpeed
HKR, Ndi\Params\WakeUpModeCap

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.WolMagic]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

[DelReg.ClockControl]
HKR, ,ClockControl

[DelReg.LAA]
HKR, Ndi\params\NetworkAddress
HKR, , NetworkAddress

[DelReg.TaskOffload]
HKR, Ndi\Params\TaskOffloadCap

[DelReg.ParamsC]
HKR, Ndi\Params\RequestedMediaType

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile.XpSys32 = 12
CopyFile.NtSys  = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57xp32.sys = 1
b57w2k.sys = 1

[CopyFile.XpSys32]
b57xp32.sys,,,1

[CopyFile.NtSys]
b57w2k.sys,,,1



;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1F          = "Broadcom NetXtreme Fast Ethernet"
BCM5714             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5722             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5786             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5787F            = "Broadcom NetLink (TM) Fast Ethernet"
BCM5755             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5754             = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1STSP       = "Embedded Broadcom NetXtreme 5721 PCI-E Gigabit NIC"

BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"

BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"

3COMCommon   = "3Com Gigabit 10/100/1000 NIC"
3C996T              = "3Com 3C996 10/100/1000 Server NIC"
3C996SX             = "3Com 3C996 Gigabit Fiber-SX Server NIC"
3C996BT             = "3Com 3C996B Gigabit Server NIC"
3C1000T             = "3Com 3C1000 Gigabit NIC"
3C940BR01           = "3Com 3C940 Gigabit LOM"
3C998T              = "3Com Dual Port 10/100/1000 PCI-X Server NIC"
3C998SX             = "3Com Dual Port 1000-SX PCI-X Server NIC"
3C999T              = "3Com Quad Port 10/100/1000 PCI-X Server NIC"
3C1000BT            = "3Com 10/100/1000 PCI"

OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1DSF      = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF    = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT      = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1DMOBILE =  "Broadcom NetXtreme 57xx Gigabit Controller"

OEM1_DEV7           = "Broadcom 570x Gigabit Integrated Controller"

; These items will be set by IHV...
DriverMfgr            = "Broadcom"                  ; IHV name
DriverVersionID       = "5.00"                      ; The IHV driver version
BaseDriverFileVersion = "10.62"
BaseDriverFileName    = "b57xp32.sys"               ; Key file for version

; These items will be set by IHV and updated by OEM
DriverOEM         = "Dell"      ; name of the OEM
DriverFamily      = "NIC"       ; device family (NIC, Storage, Video...)
DriverProduct     = "BCM5700"   ; Specific Name of device (chipset, for example)
DriverDescription = "Broadcom NetXtreme Gigabit Ethernet"  ; Description of device (product name, OS or system supported)
DriverOEMVersion  = "A00"       ; OEM-specified version


JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1 Gb Full Auto"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"



TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"


TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"

TaskOffload_LargeSend_Jumbo                           = "LSO & Jumbo Frames"
TaskOffload_LargeSend_Disable_Both                = "Both Disabled"
TaskOffload_LargeSend_Enable_JumboDisable   = "LSO Enabled,Jumbo Off"
TaskOffload_LargeSend_Disable_JumboEnable3000   = "LSO Off,Jumbo 3000"
TaskOffload_LargeSend_Disable_JumboEnable4500   = "LSO Off,Jumbo 4500"
TaskOffload_LargeSend_Disable_JumboEnable6000   = "LSO Off,Jumbo 6000"
TaskOffload_LargeSend_Disable_JumboEnable7500   = "LSO Off,Jumbo 7500"
TaskOffload_LargeSend_Disable_JumboEnable9000   = "LSO Off,Jumbo 9000"


WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"

WolSpeed       = "WOL Speed"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
WolSpeed_LowestAvail = "Lowest Speed Advertised"

NetworkAddress           = "Locally Administered Address"


LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"

