Back to Contents

# Specifications

Intel(R) Wireless WiFi Link 4965AGN
Intel(R) Wireless WiFi Link 4965AG_
Intel(R) PRO/Wireless 3945ABG Network Connection
Intel(R) PRO/Wireless 3945BG Network Connection
Intel(R) PRO/Wireless 2915ABG Network Connection
Intel(R) PRO/Wireless 2200BG Network Connection

## Intel(R) Wireless WiFi Link 4965AGN

Form Factor | PCI Express* Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n | 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows 2000*, Windows XP* (32 and 64 bit) and Windows Vista* (32 and 64 bit).
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, WPA*, WPA2*, WMM*, EAP-SIM
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) Wireless WiFi Link 4965AG_

This is a version of Intel Wireless WiFi 4965AGN with Draft N capabilities disabled. Draft N refers to: IEEE P802.11n / D1.0 Draft Amendment to STANDARD [FOR] Information Technology-Telecommunications and information exchange between systems-Local and Metropolitan networks-Specific requirements-Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) specifications: Enhancements for Higher Throughput

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows 2000, Windows XP (32 and 64 bit), and Windows Vista (32 and 64 bit)
Wi-Fi Alliance certification | Wi-Fi certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 3945ABG Network Connection

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50 to 92% non-condensing (at temperatures of 25 ºC to 55 ºC)
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 non-overlapping, dependent on country | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows 2000, Windows XP, and Windows Vista
Wi-Fi Alliance certification | Wi-Fi certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 3945BG Network Connection

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50 to 92% non-condensing (at temperatures of 25 ºC to 55 ºC)
Frequency Modulation | 2.4 GHz (802.11b/g)
Frequency band | 2.400 - 2.4835 GHz (dependent on country)
Modulation | CCK, DQPSK, DBPSK
Wireless Medium | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows 2000, Windows XP, and Windows Vista
Wi-Fi Alliance certification | Wi-Fi certification for 802.11b, 802.11g, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 2915ABG Network Connection

Form Factor | Mini PCI Type 3A
Dimensions | Width 2.85 in x Length 1.75 in x Height 0.20 in (59.75 mm x 50.95 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin SO-DIMM edge connector
Voltage | 3.3 Volt
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz | 2.400 - 2.472 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 non-overlapping, dependent on country | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows 2000, Windows XP, and Windows Vista
Wi-Fi Alliance certification | Wi-Fi certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v3.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit. 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 2200BG Network Connection

Form Factor | Mini PCI Type 3B
Dimensions | Width 2.34 in x Length 1.75 in x Height 0.20 in (59.45 mm x 44.45 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin mini PCI edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing
Frequency Modulation | OFDM with BPSK, QPSK, 16QAM, 64QAM, DBPSK, DQPSK, CCK
Frequency band | 2.400 - 2.472 GHz (US) 2.400 - 2.4835 GHz (Japan) 2.400 - 2.4835 GHz (Europe ETSI)
Modulation | OFDM with BPSK, QPSK, 16QAM, 64QAM, DBPSK, DQPSK, CCK
Channels | Full 14 channel support
Data Rates | 1, 2, 5.5, 6, 9, 11, 12, 24, 36, 48 and 54 Mbps
General
Operating Systems | Microsoft Windows 2000, Windows XP, and Windows Vista
Wi-Fi Alliance certification | Wi-Fi certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v2.0
WLAN Standard | IEEE 802.11g and 802.11b
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA, LEAP, PEAP, TKIP, EAP-TLS, EAP-TTLS, AES (128-bit), WEP 128-bit and 64-bit.
Product Safety | UL, C-UL, CB (IEC 60590)

Back to Top

Back to Contents

Trademarks and Disclaimers