Back to Contents

# Advanced Statistics (Advanced menu)

The Advanced Statistics provides current adapter connection information. This information defines how the adapter communicates with an access point. At the Advanced menu, click Advanced Statistics to access.

#### Advanced Statistics Description

Name | Description
--- | ---
Statistics | Advanced Statistics: This information pertains to how the adapter communicates with an access point. Association: If the adapter finds an access point to communicate with, the value is in range. Otherwise, the value is out of range. AP MAC Address: The twelve-digit MAC address (00:40:96:31:1C:05) of the access point. Number of associations: The number of times the access point has found the adapter. AP count: The number of available access points within range of the WiFi adapter. Number of full scans: The number of times the adapter has scanned all channels for receiving information. Number of partial scans: The number of scans that have been terminated. Roaming: This information contains counters that are related to reasons for the adapter roaming. Roaming occurs when an adapter communicates with one access point and then communicates with another for better signal strength. Roaming count: The number of times that roaming occurred. AP did not transmit: The adapter did not receive radio transmission from the access point. You may need to reset the access point. Poor beacon quality: The signal quality is too low to sustain communication with the access point. Either you have moved the adapter outside the coverage area of the access point or the access point's device address information has been changed. AP load balancing: The access point ended its association with the adapter based on the access point's inability to maintain communication with all its associated adapters. Too many adapters are trying to communicate with one access point. AP RSSI too low: The Receive Signal Strength Indicator (RSSI) is too low to maintain an association with the adapter. You may have moved outside the coverage area of the access point or the access point could have increased its data rate. Poor channel quality: The quality of the channel is low and caused the adapter to look for another access point. AP dropped mobile unit: The access point dropped a computer from the list of recognizable mobile devices. The computer must re-associate with an access point. Miscellaneous: Use this information to determine if an association with a different access point increases performance and helps maintain the highest possible data rate. Received beacons: Number of beacons received by the adapter. Percent missed beacons: Percent value for missed beacons. Percent transmit errors: The percentage of data transmissions that had errors. Signal Strength: Signal strength of the access point that the adapter communicates with displayed in decibels (dBm).
Transmit/Receive (Tx/Rx) Statistics | Displays percent values for non-directed and directed packets. Total host packets: The total number of directed and non-directed packets counts. Transmit - (Mbps) Receive - (Mbps) Non-directed packets: The number of received packets broadcast to the wireless network. Directed packets: The number of received packets sent specifically to the WiFi adapter. Total Bytes: The total number of bytes for packets received and sent by the WiFi adapter.
Logging | Set the duration that you want to record statistical data for your WiFi adapter. Configure logging settings: Click Settings to set how frequently you want to log the statistics. You can set the number of seconds and how many hours you want the statistics to be logged. To change the storage location of the log file. Click Browse to specify a new log file location. The current path is displayed. The default location is in the Intel PROSet/Wireless WiFi program files directory. Click Open to close and apply the new file path. Click Close to exit Advanced Statistics. Start/Stop Logging: Click this button to start and stop logging. When you click Start logging, statistical information (described above) is accumulated. When you click Stop Logging, the accumulation ends and this information is saved to a file that you can open and view. View Log File...: Click this button to open the Wireless folder under Program Files\Intel (this is the default location). Log files are named using the month, day, and year, plus the number of the log created on that day. For example: 03122007_001.htm. The log file provides: Date and Time Adapter Information Connection Information Transmit/Receive Statistics NOTE: An administrator can disable this feature.
Reset Stats | Resets the adapter statistical counters back to zero and begins making new data measurements.
Close | Closes and returns to the main window.
Help? | Provides help information for this page.

For information about importing/exporting user-created profiles, see Import or Export Profiles.

Back to Top

Back to Contents

Trademarks and Disclaimers