; NL92VM.inf
; Setup information file for NEC LCD Monitor LCD92VM
;
; Copyright 2005, NEC Display Solutions,Ltd
;---------------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NMD%
CatalogFile=NL92VM.cat
DriverVer=03/30/2005,2.05.0330.1808

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC665A

[DestinationDirs]
DefaultDestDir = 11
NEC-NL92VM.CopyFiles = 23

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
NL92VM.icm=1

[Manufacturer]
%NMD%=NMD,ntamd64

[NMD]
%NEC-NL92VM%=NEC-NL92VM.Install, Monitor\NEC665A

[NMD.ntamd64]
%NEC-NL92VM%=NEC-NL92VM.Install.ntamd64, Monitor\NEC665A

[NEC-NL92VM.Install]
DelReg=DEL_CURRENT_REG
AddReg=NEC-NL92VM.AddReg, 1280, DPMS
CopyFiles=NEC-NL92VM.CopyFiles

[NEC-NL92VM.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=NEC-NL92VM.AddReg, 1280, DPMS
CopyFiles=NEC-NL92VM.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,1280,1024

[DPMS]
HKR,,DPMS,,1

[NEC-NL92VM.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-83.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"NL92VM.icm"

[NEC-NL92VM.CopyFiles]
NL92VM.icm

[Strings]
NMD="NEC"
Disk1="NEC Display Solutions Installation Disk"
NEC-NL92VM="NEC LCD92VM"
