# BCM4359 FCPAGBSS 2G iPA/eLNA; 5G ePA/eLNA board for bringup -
NVRAMRev=$Rev: 506283 $
cckdigfilttype=5
# valid ofdm filter types are 0 and 1
ofdmfilttype_2gbe=127
ofdmfilttype_5gbe=127
sromrev=11
boardrev=0x1201
boardtype=0x0770
# JIRA:SW4349-945 MANDATORY! Update makefile in case you touch bfl
boardflags=0x10081201
boardflags2=0x00000000
boardflags3=0x48700186
#boardnum=57410 
macaddr=00:90:4c:12:d0:01
ccode=0
regrev=0
antswitch=0
pdgain5g=0
pdgain2g=0
tworangetssi2g=0
tworangetssi5g=0
AvVmid_c0=2,130,2,130,2,130,2,130,2,130
AvVmid_c1=2,130,2,130,2,130,2,130,2,130
# JIRA:SW4349-945 MANDATORY! Update makefile in case you touch femctl
femctrl=14
vendid=0x14e4
devid=0x43ef
manfid=0x2d0
#prodid=0x052e
nocrc=1
#btc_mode=1
btc_params82=0x1a0
otpimagesize=502
xtalfreq=37400
rxgains2gelnagaina0=3
rxgains2gtrisoa0=7
rxgains2gtrelnabypa0=1
rxgains5gelnagaina0=3
rxgains5gtrisoa0=6
rxgains5gtrelnabypa0=1
rxgains5gmelnagaina0=3
rxgains5gmtrisoa0=6
rxgains5gmtrelnabypa0=1
rxgains5ghelnagaina0=3
rxgains5ghtrisoa0=6
rxgains5ghtrelnabypa0=1
rxgains2gelnagaina1=3
rxgains2gtrisoa1=7
rxgains2gtrelnabypa1=1
rxgains5gelnagaina1=3
rxgains5gtrisoa1=6
rxgains5gtrelnabypa1=1
rxgains5gmelnagaina1=3
rxgains5gmtrisoa1=6
rxgains5gmtrelnabypa1=1
rxgains5ghelnagaina1=3
rxgains5ghtrisoa1=6
rxgains5ghtrelnabypa1=1
rxchain=3
txchain=3
aa2g=3
aa5g=3
agbg0=2
agbg1=2
aga0=2
aga1=2
tssipos2g=1
extpagain2g=2
tssipos5g=1
extpagain5g=0
tempthresh=255
tempoffset=255
rawtempsense=0x1ff
pa2gccka0=-205,7273,-878
pa2gccka1=-201,7723,-928
pa2ga0=-189,6880,-821
pa2ga1=-194,6958,-833
pa5ga0=-213,6020,-732,-215,5920,-720,-214,5912,-720,-216,5854,-714
pa5ga1=-217,5866,-716,-218,5859,-716,-213,6020,-731,-214,5994,-729
pa5gbw4080a0=-219,5963,-731,-216,6005,-732,-219,5887,-722,-222,5792,-713
pa5gbw4080a1=-215,6064,-739,-220,5934,-728,-217,6007,-732,-220,5914,-724
maxp2ga0=74
maxp2ga1=74
maxp5ga0=78,78,78,78
maxp5ga1=78,78,78,78
subband5gver=0x4
paparambwver=3
cckpwroffset0=0
cckpwroffset1=0
pdoffset40ma0=0x0000
pdoffset80ma0=0x0000
pdoffset40ma1=0x0000
pdoffset80ma1=0x0000
cckbw202gpo=0
cckbw20ul2gpo=0
mcsbw202gpo=0xA9876420
mcsbw402gpo=0xA9876420
dot11agofdmhrbw202gpo=0x6622
ofdmlrbw202gpo=0x0000
mcsbw205glpo=0xA9876420
mcsbw405glpo=0xA9876420
mcsbw805glpo=0xA9876420
mcsbw1605glpo=0
mcsbw205gmpo=0xA9876420
mcsbw405gmpo=0xA9876420
mcsbw805gmpo=0xA9876420
mcsbw1605gmpo=0
mcsbw205ghpo=0xA9876420
mcsbw405ghpo=0xA9876420
mcsbw805ghpo=0xA9876420
mcsbw1605ghpo=0
mcslr5glpo=0x0000
mcslr5gmpo=0x0000
mcslr5ghpo=0x0000
sb20in40hrpo=0x0
sb20in80and160hr5glpo=0x0
sb40and80hr5glpo=0x0
sb20in80and160hr5gmpo=0x0
sb40and80hr5gmpo=0x0
sb20in80and160hr5ghpo=0x0
sb40and80hr5ghpo=0x0
sb20in40lrpo=0x0
sb20in80and160lr5glpo=0x0
sb40and80lr5glpo=0x0
sb20in80and160lr5gmpo=0x0
sb40and80lr5gmpo=0x0
sb20in80and160lr5ghpo=0x0
sb40and80lr5ghpo=0x0
dot11agduphrpo=0x0
dot11agduplrpo=0x0
phycal_tempdelta=15
temps_period=15
temps_hysteresis=15
ltecxmux=0
ltecxpadnum=0x0504
ltecxfnsel=0x44
ltecxgcigpio=0x04
#OOB params
#device_wake_opt=1
#host_wake_opt=0
swctrlmap_2g=0x00000808,0x30300000,0x10100000,0x023010,0x1f8                                                                                                                        
swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x003
swctrlmap_5g=0x0000c0c0,0x00000000,0x80800000,0x000000,0x0c0                                                                                                        
swctrlmapext_5g=0x00000000,0x01010000,0x01010000,0x000000,0x001
rssi_delta_5gl_c0=3,3,2,2,5,5
rssi_delta_5gml_c0=0,2,0,2,3,5
rssi_delta_5gmu_c0=0,2,0,2,3,5
rssi_delta_5gh_c0=2,5,2,5,5,8
rssi_delta_5gl_c1=1,1,2,2,3,3
rssi_delta_5gml_c1=-1,1,0,2,1,3
rssi_delta_5gmu_c1=-1,1,0,2,1,3
rssi_delta_5gh_c1=0,3,2,5,3,6
rssi_delta_2g_c0=4,5,4,5
rssi_delta_2g_c1=2,3,2,3
muxenab=1

# ###########  BTC Dynctl profile params  ############
# flags:bit0 - dynctl enabled, bit1 dynamic desense, bit2 dynamic mode
btcdyn_flags=0x7
btcdyn_dflt_dsns_level=0
btcdyn_low_dsns_level=0
btcdyn_mid_dsns_level=7
btcdyn_high_dsns_level=2
btcdyn_default_btc_mode=5
btcdyn_btrssi_hyster=2
# --- number of rows in the array vars below ---
btcdyn_msw_rows=3
btcdyn_dsns_rows=2
# --- mode switch data rows (max is 4) ---
btcdyn_msw_row0=1,8,0,-50,-100
btcdyn_msw_row1=1,4,0,-55,-100
btcdyn_msw_row2=1,0,0,-70,-100
#btcdyn_msw_row3=1,-4,0,-70,-100
# --- desense switching data rows (max is 4) ---
#btcdyn_dsns_row0=5,8,0,-40,-40
btcdyn_dsns_row0=5,4,0,-60,-60
btcdyn_dsns_row1=5,0,0,0,-75
powoffs2gtna0=0,1,2,1,1,1,2,2,3,2,1,1,0,0
powoffs2gtna1=0,1,2,1,0,0,1,2,4,3,3,1,0,0
fem_table_init_val=0x10100000,0x80800000
