Intel® Rapid Storage Technology 14.6.1.1030 Production Version release

27 August 2015

DISCLAIMER: Information in this document is provided in connection with Intel products. No license, express or implied, by estoppels or otherwise, to any intellectual property rights is granted by this document. Except as provided in Intel’s Terms and Conditions of Sale for such products, Intel assumes no liability whatsoever, and Intel disclaims any express or implied warranty relating to sale and/or use of Intel products, including liability or warranties relating to fitness for a particular purpose, merchantability or infringement of any patent, copyright or other intellectual property right. Intel products are not intended for use in medical, lifesaving, or life-sustaining applications.

Intel may make changes to specifications and product descriptions at any time, without notice.

Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.
* Other names and brands may be claimed as the property of others.
Copyright © Intel Corporation 2000-2015

Supported Operating Systems

> > Microsoft Windows 7*

> > Microsoft Windows 7 x64 Edition*

> > Microsoft Windows 8*#

> > Microsoft Windows 8 x64 Edition*

> > Microsoft Windows Server 2008 R2 x64*#

> > Microsoft Windows Server 2012 x64 Edition*#

> > Microsoft Windows Server 2012 R2 x64 Edition*

> > Microsoft Windows 8.1*#

> > Microsoft Windows 8.1 x64 Edition*

> > Microsoft Windows 10*#

> > Microsoft Windows 10 x64 Edition*

> > #- These OS versions pass validation testing, but are not WHQL certified.

> > Revision History

> > Date | Driver Revision | Build Number
> > 27 August 2015 | 14.6.1.1030 Production Version release | 1030
> > 31 July 2015 | 14.6.0.1029 Production Version release | 1029
> > 28 July 2015 | 14.6.0.1029 release | 1029

> > Notes:

> > 1. Known Issue is defined as a potential RST issue that has been replicated internally by the Rapid Storage Technology team but has not been root caused to be an RST defect.

> > 2. The driver and user interface version is 14.6.1.1030.

> > 3. No RST support for PCIe storage devices in AHCI mode.

> > *Contact your Intel® Rapid Storage Technology representative with any questions.*

> > Resolved Issues

> > Resolved Issues in 14.6.1.1030 Production Version release |
> > Reference No | Description | Affected OS's
> > 4938702 | WHQL,System - Sleep and PNP (disable and enable) with IO Before and After | Win7-64
> > Resolved Issues in 14.6.0.1029 release |
> > Reference No | Description | Affected OS's
> > 4938414 | BSoD 0x154 when run S4 | Windows 10-64
> > 4938455 | IAStorUI has stopped working" when click 'Manager' tab (Unit with M2 PCIe SSD) with no empty port available | Win7-64
> > 4938614 | BSOD/Hung observed while resuming from CS with PCIe AHCI drives in remapped state | Windows 10-64
> > 4937992 | Trim doesn't work on RAID0 on SATA SSD disks | Windows 8.1 - 64
> > 4938456 | Recovery volume can’t be built in IRST when the secondary hard drives size is the same as the prim | Win7-64
> > 4938206 | BSOD 0x9F occurred as reboot system after finishing Burn-in tool (4 hours) (add HDD R/W loading) test | Windows Server 8 - 64
> > 4938363 | Cannot create RAID/SRT when RTD3 is enabled in BIOS | Windows 8.1 - 64
> > 4938562 | SCSI Compliance Test 2.0 fails with NVMe disks | Windows 10-64
> > 4938189 | Extremely low performance during copying file to RAID volume with PCIe AHCI | Windows 8.1 - 64
> > 4938046 | RAID 1 going into 'failed' state during coping files to the volume. | Win7-64,Windows 8.1 - 64

> > Known Issues

> > Known Issues in 14.6.0.1029 Production Version release |  |
> > Reference No | Description | Affected OS's |
> > 4938463 | Windows cannot boot with 4k HDD after install RST 14.0.0.1143PV/14.5.0.1059 | Windows 8.1 - 64 |
> > 4938543 | If use HDD larger than 1.3TB build recovery without show an error message when CSM disable. | Other |
> > 4938206 | BSOD 0x9F occurred as reboot system after finishing Burn-in tool (4 hours) (add HDD R/W loading) test | Windows Server 8 - 64 |
> > 4938594 | ODD add\remove when run S3 test | Other |
> > 4938451 | Intel RST driver v14.5.0.1059 cause BSOD Critical_Process_DIED during Sx | Windows 10-64 |
> > 4938615 | BSOD 7E caused by iaStorA during cold boot stress test | Windows 10-64 |
> > 4938219 | [Win10] SRT mode change to Enhanced, after setting Maximized mode and reboot PC. | Windows 8.1 - 64 |
> > 4938557 | S4 hang black screen with certain NAS HDD under 2DR0 / 3DR5 | Windows 8.1 - 64 |
> > 4938590 | D1" 8.1 screen occurred during system entered S4 via pressed power button with "This PC" and DM | Windows 10-64 |
> > 4938369 | The RST UI displays SATA ports, in spite of the proper registers programmed properly to disable unnecessary SATA ports in BIOS | Windows 8 - 64 |
> > 4938357 | Error code 0x80070017 occurred while installing Win8.1 on the NVMe remapped Raid 1 volume | Windows 8.1 - 64 |
> > 4938287 | Error message display when run NvCacheScripts | Windows 8.1 - 64 |
> > 4938405 | System hang at 0xa0 issue with certain PCIe M.2 AHCI device | Windows 8 - 64 |
> > 4938273 | Removing the lowest numbered driver causes BSOD. | Win7 |
> > 4938275 | RAID0 created using legacy OROM missing metadata on one of the drives | Windows 8.1 - 64 |
> > 4938246 | PCIe NVMe SSD 2DR0 (2-disk RAID 0) performance lower than pass-through single SSD | Windows 8.1 - 64 |
> > 4938171 | [RCfgSata][DOS] Partition table is not preserved when using the /U switch | Windows 8.1 - 64 |
> > 4938173 | [RCfgsata][EFI][DOS]Incomplete serial number of drives is output when using the /ST switch | EFI,Other |
> > 4938177 | [RST EFI CLI] EFI CLI config disk status does not show system disk information | EFI |
> > 4938175 | [rcfgsata.efi][SKL] Cannot boot to OS after creating RAID1 out of two data drives while preserving an MBR partition table | Windows 8.1 - 64 |
> > 4938111 | DevSlpRegEditTool creates reg keys with invalid disk product_id | Windows 10-64 |
> > 4937999 | WHQL test "Driver Memory Test" failed on SharkBay Refresh | Windows 8.1 |
> > 4937705 | Driver cannot be uninstalled via Device manager on Windows 8.1 August update | Windows 8.1 - 64 |
> > 4937906 | rstcli.exe, rstcli64.exe allow to create recovery volume consisted of SATA and NVMe disks | Windows 8 - 64 |
> > 4937885 | CSMI reporting invalid Serial Number during failure situations | Windows Server 8 |
> > 4937578 | Driver: CE BSOD iastorA.sys occurs while uninstalling RST driver on a custom Windows 8.1 OS | Windows 8.1 - 64 |
> > 4937417 | Enabling SRT changes Device Manager Disk Drive Information | Windows 8.1 - 64 |
> > 4937630 | UI - PCI-E SSD custom space defaults at 64 GB, even if the drive has less than 64 GB of space left | Windows 8.1 - 64 |
> > 4937470 | Cache fail results in hangs/BSOD | Windows 8.1 |
> > 4937358 | UI: BSOD when clicking "Hide recovery disk files" actionable link with On request RRT Volume. | Windows 8.1 - 64 |
> > 4937399 | UI: System drive is not displaying or being recognized in RST UI | Win7-64 |
> > 4937304 | Iastor BSOD when auto rebuilding volume to the same port | Windows 8.1 - 64 |
> > 4937256 | SRT filecopy performance much worse than HDD | Windows 8 - 64,Windows 8.1 - 64 |
> > 4937286 | UI Writeback Cache checkbox (Advanced tab) disabled during IRRT volume creation | Windows 8 |
> > 4937082 | All expected TRIMs are not occurring on SRT | Windows 8.1 - 64 |
> > 4937196 | "Offline" disk shows up as "Normal" after reinserting back into system while RAID 5(or RAID 10) is rebuilding and restarting system | Win7-64,Windows 8 - 64,Windows 8.1 - 64 |
> > 4937109 | BSOD 9f occurs when certain PCIe-AHCI SSD is attached. | Windows 8 - 64 |
> > 4936925 | After multiple iterations of Hybrid S3 or S4, the sleep utility tool indicates errors when RST driver is installed. | Windows 8.1 - 64 |
> > 4936995 | Dump Driver fails to capture Crash Dump when OS is installed on certain NVMe devices. | Windows 8.1 - 64 |
> > 4937083 | OS Spindown of matrix RAID volumes causes hang | Windows 8 - 64 |
> > 4937068 | SMART Event disk rebuilding after system reboot of successful Raid 1 creation | Windows 8 - 64,Windows 8.1 - 64 |
> > 4937046 | internal_power_error (A0) BSOD with hybrid S3 | Win7-64,Windows 8.1 - 64 |
> > 4936840 | BSOD 0xD1 reported with inbox driver 12.0.1.1018 | Windows 8.1 - 64 |
> > 4936673 | No timeout for a device that does not enumerate and stalls the OS boot process | Windows 8 - 64,Windows 8.1 - 64 |
> > 4630242 | Refresh issues when changing from Windows default theme to high contrast | Win7-64,Windows 2008-64,Windows 8 - 64 |
> > 4628030 | After configuring SRT and conducting Dirty Shutdowns error: Unable to find System Disk | Windows 8 |
> > 4628443 | RST Driver – Test hangs while running Inquiry command on ODD | Other |
> > 3236644 | SRT: Driver fails to enumerate an accelerated disk or volume during an F6 install if a system disk is already attached to the system | Win7-64 |
> > 4160949 | UI reports Unknown status and incorrect sync mode after hot-removing the recovery disk of an IRRTm while the sync is initializing. | Win7-64 |
> > 4160928 | WHQL: RST not compliant with Device.DevFund.Memory.DriverFootprint requirements for x86 | Windows 8 |
> > 4628161 | ZPODD power off timer does not reset upon receipt of CSMI I/O | Win7,Windows 8 |