Back to Contents

# Specifications

This section provides specification information for the family of Intel® wireless adapters. The following list may not be all inclusive.

- Intel® Centrino® Wireless-N 100
- Intel® Centrino® Wireless-N 105
- Intel® Centrino® Wireless-N 130
- Intel® Centrino® Wireless-N 135
- Intel® Centrino® Wireless-N 1000
- Intel® Centrino® Wireless-N 1030
- Intel® Centrino® Wireless-N 2200
- Intel® Centrino® Wireless-N 2230
- Intel® Centrino® Wireless-N + WiMAX 6150
- Intel® Centrino® Advanced-N 6200
- Intel® Centrino® Advanced-N 6205
- Intel® Centrino® Advanced-N 6230
- Intel® Centrino® Advanced-N 6235
- Intel® Centrino® Advanced-N + WiMAX 6250
- Intel® Centrino® Ultimate-N 6300
- Intel® Dual Band Wireless-AC 7260
- Intel® Dual Band Wireless-N 7260
- Intel® Wireless-N 7260
- Intel® Dual Band Wireless-AC 3160
- Intel® Dual Band Wireless-AC 3165
- Intel® Dual Band Wireless-AC 3168
- Intel® Dual Band Wireless-AC 7265
- Intel® Dual Band Wireless-N 7265
- Intel® Wireless-N 7265
- Intel® Dual Band Wireless-AC 8260
- Intel® Dual Band Wireless-AC 8265
- Intel® Tri-Band Wireless-AC 17265
- Intel® Tri-Band Wireless-AC 18260
- Intel® Wireless Gigabit Sink W13100
- Intel® Wireless Gigabit 11000

## Intel® Centrino® Wireless-N 100, Intel® Centrino® Wireless-N 105, Intel® Centrino® Wireless-N 130 and
Intel® Centrino® Wireless-N 135

Form Factor | PCI Express* Half-Mini Card
Dimensions | Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | 2.4 GHz (802.11b/g/n)
Frequency band | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | MIMO Configuration: 1X1 Tx/Rx: 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth Support | Intel® Centrino® Wireless-N 100: None Intel® Centrino® Wireless-N 105: None Intel® Centrino® Wireless-N 130: Bluetooth 2.1, 2.1 + EDR, 3.0, 3.0+HS Intel® Centrino® Wireless-N 135: Bluetooth 4.0 (Bluetooth Low-Energy and Bluetooth 3.0 +HS)
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11n, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WPS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
IEEE Feature Sets | IEEE 802.11b, 802.11g, 802.11n, 802.11e, 802.11i, 802.11d, 802.11h
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Centrino® Wireless-N 1000

Form Factor | PCI Express* Mini Card and Half-Mini Card
SKUs | Intel® Centrino® Wireless-N 1000 - 1X2 MC/HMC
Dimensions | Mini Card: Width 2.0 in x Length 1.18 in x Height 0.18 in (50.80 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | 2.4 GHz (802.11b/g/n)
Frequency band | 2.41-2.474 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, CCK, DQPSK, DBPSK
Wireless Medium | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows* XP (32 and 64 bit) and Windows Vista* (32 and 64 bit), Ubuntu Linux*
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11n, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WPS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11n, 802.11d, 802.11e, 802.11i,
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, 802.1X: EAP-SIM, LEAP, PEAP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Encryption | AES-CCMP 128-bit, WEP 128-bit and 64-bit, CKIP, TKIP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Centrino® Wireless-N 2200 and Intel® Centrino® Wireless-N 2230

Form Factor | PCI Express* Half-Mini Card
Dimensions | Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | 2.4 GHz (802.11b/g/n)
Frequency band | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | MIMO Configuration: 2X2 Tx/Rx: 300, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth Support | Intel® Centrino® Wireless-N 2200: None Intel® Centrino® Wireless-N 2230: Bluetooth 4.0 (Bluetooth Low-Energy and Bluetooth 3.0 +HS)
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11n, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WPS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
IEEE Feature Sets | IEEE 802.11b, 802.11g, 802.11n, 802.11e, 802.11i, 802.11d, 802.11h
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Centrino® Wireless-N 1030 and Intel® Centrino® Advanced-N 6230

Form Factor | PCI Express* Half-Mini Card
Dimensions | Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Network Standards | 802.11a/b/g/n (varies by adapter) and Bluetooth 3.0 + HS
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi Network Standards | Intel® Centrino® Wireless-N 1030: 802.11b/g/n Intel® Centrino® Advanced-N 6230: 802.11a/g/n
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | Intel® Centrino® Advanced-N 6230: Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
Intel® Centrino® Wireless-N 1030: Rx (Mbps): 300, 270, 243, 240, 180 Rx/Tx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Bluetooth Version 3.0 + HS
General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit) Windows* 8 (32-bit and 64-bit) Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WPS, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA, P2P
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Centrino® Advanced-N 6235

Form Factor | PCI Express* Half-Mini Card
Dimensions | Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Network Standards | 802.11a/b/g/n and Bluetooth 4.0
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Bluetooth Version 4.0 (3.0 +HS )
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WPS, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA, P2P
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Centrino® Advanced-N + WiMAX 6250 and Intel® Centrino® Wireless-N + WiMAX 6150

Form Factor | PCI Express* Half-Mini Card
Dimensions | Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | Intel® Centrino® Advanced-N + WiMAX 6250 2.4 GHz (802.11b/g/n), 5 GHz (802.11a/n) | Intel® Centrino® Wireless-N + WiMAX 6150 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | Intel® Centrino® Wireless-N + WiMAX 6150 MIMO Configuration: 1X2 Rx: 300, 270, 243, 240, 180 Mbps Rx/Tx: 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
Intel® Centrino® Advanced-N + WiMAX 6250 MIMO Configuration: 2X2 Tx/Rx: 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit) Windows* 8 (32-bit and 64-bit) Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
IEEE Feature Sets | Intel® Centrino® Wireless-N + WiMAX 6150: IEEE 802.11b, 802.11g, 802.11n, 802.11e, 802.11i, 802.11h, 802.11d Intel® Centrino® Advanced-N + WiMAX 6250: 802.11a, IEEE 802.11b, 802.11g, 802.11n, 802.11e, 802.11i, 802.11h, 802.11d
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)
WiMAX General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit) Windows* 8 (32-bit and 64-bit) Windows* 8.1 (32-bit and 64-bit)
Standard Compliance | 802.16e-2005 Corrigenda 2 (D4)
WiMAX System Profile Feature set | Intel® Centrino® Wireless-N + WiMAX 6150: Mobile WiMAX release 1, Wave II. Supports 3A and 1A/B profiles Intel® Centrino® Advanced-N + WiMAX 6250: Mobile WiMAX release 1, Wave II. Supports 3A, 5A/C, 1A/B, and 5BL profiles
Security | Key Management Protocol (PKMv2)
Encryption | 128-bit CCMP (Counter-Mode/CBC-MAC) based on AES encryption
WiMAX
Frequency band | Intel® Centrino® Wireless-N + WiMAX 6150: 2.3-2.4 GHz / 2.496-2.690 GHz Intel® Centrino® Advanced-N + WiMAX 6250: 2.3-2.4 GHz / 2.496-2.690 GHz / 3.4-3.8 GHz
Modulation | UL - QPSK, 16 QAM DL - QPSK, 16 QAM, 64 QAM
Wireless Medium | Duplex mode: TDD operations | Scalable OFDMA (SOFDMA): 512 and 1024 FFT
sub-carrier permutation: PUSC | Intel® Centrino® Wireless-N + WiMAX 6150: Channel bandwidths: 5 and 10 MHz Intel® Centrino® Advanced-N + WiMAX 6250: Channel bandwidths: 5, 7, 8.75 and 10 MHz
WiMAX Network Release Feature set | SPWG/NWG Release 1.5
Rate Performance | Intel® Centrino® Wireless-N + WiMAX 6150: Up to 10 Mbps DL and 4 Mbps UL @ peak rate (OTA performance, 10MHz channel) Intel® Centrino® Advanced-N + WiMAX 6250: Up to 20 Mbps DL and 6 Mbps UL @ peak rate (OTA performance, 10MHz channel)
RF Transmitter Output Power | Compliance with Power class 2

## Intel® Centrino® Advanced-N 6200, Intel® Centrino® Advanced-N 6205 and Intel® Centrino® Ultimate-N 6300

Form Factor | Intel® Centrino® Advanced-N 6200, Intel® Centrino® Ultimate-N 6300: PCI Express* Full-Mini Card and Half-Mini Card. Intel® Centrino® Advanced-N 6205: PCI Express* Half-Mini Card.
Dimensions | Full-Mini Card: Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
IEEE 802.11n Data Rates | Intel® Centrino® Ultimate-N 6300: Tx/Rx: 450, 405, 360, 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
Intel® Centrino® Advanced-N 6200, Intel® Centrino® Advanced-N 6205: Tx/Rx: 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit) Windows* 8 (32-bit and 64-bit) Windows* 8.1 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 7260

Form Factors | Half-Mini Card and M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0 for both form factors
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 7260 Model 7260HMW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, HMC Model 7260NGW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 7260: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 7260: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7260HMW Model 7260NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-N 7260
Intel® Wireless-N 7260

Form Factors | Half-Mini Card, M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe, USB 2.0 for both form factors
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-N 7260 Model 7260HMW AN - 802.11agn, 2x2, Bluetooth 4.0, PCIe, USB, HMC Model 7260NGW AN - 802.11agn, 2x2, Bluetooth 4.0, PCIe, USB, M.2 Model 7260HMW NB - 802.11agn, 2x2, PCIe, USB, HMC Model 7260NGW NB - 802.11agn, 2x2, PCIe, USB, M.2 Intel® Wireless-N 7260 Model 7260HMW BN - 802.11agn, 2x2, Bluetooth 4.0, PCIe, USB, M.2 Model 7260NGW BN - 802.11bgn, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation (See above, not all bands supported by all adapters) | 5GHz (802.11a/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
802.11n spatial streams | All adapters: 2 X 2 spatial streams
Data Rates | All data rates are theoretical maximums.
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7260HMW AN Model 7260NGW AN Model 7260HMW BN Model 7260NGW BN
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 3160

Form Factors | Half-Mini Card and M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0 for both form factors
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 3160 Model 3160HMW - 802.11agn, ac, 1x1, Bluetooth 4.0, PCIe, USB, HMC Model 3160NGW - 802.11agn, ac, 1x1, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 3160: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 3160: Up to 433 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 3160HMW Model 3160NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 3165 (Model 3165NGW)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11abgn, 802.11ac, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 3165: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 3165: Up to 433 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE)
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 3168

Form Factors | M.2 2230 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11abgn, 802.11ac, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 3168: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 3168: Up to 433 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.2 (BLE)
General
Operating Systems | Linux, Windows* 8.1 (64-bit), Windows* 10 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 7265 (Model 7265NGW)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 7265 Model 7265NGW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 7265: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 7265: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7265NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-N 7265 (Models 7265NGW AN and 7265NGW NB)
Intel® Wireless-N 7265 (Model 7265NGW BN)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe, USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-N 7265 Model 7265NGW AN - 802.11agn, 2x2, Bluetooth 4.0, PCIe, USB, M.2 Model 7265NGW NB - 802.11agn, 2x2, PCIe, USB, M.2 Intel® Wireless-N 7265 Model 7265NGW BN - 802.11bgn, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation (See above, not all bands supported by all adapters) | 5GHz (802.11a/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
802.11n spatial streams | All adapters: 2 X 2 spatial streams
Data Rates | All data rates are theoretical maximums.
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7265NGW AN Model 7265NGW NB Model 7265NGW BN
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 8260

Form Factors | Half-Mini Card and M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0 for both form factors
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 8260 Model 8260NGW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 8260: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 8260: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 8260NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Dual Band Wireless-AC 8265 (Models 8265NGWH/8265NGW/8265D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm M.2 1216: 12 mm x 16 mm x 1.8 mm
Weight | M.2 2230: 2.6g M.2 1216: 0.6g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe, USB, or UART (M.2 1216 only)
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1*, Microsoft Windows 10*, Linux* (limited feature support), Android
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Direct* for peer to peer device connections, Wi-Fi Miracast* as Source.
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11REVmc
Roaming | Supports seamless roaming between access points
Bluetooth | Dual Mode Bluetooth* 4.2, BLE
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
Product Safety | UL, C-UL, CB (IEC 60950-1)
Model Numbers
Models | Model 8265NGWH | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, USB, LTE Coexistence, eFEM, M.2 2230 HE
| Model 8265NGW | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, USB, M.2 2230 MS | Model 8265D2W | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, LTE Coexistence, M.2 1216 SD
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 8265: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 8265: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Tri-Band Wireless-AC 17265 (17265NGW/17265NGW LC)

Form Factors | M.2 Type 3030
Electrical interfaces | M.2 Key 1-DP: 2xPCIe, USB, DP. Interface to Intel® Wireless Gigabit-Antenna M10041 Module using X-FL, and one dedicated for Bluetooth
Antenna Interface Connector | X.FL; Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11ac, 802.11ad, 802.11abgn, 802.11a, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 60GHz (802.11ad) | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 57GHz - 64GHz (dependent on country) | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | DPSK, BPSK, QPSK, 16 QAM, | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | DMG control PHY, DMG SC PHY | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 1, 2 and 3, subject to country rules | All channels as defined by the relevant specification and country rules.
Spatial streams | N/A | Intel® Tri-Band Wireless-AC 17265
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Tri-Band Wireless-AC 17265: Up to 867 Mbps
IEEE 802.11ad Data Rates | 4620, 3850, 3080, 2503, 2310, 1925, 1540, 1251, 1155, 963, 770, 385 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE)
General
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1* with connected standby
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, AES-CGMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Tri-Band Wireless-AC 18260 (18260NGW)

Form Factors | M.2 Type 2230
Electrical interfaces | M.2 Key 1-DP: 2xPCIe, USB, DP. Interface to Intel® Wireless Gigabit-Antenna M10041 or M10042 Module using X-FL (single coax cable to carry power, IF and control)
Dimensions | 22 mm x 30 mm x S3 [1.5mm Max (Top Side)/ 0.1mm max (bottom side)]
Antenna Interface Connector | X.FL; Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | IEEE 802.11abgn, 802.11ac, 802.11ad, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 60GHz (802.11ad) | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 57GHz - 64GHz (dependent on country) | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | DPSK, BPSK, QPSK, 16 QAM, | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | DMG control PHY, DMG SC PHY | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 1, 2 and 3, subject to country rules | All channels as defined by the relevant specification and country rules.
Spatial streams | N/A | Intel® Tri-Band Wireless-AC 18260
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Tri-Band Wireless-AC 18260: Up to 867 Mbps
IEEE 802.11ad Data Rates | 4620, 3850, 3080, 2503, 2310, 1925, 1540, 1251, 1155, 963, 770, 385 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE), 4.1
General
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1* with connected standby
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, AES-CGMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Wireless Gigabit Sink W13100

Form Factors | M.2 Type 3030
Electrical interfaces | M.2 Key 1-DP: 2xPCIe, USB, DP. Interface to Intel® Wireless Gigabit-Antenna M10041 Module using X-FL, and one dedicated for Bluetooth
Antenna Interface Connector | X.FL
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11ac, 802.11ad, 802.11abgn, 802.11a, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 60GHz (802.11ad)
Frequency band | 57GHz - 64GHz (dependent on country)
Modulation | DPSK, BPSK, QPSK, 16 QAM,
Wireless Medium | DMG control PHY, DMG SC PHY
Channels | 1, 2 and 3, subject to country rules
Spatial streams | Intel® Wireless Gigabit Sink W13100
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ad Data Rates | 4620, 3850, 3080, 2503, 2310, 1925, 1540, 1251, 1155, 963, 770, 385 Mbps
General
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1* with connected standby
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, AES-CGMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 60950-1)

## Intel® Wireless Gigabit 11000

Dimensions | 20.5 mm x 14.2 mm x 1.8 mm (shield included)
Weight | 2 grams
Electrical interfaces | Soldered module has a proprietary land plan. Interface to Intel® Wireless Gigabit-Antenna M10041 Module or Intel® Wireless Gigabit Antenna-M 10042R using X-FL (single coax cable to carry power, IF and control)
Antenna Interface Connector | X.FL
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11ad
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 60GHz (802.11ad)
Frequency band | 57GHz - 64GHz (dependent on country)
Modulation | DPSK, BPSK, QPSK, 16 QAM,
Channels | 1, 2 and 3, subject to country rules
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ad Data Rates | 4620, 3850, 3080, 2503, 2310, 1925, 1540, 1251, 1155, 963, 770, 385 Mbps
General
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1* with connected standby, Microsoft Windows 10* with connected standby

Back to Top

Back to Contents

Trademarks and Disclaimers