; ** Copyright (c) 2007-2021 Realtek Corporation. All rights reserved.
;
; Realtek PCIe GbE Family Controller
;

;
; This product is covered by one or more of the following patents:
; US6,570,884, US6,115,776, and US6,327,625.
;

;
; This file registers your driver, service, and network interface with the
; operating system.  Search this file for "TODO" to see sections you should
; customize to fit your driver.  You can delete the TODO comments if you like.
;

[version]
Signature               = "$Windows NT$"
Class                   = Net
ClassGUID               = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider                = %Provider%
PnpLockDown             = 1
DriverVer = 09/09/2021,1168.002.0909.2021
CatalogFile = rt68cx21x64.cat

;
; This directive limits the OS versions that this driver can be installed on.
; Because NetAdapter is not available prior to build 16299 (version 1709), this
; sample targets build 15063.
;
[Manufacturer]
%Provider%=Realtek, NTx86, NTamd64, NTamd64.10.0...21390

;
; TODO: Update this with a list of your hardware IDs.
;
[Realtek]
;Empty section, so this INF does not support win2000

[Realtek.NTx86]
;Empty section, so this INF does not support x86

[Realtek.NTamd64]
;Empty section, so this INF does not support x64

[Realtek.NTamd64.10.0...21390]
; 8168H
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&REV_15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00083100&REV_15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8161&REV_15 ;_Add-on card
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8161&SUBSYS_816810EC&REV_15 ;_Add-on card
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_095E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_095F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09601025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09611025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_096F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09711025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09721025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09741025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09831025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09851025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09871025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09881025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09891025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09961025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09971025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09981025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_099D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_099E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_099F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10101025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10111025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10121025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10131025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10141025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10151025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10171025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10191025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_101A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10221025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10241025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10251025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10301025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10311025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10321025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10331025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10341025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10351025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10361025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10371025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10391025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103A1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103D1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_103F1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10401025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10411025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10421025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10431025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_104B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_104C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10651025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10791025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107C1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107F1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10841025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10851025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10861025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10871025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10881025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10891025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110C1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110D1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110E1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110F1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_111D1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11231025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11271025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11331025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_114B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_114C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_114E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_114F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11541025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11551025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11561025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11571025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11581025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_115E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_116C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11721025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11981025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_120A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_120B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12151025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12181025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12191025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12231025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12241025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12271025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12321025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12551025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_126C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_126E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12711025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12871025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12881025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_128A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_128B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_128C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12941025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12971025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12981025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_129F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13071025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13081025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_130C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_130F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13111025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13131025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13151025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_131A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13251025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13271025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13281025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13291025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_133E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13451025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13461025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13471025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13481025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_134D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_134F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13551025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13571025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_135C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_135E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13601025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13621025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13631025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13661025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13731025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_137B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_137D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_137F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13801025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13951025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13961025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13991025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_139A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_139B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_139C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_141C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14221025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14291025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14301025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14311025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14341025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14361025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14371025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14381025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14391025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14541025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14561025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14571025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14581025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14591025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_145C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_145E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14611025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14621025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14641025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14651025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14681025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14691025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14751025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14761025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14841025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14861025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148F1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14941025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14951025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14981025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15031025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_150B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_150D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15101025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15111025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15151025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15181025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15191025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_151B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_151C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_151D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15221025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15241025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15271025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15281025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_152B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15411025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15421025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15491025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_154A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_154B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_154D1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15521025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15571025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15611025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15711025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15721025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157E1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_158D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_158F1025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15901025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15911025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15921025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15931025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15941025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15951025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15961025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16071025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_160A1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_160B1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21771019&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9BEE1019&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5141019&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A59F1019&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A9921025&REV_15 ;ACER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_4550105B&REV_15 ;America
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01111849&REV_15 ;asrock
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30121849&REV_15 ;ASRock
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81681849&REV_15 ;ASRock
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1AA21043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_205F1043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86771043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86771D05&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E31043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_23121565&REV_15 ;BIOSTAR
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20371D72&REV_15 ;Bitland
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21011D72&REV_15 ;bitland
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30040526&REV_15 ;bitland
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1241152D&REV_15 ;Casper
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1135152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1136152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1152152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1153152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1154152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1155152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1158152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1159152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1160152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1173152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1193152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1194152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1196152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1197152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1198152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1200152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1202152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01561558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40301558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65F11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67E51558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6001558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_011E14C0&REV_15 ;Compal
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06BB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06CC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06CD1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06CF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D01028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D11028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D31028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D41028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D417AA&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D51028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06D517AA&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06E31028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06EF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F41028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F51028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F71028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F81028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06F91028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06FA1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06FB1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06FC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_072B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_072C1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_074A1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_074B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07501028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07511028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07521028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07531028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07541028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07551028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07561028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_075E1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_075F1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07601028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07611028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07621028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07631028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07641028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07671028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07681028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07691028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_076A1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_076B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_076C1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_077B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_077C1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_077D1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_077F1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07801028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07811028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07821028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07831028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07841028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07851028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07861028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07971028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07981028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_079B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_079E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_079F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07A31028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07B41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07B51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07B61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07B71028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07B81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07BB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07BC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07BD1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07C41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07C61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07C71028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07CE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07D61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07D81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07D91028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07E91028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07EA1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07EB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07EC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07EE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07FA1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_07FB1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08021028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08031028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08241028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08251028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08261028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08271028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08281028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08291028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_082F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08301028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08391028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_083A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08411028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08421028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08431028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08441028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08451028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08481028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08491028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08521028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08531028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08541028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08551028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_085C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_085F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08601028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08611028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08651028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08661028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08671028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08681028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08691028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_086A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_086B1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_086C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_086F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08701028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08741028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08851028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08861028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08971028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08981028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_089A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_089C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_089D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_089E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_089F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08A51028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08A61028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08A71028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08A81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08A91028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08BB1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08BC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08BD1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08BE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08BF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08C01028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08C11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08EA1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08EB1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08EC1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08ED1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08EE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08EF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08F81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08F91028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08FA1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08FB1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_092E1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_092F1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09301028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09311028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09321028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09331028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09491028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09521028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09531028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09541028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09591028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_095A1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_097F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098B1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09921028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09931028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09941028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09951028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09961028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09971028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09981028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09991028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09A81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09A91028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09AE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09AF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B01028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09B61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09E11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09E21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09EA1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09EB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09EC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09ED1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F31028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F41028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F91028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A011028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A021028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A031028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A041028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A061028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A071028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A081028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A091028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A131028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A301028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A311028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A4B1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A4E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A4F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A501028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A511028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A581028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A591028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A641028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A651028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A6E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A6F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A711028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A791028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7A1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7C1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A7F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A801028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A841028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A851028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AA31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AA41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AB21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AB31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AB51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AC51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AC61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ACD1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ACE1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ACF1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AD01028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AD11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AD21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AD31028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ADB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ADC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0ADF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE01028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE11028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE41028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE51028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AE81028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AEB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AEC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AED1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AEE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AEF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AF01028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AF11028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AF21028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AF51028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B1C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B1D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B1E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B1F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B201028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B211028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B231028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B241028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B251028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B261028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B2C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B2D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B2E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B2F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B301028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B311028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B321028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B331028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B3E1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B3F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B411028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B421028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B441028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B451028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B481028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B551028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B571028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B591028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B5B1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B5D1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B5E1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B641028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B661028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B671028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B691028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B6A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B6C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B6D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B6F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B771028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B781028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B791028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B7A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B7C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B7D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B801028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B811028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B821028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B831028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B841028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B851028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B861028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0B871028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319417AA&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00023100&REV_15 ;Dynabook
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00043100&REV_15 ;Dynabook
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00053100&REV_15 ;Dynabook
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00063100&REV_15 ;Dynabook
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00073100&REV_15 ;Dynabook_DBH
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16011BAB&REV_15 ;EA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16A11BAB&REV_15 ;EA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10199858&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81171019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_96261019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_983C1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_983E1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98401019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98411019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98451019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98461019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98541019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98551019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98571019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98591019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98641019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_98661019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9A001019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9C551019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9C561019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9C801019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9CC41019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9CC71019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9CE61019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9CED1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9D091019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A3ED1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A3F51019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4121019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4381019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A43D1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4591019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A47E1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4A51019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4A71019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4A81019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4A91019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5341019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5561019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5591019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A55C1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A55D1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A57C1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A57D1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A57F1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5A01019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5A11019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5EA1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A60D1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6521019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6561019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6OO1019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A9461019&REV_15 ;ECS_Medion
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A9901019&REV_15 ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E65105B&REV_15 ;FOXCONN
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E6D105B&REV_15 ;Foxconn_Clone MB
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E6F105B&REV_15 ;FOXCONN_CLONE MB
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_125F1734&REV_15 ;Fujitsu
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40061071&REV_15 ;Getac
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A1601071&REV_15 ;Getac
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B3601071&REV_15 ;Getac
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_15 ;GigaByte
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10891D05&REV_15 ;Haier
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10961D05&REV_15 ;Haier
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10801D05&REV_15 ;Hansung
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20011DEA&REV_15 ;Hibertek International Limited
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8043103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8044103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_806C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_806D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_806E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_806F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8072103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8073103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8074103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8075103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8078103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80BF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80C9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80CF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80D0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80D1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80D7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80D8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80D9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80DF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80E9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80EA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80EB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80EC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80ED103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80EE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8131103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8132103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8133103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8134103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8135103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8136103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8137103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8138103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8143103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8154103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8155103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8187103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8188103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_818F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8191103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8192103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8193103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8194103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8195103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8196103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_819F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81CB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81CC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81CF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81D0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81D1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81D2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81D3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81D4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81DB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81DC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81DD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81DE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81DF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81E9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81EA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81EB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81EC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81ED103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81EE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81EF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81F9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81FA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81FF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8200103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8201103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8202103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8203103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8204103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8205103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8206103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8207103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8208103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8209103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_820F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8210103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8211103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8212103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8213103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8214103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8215103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8216103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8217103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8218103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8219103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_821A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_821B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_821C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_821E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_821F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8220103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8221103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8222103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8223103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8224103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8226103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8228103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8229103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8251103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8252103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8253103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8257103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8258103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8259103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_825F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8260103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8261103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8262103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8263103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8264103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_828B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8294103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8295103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82EA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82EE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82F6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82F7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8305103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8306103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8307103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8308103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8309103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_831C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_831D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_831E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_831F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8320103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8321103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8322103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8323103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8324103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8325103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8326103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8327103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8328103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8329103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_832F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8330103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8331103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8332103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8333103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8334103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8339103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_833F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8340103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8341103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8342103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8343103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8345103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8346103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8347103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8348103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8353103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8354103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8355103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8356103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8357103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8358103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8359103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_835A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_835D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_835E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_835F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8360103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8361103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8362103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8363103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8364103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8365103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8366103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8367103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8368103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8369103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_836A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_836B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_836C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8385103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8389103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8395103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83C0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83C1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83FA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83FB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8406103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8407103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8408103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_840D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_841B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_841C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8421103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8422103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8433103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8434103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8435103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8436103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_843B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_843C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_843D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_843E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_843F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8440103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8441103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8444103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8445103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_844C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8459103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_845E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_847D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_847E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_847F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8480103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8498103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8499103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_849F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84A9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84AF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84B9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84BF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84C9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84CF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84E5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84E6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84E7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84E8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84ED103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8511103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8513103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8527103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_852C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_852D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_852E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_852F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8530103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8531103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8532103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8533103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8544103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8545103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8546103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8547103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_855A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_855B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_855E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_855F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8560103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8561103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8562103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8563103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_856A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8578103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8579103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_857A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_857B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8581103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85B1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85B2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85B3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85B4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85BB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85BC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85BD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85BE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85D3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85D4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85D5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85D6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85E0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85E1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85E4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85E5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85EA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85EC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85ED103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85EE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85EF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85F6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8615103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8616103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_861B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_861C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_861D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_861E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8627103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8628103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8629103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_862F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8630103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8631103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8632103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8633103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8634103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8638103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8639103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_863A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_863B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_863C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_863D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8640103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8641103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8646103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8647103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8653103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8656103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8657103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8658103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8659103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_865A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_865B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_865E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_866A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_866B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_868F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8692103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8693103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8694103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8695103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86AA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86AB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86AC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86AF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86BF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CB103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CC103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D5103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D7103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D8103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86DA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86ED103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86EE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8778103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8796103C&REV_15 ;HP_Dali_UMA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8797103C&REV_15 ;HP_Dali_DIS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8798103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8799103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879A103C&REV_15 ;HP_Dali_UMA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879B103C&REV_15 ;HP_Dali_DIS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879E103C&REV_15 ;HP_Dali_UMA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_879F103C&REV_15 ;HP_Dali_DIS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87A0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87A1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87AA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87AD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87AE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87AF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87C1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87C2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87CE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D2103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D4103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87DA103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_880E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8817103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8818103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8819103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_881A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_881B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_881C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_881D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_881E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_885E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DD103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DE103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DF103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8905103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8908103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8909103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_890E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8911103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_892C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_892D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_894B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8996103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8997103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8998103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8999103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_899A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_899F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89A0103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89A1103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A1B103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A1C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A1D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A1E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_125D152D&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1260152D&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_127D152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1301152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1307152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1319152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1322152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1346152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1351152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1365152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1368152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1371152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1372152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E0A19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E0C19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E0D19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E1119E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E1519E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E1719E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E1F19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2019E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2A105B&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2A19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2B105B&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2B19E5&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E40105B&REV_15 ;Huawei
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E6E1028&REV_15 ;InFocus
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20678086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20728086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20868086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20878086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30118086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30128086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30278086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_46071B50&REV_15 ;Lengda
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004517AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004717AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_004D17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30DA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30FC17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_310217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_312F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_316117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_316917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_318F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31A017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31B717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31BB17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31BF17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32C017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32F417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32F617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_330317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_330417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_362E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_363617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36B917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36BB17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36BC17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36BD17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36BE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36CC17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36D017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36D917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DB17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DC17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DD17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36DF17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36ED17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36EE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FB17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FC17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FD17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36FF17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_371F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_372F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_380117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_380A17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_380D17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_380E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_381517AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38171025&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_381717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_381A17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383D17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383E17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384117AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384317AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384B17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384E17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_384F17AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_385017AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_385217AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_385317AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_385417AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_385E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_386617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_386717AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_386817AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_387417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_387517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_387F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_388E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_389F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38A917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38AC17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38B117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38B417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38B517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38B717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38BA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38BE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38BF17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38C017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38C217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38C317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38C817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38CA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38CD17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38CE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38D017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38D317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38D417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38D617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38D717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38DA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38DB17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38DD17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38DE17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38F217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38F417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38F817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38F917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_390B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_392F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_393017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_393517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_507E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_508717AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_509117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_509417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_509C17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50AA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50AB17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_612817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_614F17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_740117AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03061854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03071854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03101854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03111854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03121854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03131854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03391854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03401854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03441854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03451854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03511854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03521854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03531854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03861854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03871854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04151854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04161854&REV_15 ;LGE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_106A1D05&REV_15 ;MBB
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10661D05&REV_15 ;MCJ
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10771D05&REV_15 ;MCJ
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107A1D05&REV_15 ;MCJ
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107B1D05&REV_15 ;MCJ
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110917C0&REV_15 ;MEDION
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_110C17C0&REV_15 ;Medion
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20608086&REV_15 ;MEDION
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20D91B0A&REV_15 ;Medion
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A481462&REV_15 ;MEDION
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D0121E39&REV_15 ;MEDION
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D7831071&REV_15 ;Mitac
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12441462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_126D1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_127E1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12831462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12871462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12991462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_129A1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_129B1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12A11462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12A51462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12A71462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12AA1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12AC1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12B51462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12B81462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12B91462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12BA1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12BB1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12BD1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12BE1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12C01462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12CD1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12CE1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12E91462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12EA1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12EB1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12EC1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12ED1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12F21462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12F41462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12F51462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12F91462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_130E1462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_132E1462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13311462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13321462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13331462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13341462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13431462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79701462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79711462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79811462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79821462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79831462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_79961462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A131462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A151462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A331462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A341462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A361462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A371462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A381462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A391462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A401462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A441462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A451462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A461462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A491462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A501462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A561462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A671462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A701462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A711462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A741462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A791462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A831462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A851462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A861462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7A991462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B021462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B071462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B081462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B241462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B271462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B291462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B301462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B311462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B331462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B361462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B381462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B481462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B661462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B731462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B751462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B791462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B801462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B841462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B851462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B861462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B871462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B891462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B901462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B951462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B971462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C011462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C021462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C041462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C091462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C101462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C131462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C141462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C161462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C181462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C221462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C241462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C311462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C371462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C391462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C511462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C521462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C561462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C671462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C831462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C851462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C871462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C881462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C911462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C931462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C951462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7C961462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7D021462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7D141462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7D231462&REV_15 ;msi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7D491462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9C091462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6171462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6181462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6251462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AAC11462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AAC21462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_ACD11462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_ACD21462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AE811462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AEC11462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AF811462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0901462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A11462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A21462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1401462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1421462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1581462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1711462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B1781462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B9011462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_CC021462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D9701462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60EE17AA&REV_15 ;NEC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_611917AA&REV_15 ;NEC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_611C17AA&REV_15 ;NEC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01D61B0A&REV_15 ;Pegatron
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_22BB1B0A&REV_15 ;PEGATRON
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30031D05&REV_15 ;Pegatron
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30041D05&REV_15 ;Pegatron
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01CD1B0A&REV_15 ;Positivo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50221180&REV_15 ;Ricoh
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E401EE8&REV_15 ;Shenzhen BXC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E4F1EE8&REV_15 ;Shenzhen BXC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E501EE8&REV_15 ;Shenzhen BXC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E511EE8&REV_15 ;Shenzhen BXC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20841297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20861297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20871297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20891297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20901297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20911297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20921297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20931297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20941297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20951297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20961297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20971297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20981297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20991297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21001297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21011297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21021297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21031297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21041297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21051297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21061297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21071297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21081297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21091297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21101297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21111297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21121297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21131297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21141297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21151297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21161297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21171297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21181297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21191297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21201297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21211297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21221297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21231297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21241297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21251297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21261297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21271297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21281297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21291297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_21301297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30071297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40781297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40861297&REV_15 ;Shuttle
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01B81B0A&REV_15 ;SI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01D71B0A&REV_15 ;SI
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03141B21&REV_15 ;STLab
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11011D05&REV_15 ;Thirdwave
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102B1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_102D1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10421D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10431D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10441D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10451D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10571D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10581D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10591D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105D1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105E1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_105F1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10601D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10621D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10641D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10651D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10691D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10701D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10721D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10741D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10781D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_107C1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10851D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108A1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_108B1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_109E1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_109F1D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11001D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11021D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11041D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20121D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20131D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20151D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20161D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20171D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20181D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20191D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20201D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20211D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20221D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20231D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20241D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20251D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20261D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20271D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20281D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20291D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20301D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20311D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20321D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20341D05&REV_15 ;THTF
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10971D05&REV_15 ;THTF(Haier)
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10991D05&REV_15 ;THTF(Haier)
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00013100&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00061179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F7001179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F7101179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F7121179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F7251179&REV_15 ;TOSHIBA
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F80B1179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F8901179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F8F01179&REV_15 ;Toshiba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1019A6C2&REV_15 ;Trigem Computer Inc.
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A6C21019&REV_15 ;Trigem Computer Inc.
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0D5C1D05&REV_15 ;Tsinghua Tongfang
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0F3C1D05&REV_15 ;Tsinghua Tongfang
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60041D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60051D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60081D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60091D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60101D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60111D05&REV_15 ;Tsinghua Tongfang Co.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60121D05&REV_15 ;Tsinghua Tongfang Co.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60161D05&REV_15 ;Tsinghua Tongfang CO.,LTD
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30010526&REV_15 ;UNIS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30020526&REV_15 ;UNIS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_30030526&REV_15 ;Unis
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60020526&REV_15 ;Unis
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00061D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00071D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00081D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_000D1D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_000F1D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00101D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00121D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00141D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00161D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00171D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00181D19&REV_15 ;VAIO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A4141019&REV_15 ;Vestel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10681D05&REV_15 ;Vulcan
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_006314C0&REV_15 ;WB
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_100A15BD&REV_15 ;WHITE BRAND
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_01C61B0A&REV_15 ;Wortmann
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1B0A01C6&REV_15 ;Wortmann
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17091D72&REV_15 ;Xiaomi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_19331D72&REV_15 ;Xiaomi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_19451D72&REV_15 ;Xiaomi

; 8168H default TRx optimize Threshold 1000
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A0A1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A0C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A0D1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A0F1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A101028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A111028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A151028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A231028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A241028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A251028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A261028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A291028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A2A1028&REV_15 ;Dell

;8168H Default Disable clkreq and L1 substate
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38C717AA&REV_15 ;Lenovo

;8168H TxRx Optimize Threshold 500
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_128D1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_133C1025&REV_15 ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08C81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08CB1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08CC1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08CF1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08D21028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08D31028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08D61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08DA1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08DD1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08DE1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08F61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09681028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_096A1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F71028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09F81028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8643103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8648103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E9103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_870E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_871E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8768103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_876C103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_877E103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D6103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_885F103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8948103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89B3103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89B4103C&REV_15 ;HP

;8168H Wake On Link Up
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50D31558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65D11558&REV_15 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65E21558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67D11558&REV_15 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85211558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_95E61558&REV_15 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_97E11558&REV_15 ;Clevo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A0011E39&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5001558&REV_15 ;CLEVO

;8168H S0 Magic Packet Default Enable
%RTL8168.DeviceDesc%  = RTL8168HS0MgcPktEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AF061170&REV_15 ;Inventec
%RTL8168.DeviceDesc%  = RTL8168HS0MgcPktEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08AD1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168HS0MgcPktEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_08AE1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168HS0MgcPktEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_006611D9&REV_15 ;TEC
%RTL8168.DeviceDesc%  = RTL8168HS0MgcPktEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_900714CD&REV_15 ;USI

;8168H + RT8211FS
%RTL8168.DeviceDesc%  = RTL8168HFiber.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06121170&REV_15 ;Inventec
%RTL8168.DeviceDesc%  = RTL8168HFiber.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_080C1028&REV_15 ;DELL
%RTL8168.DeviceDesc%  = RTL8168HFiber.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_311B17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HFiber.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_315717AA&REV_15 ;Lenovo

;8168H S5 WOL Default Disable
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1123152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1124152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1125152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1126152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1127152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B3E103C&REV_15 ;HP_Bulldozer-GS
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_826A103C&REV_15 ;HP_Schumi34 1.0
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82F3103C&REV_15 ;HP_Schumi27 1.1
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8373103C&REV_15 ;HP_Suliban
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8374103C&REV_15 ;HP_MoscatoR238A
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_838B103C&REV_15 ;HP_Klingon
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_838C103C&REV_15 ;HP_Kazon
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_839D103C&REV_15 ;HP_Saurian
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_839E103C&REV_15 ;HP_Bajoron
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8419103C&REV_15 ;HP_Schumi27 3.0
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8425103C&REV_15 ;HP_Anna-KBL
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8430103C&REV_15 ;HP_Rhone
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8431103C&REV_15 ;HP_Lazio
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8432103C&REV_15 ;HP_Nihau
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8446103C&REV_15 ;HP_Aqulia
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8447103C&REV_15 ;HP_Tuscany
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8448103C&REV_15 ;HP_Vulcan
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8449103C&REV_15 ;HP_Orion
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_844B103C&REV_15 ;HP_Vorta
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_844E103C&REV_15 ;HP_Schumi34 3.1
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8475103C&REV_15 ;HP_Krabi
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84DE103C&REV_15 ;HP_Tuscany-R
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84EE103C&REV_15 ;HP_Diamaster
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84EF103C&REV_15 ;HP_Centrix
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F0103C&REV_15 ;HP_Sintra
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8526103C&REV_15 ;HP_PrincetonC
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8534103C&REV_15 ;HP_VinsonC
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8582103C&REV_15 ;HP_Savoy
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85BA103C&REV_15 ;HP_Ceramica
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8664103C&REV_15 ;HP_Savoy
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8665103C&REV_15 ;HP_Shiraz
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B6103C&REV_15 ;HP_Ceramica
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B7103C&REV_15 ;HP_Diamaster
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B8103C&REV_15 ;HP_Tuscany-R
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86B9103C&REV_15 ;HP_Apulia
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C6103C&REV_15 ;HP_Volfoni_CFLR
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86C7103C&REV_15 ;HP_Volfoni_CML
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86E4103C&REV_15 ;HP_Sintra
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86EF103C&REV_15 ;HP_Mill-W
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F0103C&REV_15 ;HP_Timber
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F1103C&REV_15 ;HP_Weaver
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F2103C&REV_15 ;HP_Monk-D
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F3103C&REV_15 ;HP_Monk-P
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F7103C&REV_15 ;HP_Village
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86F8103C&REV_15 ;HP_Mill-C
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8705103C&REV_15 ;HP_Syrah
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8708103C&REV_15 ;HP_Florence
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87F8103C&REV_15 ;HP_Cardiff(ICL-U)
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87F9103C&REV_15 ;HP_Offa(GML)
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87FA103C&REV_15 ;HP_Boudica(AMD Stoney Ridge)
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382817AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_382E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383917AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_383A17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38BC17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38FF17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60010526&REV_15 ;Unis

;8168H S5 WOL Hide and Default Disable
%RTL8168.DeviceDesc%  = RTL8168HS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_208F1043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168HS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_386917AA&REV_15 ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168HS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_387117AA&REV_15 ;LENOVO

;8168H Default S5 Arp Offload Enable and 100M Default Disable Interrupt Moderation
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_194510CF&REV_15 ;FUJI

;8168H Default S5 Arp Offload Enable
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_00171E26&REV_15 ;Fujitsu

;8168H 100M Default Disable Interrupt Moderation
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13911043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8536103C&REV_15 ;HP_Reef
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8537103C&REV_15 ;HP_Ramia
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8538103C&REV_15 ;HP_Revere
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B09A144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B09B144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B09F144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A0144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A1144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A2144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A7144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A9144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0AA144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C133144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C139144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C142144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C144144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C14C144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C14D144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C14E144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C156144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C157144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C15A144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C160144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C161144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C162144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C166144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C167144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C16A144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C16E144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C175144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C177144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C17A144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C186144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C187144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C18C144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C192144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C195144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C198144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C1A7144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C1A8144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C774144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C776144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C778144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C789144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C790144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C792144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C798144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C803144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C804144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C806144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C816144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C820144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C822144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C823144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C826144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C834144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C838144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100M.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C862144D&REV_15 ;Samsung

;8168H 100M Default Disable Interrupt Moderation and S5wol Default Disable
%RTL8168.DeviceDesc%  = RTL8168HDisIntModer100MS5wolDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_200F1043&REV_15 ;ASUS

;8168H EEE & Flow control & AdvancedEEE & GigaLite Default Disable
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_608817AA&REV_15 ;NEC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_608D17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60A017AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60A917AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60B817AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60BE17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60C317AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60C717AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60E117AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60E317AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_60FC17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_610917AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_610B17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_610D17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_612B17AA&REV_15 ;NECPC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_613917AA&REV_15 ;NECPC

;8168H Default Enable SelectiveSuspend
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_204F1043&REV_15 ;ASUS
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_40181558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50151558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50C51558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50E11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50E21558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_50F41558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_51631558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_51A11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65E11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_65E51558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67E11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_67F11558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85111558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_866B1558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_866D1558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_867B1558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_96001558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A5011558&REV_15 ;CLEVO
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_06C61028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_070C1028&REV_15 ;Dell
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_7B531462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_ACD31462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AE011462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AE031462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AE041462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_AEC21462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B0A41462&REV_15 ;MSI
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20191A58&REV_15 ;Razer
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_000C1D19&REV_15 ;VAIO

;8168H S5 WOL Hide and Default Enable Type2
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8053103C&REV_15 ;HP_Spitfire
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_805F103C&REV_15 ;HP_Berlinetta
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8060103C&REV_15 ;HP_Barchetta
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8061103C&REV_15 ;HP_Maranello
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8062103C&REV_15 ;HP_Enzo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8063103C&REV_15 ;HP_Corsa
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_806A103C&REV_15 ;HP_Dino
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80EF103C&REV_15 ;HP_Palazzo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80F0103C&REV_15 ;HP_Palazzo Carrizo-L
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80F3103C&REV_15 ;HP_Palazzo-L
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80FE103C&REV_15 ;HP_Tropicana
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_80FF103C&REV_15 ;HP_Royal
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8100103C&REV_15 ;HP_Riata
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8101103C&REV_15 ;HP_Regent
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8102103C&REV_15 ;HP_Riviera
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8103103C&REV_15 ;HP_Pixar
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8158103C&REV_15 ;HP_Tristar
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_822C103C&REV_15 ;HP_REILLY
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_822E103C&REV_15 ;HP_ROURKE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8231103C&REV_15 ;HP_RENNER
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8234103C&REV_15 ;HP_REDMAYNE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_823A103C&REV_15 ;HP_TATUM14/15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_823C103C&REV_15 ;HP_PITT-B
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_823E103C&REV_15 ;HP_PITT-S
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8245103C&REV_15 ;HP_Prost-A
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8267103C&REV_15 ;HP_Yoshi
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A1103C&REV_15 ;HP_Crux
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A2103C&REV_15 ;HP_Cetus
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A4103C&REV_15 ;HP_Carina
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A5103C&REV_15 ;HP_Virgo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82A6103C&REV_15 ;HP_Pyxis
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82C9103C&REV_15 ;HP_Anna
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82EF103C&REV_15 ;HP_Ramoth
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_834F103C&REV_15 ;HP_Bonnie
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8350103C&REV_15 ;HP_Stu
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_836E103C&REV_15 ;HP_Perceptor
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8370103C&REV_15 ;HP_Perceptor-SR
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8377103C&REV_15 ;HP_Ripper
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_837B103C&REV_15 ;HP_Ratchet
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_837D103C&REV_15 ;HP_Rollbar
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_837F103C&REV_15 ;HP_Razorclaw
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83C3103C&REV_15 ;HP_Catan
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83D0103C&REV_15 ;HP_Rubik
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F0103C&REV_15 ;HP_Sousaphone
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F1103C&REV_15 ;HP_Suona
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F2103C&REV_15 ;HP_Saxtuba
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83F3103C&REV_15 ;HP_Mandolin
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83FD103C&REV_15 ;HP_Ramjet
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_846E103C&REV_15 ;HP_CarinaB
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8471103C&REV_15 ;HP_Ramjet_OOC
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84D8103C&REV_15 ;HP_Rumble
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F5103C&REV_15 ;HP_Pippin3
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8521103C&REV_15 ;HP_Balos1.0
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8524103C&REV_15 ;HP_Balos2.0
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8598103C&REV_15 ;HP_Saxtuba-R
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8599103C&REV_15 ;HP_Sousaphone-R
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_859A103C&REV_15 ;HP_Suona-R
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85A3103C&REV_15 ;HP_Reiley13
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85A5103C&REV_15 ;HP_Reiley14
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85AA103C&REV_15 ;HP_Reiley15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85AD103C&REV_15 ;HP_Pelican
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85D9103C&REV_15 ;HP_Pigeon14/15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CA103C&REV_15 ;HP_Mulan
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86CF103C&REV_15 ;HP_Aloe1.0
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D0103C&REV_15 ;HP_Aloe2.0
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D1103C&REV_15 ;HP_Pangu
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86FB103C&REV_15 ;HP_PrincetonR
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86FC103C&REV_15 ;HP_VinsonR
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_872C103C&REV_15 ;HP_Cubano
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_872E103C&REV_15 ;HP_Doppio
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8730103C&REV_15 ;HP_Pecan14/15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_873A103C&REV_15 ;HP_Yellowfin
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_876B103C&REV_15 ;HP_Sycamore
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8777103C&REV_15 ;HP_Jorah
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87DF103C&REV_15 ;HP_Reeds 13
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87E0103C&REV_15 ;HP_Rabon 14
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87E1103C&REV_15 ;HP_Raritan 15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87E2103C&REV_15 ;HP_Dianshan 14
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8861103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8864103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8867103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_886A103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_887D103C&REV_15 ;HP
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9176103C&REV_15 ;HP_Miramax
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8105103C&REV_15 ;HP TC

;8168H S5 WOL Hide and Default Enable Type2 and Default Disable 100M interrupt moderation
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_869B103C&REV_15 ;HP_Rimu
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_869D103C&REV_15 ;HP_Redbay
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86A0103C&REV_15 ;HP_Redpine
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86A3103C&REV_15 ;HP_Sourwood13
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86A5103C&REV_15 ;HP_Sourwood14
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86A8103C&REV_15 ;HP_Sourwood15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_859B103C&REV_15 ;HP Saxtuba-R
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_859C103C&REV_15 ;HP Mandolin-R

;8168H S5 WOL Hide and Default Enable Type2 and Default Enable SelectiveSuspend
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2B4C103C ;HP_Superion

;8168H Default disable S5WOL and GreenEthernet
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1380152D&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1384152D&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1238152D&REV_15 ;CB-Haier
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_18540378&REV_15 ;CB-Haier
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1244152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1248152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1282152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1284152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1297152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1344152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1330152D&REV_15 ;Haier
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1354152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1360152D&REV_15 ;HUAWEI
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03541854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34901458&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34911458&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34921458&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34931458&REV_15 ;CB
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1122152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1137152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1138152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1139152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1148152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1149152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1150152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1151152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1156152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1157152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1166152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1167152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1169152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1176152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1177152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1185152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1199152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1201152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1209152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1217152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1218152D&REV_15 ;Channel
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02591854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02601854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02611854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02651854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02661854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02891854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02921854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_02931854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03041854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03051854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03211854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03351854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03421854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03781854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03881854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_03941854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04091854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04121854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04311854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_04601854&REV_15 ;LG
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1317152D&REV_15 ;Quanta
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisableGreenEthernetDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1315152D&REV_15 ;Qunata

;8168H Default Enable CS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D6158086&REV_15 ;Intel
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20838086&REV_15 ;Intel Corporation
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20958086&REV_15 ;Intel Corporation
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313D17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_313E17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F217AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F317AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F417AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36F517AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_F008144D&REV_15 ;Samsung
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_19031D72&REV_15 ;Xiaomi

;8168H Default enable RTD3 and disable S5WOL
%RTL8168.DeviceDesc%  = RTL8168HSSS5wolDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_209F1043&REV_15 ;Asus

;8168H Disable force clkreq
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38E017AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38F617AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_38FA17AA&REV_15 ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_508117AA&REV_15 ;Lenovo

; 8118AS_16
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_16
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_16
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098D1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09951025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_11631025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12261025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_122C1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12381025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_123C1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12561025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12681025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_127C1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_12891025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14331025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14471025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144F1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14551025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14751025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14761025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148A1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148B1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14951025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15031025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_152D1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_154E1025&REV_16 ;ACER
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15611025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15671025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15731025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157A1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157B1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157C1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157D1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_157E1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16071025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_160A1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_160B1025&REV_16 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_23131565&REV_16 ;BIOSTAR
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E401EE8&REV_16 ;bitland
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E4F1EE8&REV_16 ;bitland
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E501EE8&REV_16 ;bitland
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E511EE8&REV_16 ;bitland
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1019&REV_16 ;ECS
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9CEA1019&REV_16 ;ECS
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E65105B&REV_16 ;FOXCONN
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14641458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15601458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16501458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16511458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16521458&REV_16 ;Gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16531458&REV_16 ;Gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_25541458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_25551458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_45551458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_47561458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A7571458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B4561458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_B7581458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_C5561458&REV_16 ;GIGABYTE
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D4561458&REV_16 ;Gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D5551458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_D5571458&REV_16 ;gigabyte
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15111458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15121458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15131458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15141458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15151458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_16 ;Giga-Byte Technology
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8307103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8308103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8309103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_838F103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8390103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8391103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8392103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8393103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8394103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_839F103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8437103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8466103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8467103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8468103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8469103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_846A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_846B103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8477103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8478103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8479103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84DA103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84DB103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84DC103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84F6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84FD103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_84FE103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8509103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8572103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8573103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8574103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8575103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FA103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FB103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FC103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FD103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FE103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_85FF103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8600103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8601103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8602103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8603103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8604103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8605103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8606103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8607103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_860A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D2103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D3103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D4103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_86D6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8703103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8704103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8740103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8741103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8742103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8744103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8745103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8746103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8747103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8748103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8749103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_874A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8786103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8787103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8788103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_878A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_878B103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_878C103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B0103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B1103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B2103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B3103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87B5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87C3103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87DA103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_886B103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_886C103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8876103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88C8103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88C9103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88CA103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88CB103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88D1103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88D2103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DD103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DE103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88DF103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88E4103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88E5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88E6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88E7103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88EB103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88EC103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88ED103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88EE103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F4103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F7103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F8103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88F9103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88FA103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88FD103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88FE103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_88FF103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8900103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8901103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8902103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8911103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8912103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8917103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8918103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8934103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_893C103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_893D103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8949103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_894A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89EB103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A13103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A14103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A15103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A16103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A17103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A18103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A19103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A1A103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A21103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A22103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A25103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A26103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8A27103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_126E152D&REV_16 ;HUAWEI
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2A19E5&REV_16 ;Huawei
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_3E2B19E5&REV_16 ;Huawei
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36D917AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E717AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E817AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36E917AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_36EF17AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370417AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_370917AA&REV_16 ;Lenovo
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17051D72&REV_16 ;Xiaomi
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_18011D72&REV_16 ;Xiaomi
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_18061D72&REV_16 ;Xiaomi

;8118AS_16 TxRx Optimize Threshold 500
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8643103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8653103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8767103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87D6103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8860103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_8906103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89B5103C&REV_16 ;HP
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_89D8103C&REV_16 ;HP

; 8118AS_17
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_17
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_17
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_098D1025&REV_17 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_09951025&REV_17 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8186&SUBSYS_81AA1019&REV_17 ;ECS
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0E65105B&REV_17 ;FOXCONN

; 8168K
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&REV_1B
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1B
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13881025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13891025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_138A1025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_138B1025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14131025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14151025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142D1025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148D1025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14901025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14911025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_152E1025&REV_1B ;Acer
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_205F1043&REV_1B ;ASUS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A4C1028&REV_1B ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A4D1028&REV_1B ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A541028&REV_1B ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0A551028&REV_1B ;Dell
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_0AC51028&REV_1B ;DELL
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_81BB1019&REV_1B ;ECS
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_1B ;GIGABYTE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_FE011458&REV_1B ;GIGABYTE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_10001458&REV_1B ;Giga-Byte Technology
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314C17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_314D17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_316717AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317417AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_317917AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319417AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319B17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319C17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319D17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_319E17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31AF17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31B017AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31B417AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31B517AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31BB17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31BC17AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_31C217AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32C117AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32C617AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32D117AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32D217AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32D317AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32D417AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E617AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E717AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32E917AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32F317AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_32F517AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_330217AA&REV_1B ;Lenovo
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_373F17AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374017AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_374117AA&REV_1B ;LENOVO
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_375317AA&REV_1B ;Lenovo

; 8168K default disable EEE
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1A411462&REV_1B ;SHARP

;8168K S5 WOL Default Disable
%RTL8168.DeviceDesc%  = RTL8168HS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_200F1043&REV_1B ;ASUS

;8168K S5 WOL Hide and Default Disable
%RTL8168.DeviceDesc%  = RTL8168HS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_208F1043&REV_1B ;ASUS

;8168K Default enable SelectiveSuspend
%RTL8168.DeviceDesc%  = RTL8168HSS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_204F1043&REV_1B ;ASUS

; 8168L
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&REV_1E
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1E

; 8118AN
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_20
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_20
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13491025&REV_20 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_134A1025&REV_20 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14981025&REV_20 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149B1025&REV_20 ;Acer

; 8118ASA
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_25
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_25
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13311025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13331025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13381025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_133A1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13661025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_13971025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_139D1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_139F1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142E1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143D1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143F1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14411025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14431025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14451025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14471025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14481025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144F1025&REV_25 ;Acer
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_14551025&REV_25 ;Acer

; 8118ASU
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_26
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_26
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_87C31043&REV_26 ;ASUS

; 8118K
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_27
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_27


; 8107E
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&REV_0A
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0A
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_089C1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_089D1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08A71028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08A81028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08BC1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08BD1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08BE1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08BF1028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08C01028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08C11028&REV_0A ;Dell
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08FA1028&REV_0A ;DELL
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_08FB1028&REV_0A ;DELL
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_092A1028&REV_0A ;DELL
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_092B1028&REV_0A ;DELL
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_806E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8073103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8074103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8075103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8092103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8093103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8094103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8095103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8096103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8097103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8098103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8099103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_809A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A0103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A1103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A2103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A3103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A4103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A5103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A6103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A7103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A8103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80A9103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_80D1103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8119103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_811A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8136103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_816B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_816C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_816D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_816E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_816F103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8189103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_818A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_818B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_818C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_818D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_818E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_819F103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8209103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_820F103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8210103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8211103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8212103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8213103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8214103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8215103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8216103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8217103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8218103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8219103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_821A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_821B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_821C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8257103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8258103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8259103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_825F103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8260103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8261103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8262103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8263103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8264103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8294103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_82EA103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_835E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_835F103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8360103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8361103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8362103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8363103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8364103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8365103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8366103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8367103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8368103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8369103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_836A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_836B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_836C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83A3103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83A4103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83C0103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83CD103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83CE103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83F6103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83F7103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83F8103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83F9103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83FA103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83FB103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_840D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_841B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_841C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8421103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8422103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_845E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84B9103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BA103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BB103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BC103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BD103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BE103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84BF103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84C0103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84C1103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84C2103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84C3103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84C4103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84ED103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84F7103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_84F8103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_856A103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8581103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_861B103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_861C103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_861D103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_861E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8640103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8641103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_865E103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8692103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8693103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8694103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_8695103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86AA103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86AB103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86AC103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86E1103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86E2103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_86E3103C&REV_0A ;HP
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_003417AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30DA17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_362E17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_363617AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_380D17AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_380E17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_381A17AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382617AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382717AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382817AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382917AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382A17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_382E17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383217AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383317AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383417AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383517AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383617AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383717AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383817AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_384617AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_384D17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_385717AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_385817AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_385C17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_386217AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_386717AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_386817AA&REV_0A ;LENOVO
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_386A17AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_22BA1B0A&REV_0A ;PEGATRON
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_F7001179&REV_0A ;Toshiba
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_F7251179&REV_0A ;TOSHIBA
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_F80B1179&REV_0A ;Toshiba

;8107E S5 WOL Default Disable
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383017AA&REV_0A ;Lenovo
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_383917AA&REV_0A ;Lenovo



;
; NDI: This section declares your network interface characteristics.
;
[RTL8168H.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

[RTL8168HDisIntModer100M.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = DisIntModer100M.kw

[RTL8168HDisIntModer100MS5wolDisable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
;AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = DisIntModer100M.kw
AddReg                  = s5woldefaultdisable.kw

[RTL8168HS5WOLDisableGreenEthernetDisable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
;AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
;AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = GreenEthDisabled.kw
AddReg                  = s5woldefaultdisable.kw

[RTL8168HSSS5wolDisable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
;AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = s5woldefaultdisable.kw

[RTL8168HSS.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

[RTL8168HS0MgcPktEnable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = S0MgcPktEnabled.kw

[RTL8168HFiber.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEEDisable.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw
AddReg                  = S0MgcPktEnabled.kw
AddReg                  = FiberMode1.kw

[RTL8168HS5WOLDisable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
;AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = s5woldefaultdisable.kw

[RTL8168HS5WOLHideDisable.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
;AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

AddReg                  = s5wolhidedisable.kw

[RTL8118AS.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw, Speed1000.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = Jumboframe9k.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = GreenEthEnabled.kw
AddReg                  = EEEDisable.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = GigaLite.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw
AddReg                  = GPPSWEnabled.kw

[RTL8107E.ndi.NT]
;FeatureScore            = 0xFF

Characteristics         = 0x04  ; NCF_PHYSICAL

; TODO: Update with the type of bus (PCI, USB, or custom) your device uses.
BusType                 = 5     ; PCIBus

; TODO: Update these next 3 values based on your device's media type.
*IfType                 = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType              = 0     ; NdisMedium802_3
*PhysicalMediaType      = 14    ; NdisPhysicalMedium802_3

; TODO: Set this to 0 if your device is not a physical device.
*IfConnectorPresent     = 1     ; true

; In most cases, you can keep these at their default values.
*ConnectionType         = 1     ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0     ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2     ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0     ; false

CopyFiles               = MyCopyFiles
AddReg                  = ndi.reg

; To make it easier to share common keywords across different devices, we have
; a separate AddReg section for each Advanced Keyword.
; TODO: Add or remove keywords depending on the features your NIC supports.
DelReg                  = del.reg
AddReg                  = Common.kw
AddReg                  = Speed.kw
AddReg                  = NetworkAddress.kw
AddReg                  = FlowControl.kw
AddReg                  = WakeOnPattern.kw
AddReg                  = WakeOnMagicPacket.kw
AddReg                  = WolShutdownLinkSpeed.kw
AddReg                  = InterruptModeration.kw
;AddReg                  = InterruptModerationLevel.kw
AddReg                  = OffloadChecksum.kw
AddReg                  = OffloadLsoV2.kw
AddReg                  = PriorityVlanTag.kw
AddReg                  = TxRxBuf.kw
;AddReg                  = Rss.kw, Rss4Q.kw
AddReg                  = EEE.kw
AddReg                  = AdvancedEEEDisable.kw
AddReg                  = ArpNsProtOffload.kw
AddReg                  = s5wol.kw
AddReg                  = PDPllEnabled.kw
AddReg                  = Rsc.kw
;AddReg                  = IdleRestriction.kw


[ndi.reg]
; TODO: Update these if your device is not Ethernet.
; Note that "ndis5" simply means to bind to TCPIP; it is not a version number.
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR, Ndi,               Service,    0, %ServiceName%

[RTL8168H.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HDisIntModer100M.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HDisIntModer100MS5wolDisable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HS5WOLDisableGreenEthernetDisable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HSSS5wolDisable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HSS.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HS0MgcPktEnable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HFiber.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HS5WOLDisable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8168HS5WOLHideDisable.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8118AS.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf

[RTL8107E.ndi.NT.Wdf]
KmdfService = %ServiceName%, wdf


[wdf]
KmdfLibraryVersion      = 1.31


[RTL8168H.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HDisIntModer100M.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HDisIntModer100MS5wolDisable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HS5WOLDisableGreenEthernetDisable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HSSS5wolDisable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HSS.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HS0MgcPktEnable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HFiber.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HS5WOLDisable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8168HS5WOLHideDisable.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8118AS.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported

[RTL8107E.ndi.NT.HW]
AddReg = MSI.01.AddReg
Include = pci.inf
Needs = PciIoSpaceNotRequired.HW
; Needs = PciASPMOptOut.HW
; Needs = PciD3ColdSupported


[MSI.00.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[MSI.01.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[MSI.04.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4

[MSI.16.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 16

[MSI.32.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 32


[RTL8168H.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HDisIntModer100M.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HDisIntModer100MS5wolDisable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HS5WOLDisableGreenEthernetDisable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HSSS5wolDisable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HSS.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HS0MgcPktEnable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HFiber.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HS5WOLDisable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8168HS5WOLHideDisable.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8118AS.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog

[RTL8107E.ndi.NT.Services]
AddService = %ServiceName%, 2, rt68cx21.Service, Service.EventLog



[rt68cx21.Service]
DisplayName             = %Service.DisplayName%
ServiceType             = 1 ; SERVICE_KERNEL_DRIVER
StartType               = 3 ; SERVICE_DEMAND_START
ErrorControl            = 1 ; SERVICE_ERROR_NORMAL
; TODO: Update the name of your binary.
ServiceBinary           = %13%\rt68cx21x64.sys
; ServiceBinary           = %12%\rt68cx21x64.sys
AddReg                  = rt68cx21.Service.Reg
AddReg                  = DrvOption.reg, DrvMode.reg, DMAr.reg

[rt68cx21.Service.Reg]
HKR,,                   BootFlags, 0x00010001, 1 ; CM_SERVICE_NETWORK_BOOT_LOAD

[Service.EventLog]
AddReg                  = Service.AddEventLog.reg

[Service.AddEventLog.reg]
HKR,,                   EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%13%\rt68cx21x64.sys"
HKR,,                   TypesSupported,   0x00010001, 7

; TODO: List off all the binaries that are part of your driver package.
; Typically this is just the .sys file.
[MyCopyFiles]
rt68cx21x64.sys

[DestinationDirs]
MyCopyFiles   = 13
; MyCopyFiles   = 12

[SourceDisksNames]
1 = %DiskDescription%

[SourceDisksFiles]
rt68cx21x64.sys         = 1

;
; Advanced Keywords
;
[Common.kw]
HKR,,DeviceRemovable,0,"0"

HKR,,HwParaMask,0x00010001,0

HKR,,HwPciOtherFunDevMask,0x00010001,0

HKR,,HwOptimize,0x00010001,0

HKR,,HwOption,0x00010001,0

HKR,,HwWolCrcVal,0x00010001,0

HKR,,LogDisconnectEvent,0,"0"

HKR,,EnableEDT,0,"1"

HKR,,RIACP,0,"0"

HKR,,S5NicKeepOverrideMacAddr,0,"0"

HKR,,S5NicKeepOverrideMacAddrV2,0,"1"

HKR,,PPSW,0,"1"

HKR,,GPPSW,0,"0"

HKR,,S0MgcPkt,0,"0"

HKR,,HwFPSM,0x00010001,0

HKR,,SwIML,0x00010001,0

HKR,,SwIML100,0x00010001,0

HKR,,SwIMLV2,0x00010001,0

HKR,,SwIML100V2,0x00010001,0

HKR,,ENPWMode,0,"0"

HKR,,Diskless,0,"0"

HKR,,DisklessOption,0,"0"

HKR,,TxOptimizeThreshold,0x00010001,0

HKR,,RxOptimizeThreshold,0x00010001,0

HKR,,CFHTime,0x00010001,0

HKR,,LDWTime,0x00010001,0

HKR,,RMPT,0x00010001,0

HKR,,CRSPDThreshold,0x00010001,0

HKR,,ComboPerfAdjust,0,"0"

HKR,,CHNLWTime,0x00010001,0

HKR,,CHNLWCnt,0x00010001,0

HKR,,L1L0sLT,0x00010001,0

HKR,,MRRSize,0x00010001,0

HKR,,TDBSize,0x00010001,0xFFFFFFFF

HKR,,RDBSize,0x00010001,0xFFFFFFFF

HKR,,HwOptionV2,0x00010001,0

HKR,,HwOptionV3,0x00010001,0

HKR,,HwOptionV4,0x00010001,0

HKR,,HwBpMask,0x00010001,0

HKR,,MonitorModeEnabled,0,"0"

HKR,,UCEM,0x00010001,0

HKR,,FactoryMode,0,"0"

HKR,,SwParaMask,0x00010001,0

HKR,,ForceMode,0,"0"

HKR,Ndi\params\PowerSavingMode,    ParamDesc,  0, %PowerSavingMode%
HKR,Ndi\params\PowerSavingMode,    default,    0, "1"
HKR,Ndi\params\PowerSavingMode,    type,       0, "enum"
HKR,Ndi\params\PowerSavingMode\enum,   "0",    0, %Disabled%
HKR,Ndi\params\PowerSavingMode\enum,   "1",    0, %Enabled%
HKR,,PowerSavingMode,0,"1"

[Speed.kw]
HKR,Ndi\params\*SpeedDuplex,                    ParamDesc,      0,  %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,                    default,        0,  "0"
HKR,Ndi\params\*SpeedDuplex,                    type,           0,  "enum"
HKR,Ndi\params\*SpeedDuplex\enum,               "0",            0,  %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,               "1",            0,  %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,               "2",            0,  %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,               "3",            0,  %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,               "4",            0,  %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

[Speed1000.kw]
HKR,Ndi\params\*SpeedDuplex\enum,               "6",            0,  %1000Mb-Full-Duplex%

[Speed2500.kw]
HKR,Ndi\params\*SpeedDuplex\enum,               "2500",         0,  %2.5Gb-Full-Duplex%

[DisIntModer100M.kw]
HKR,,SwIML100,0x00010001,0x140

[NetworkAddress.kw]
HKR,Ndi\params\NetworkAddress,                  ParamDesc,      0,  %NetworkAddress%
HKR,Ndi\params\NetworkAddress,                  type,           0,  "edit"
HKR,Ndi\params\NetworkAddress,                  default,        0,  ""
HKR,Ndi\params\NetworkAddress,                  LimitText,      0,  "12"
HKR,Ndi\params\NetworkAddress,                  UpperCase,      0,  "1"
HKR,Ndi\params\NetworkAddress,                  Optional,       0,  "1"

[FlowControl.kw]
HKR,Ndi\params\*FlowControl,                    ParamDesc,      0,  %FlowControl%
HKR,Ndi\params\*FlowControl,                    default,        0,  "3"
HKR,Ndi\params\*FlowControl,                    type,           0,  "enum"
HKR,Ndi\params\*FlowControl\enum,               "0",            0,  %Disabled%
;HKR,Ndi\params\*FlowControl\enum,               "1",            0,  %TxEnabled%
;HKR,Ndi\params\*FlowControl\enum,               "2",            0,  %RxEnabled%
HKR,Ndi\params\*FlowControl\enum,               "3",            0,  %RxTxEnabled%
HKR,,*FlowControl,0,"3"

[WakeOnPattern.kw]
HKR,Ndi\params\*WakeOnPattern,                  ParamDesc,      0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,                  default,        0, "1"
HKR,Ndi\params\*WakeOnPattern,                  type,           0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,             "0",            0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,             "1",            0, %Enabled%
HKR,,*WakeOnPattern,0,"1"

[WakeOnMagicPacket.kw]
HKR,Ndi\params\*WakeOnMagicPacket,              ParamDesc,      0,  %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,              default,        0,  "1"
HKR,Ndi\params\*WakeOnMagicPacket,              type,           0,  "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,         "0",            0,  %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,         "1",            0,  %Enabled%
HKR,,*WakeOnMagicPacket,0,"1"

[GreenEthEnabled.kw]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
;HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "1"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"1"

[GreenEthDisabled.kw]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
;HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "0"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"0"

[ArpNsProtOffload.kw]
HKR,Ndi\params\*PMARPOffload,       ParamDesc,  0, %ArpOffload%
HKR,Ndi\params\*PMARPOffload,       default,    0, "1"
HKR,Ndi\params\*PMARPOffload,       type,       0, "enum"
HKR,Ndi\params\*PMARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*PMARPOffload\enum,  "1",        0, %Enabled%
HKR,,*PMARPOffload,0,"1"

HKR,Ndi\params\*PMNSOffload,        ParamDesc,  0, %NsOffload%
HKR,Ndi\params\*PMNSOffload,        default,    0, "1"
HKR,Ndi\params\*PMNSOffload,        type,       0, "enum"
HKR,Ndi\params\*PMNSOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*PMNSOffload\enum,   "1",        0, %Enabled%
HKR,,*PMNSOffload,0,"1"

[EEEMaxSupportSpeed2500_1000.kw]
HKR,Ndi\params\EEEMaxSupportSpeed,       ParamDesc,  0, %EEEMaxSupportSpeed%
HKR,Ndi\params\EEEMaxSupportSpeed,       default,    0, "1000"
HKR,Ndi\params\EEEMaxSupportSpeed,       type,       0, "enum"
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "10",       0, %10Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "100",      0, %100Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "1000",     0, %1000Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "2500",     0, %2.5Gb-Full-Duplex%
HKR,,EEEMaxSupportSpeed,0,"1000"

[EEE.kw]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "1"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"1"

[EEEDisable.kw]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "0"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"0"

[AdvancedEEEDisable.kw]
HKR, Ndi\params\AdvancedEEE,        ParamDesc,  0, %AdvancedEEE%
;HKR, Ndi\params\AdvancedEEE,        optional,   0, "1"
HKR, Ndi\params\AdvancedEEE,        type,       0, "enum"
HKR, Ndi\params\AdvancedEEE,        default,    0, "0"
HKR, Ndi\params\AdvancedEEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\AdvancedEEE\enum,   "1",        0, %Enabled%
HKR,,AdvancedEEE,0,"1"

[GigaLite.kw]
HKR, Ndi\params\GigaLite,        ParamDesc,  0, %GigaLite%
;HKR, Ndi\params\GigaLite,        optional,   0, "1"
HKR, Ndi\params\GigaLite,        type,       0, "enum"
HKR, Ndi\params\GigaLite,        default,    0, "1"
HKR, Ndi\params\GigaLite\enum,   "0",        0, %Disabled%
HKR, Ndi\params\GigaLite\enum,   "1",        0, %Enabled%
HKR,,GigaLite,0,"1"

[InterruptModeration.kw]
HKR,Ndi\Params\*InterruptModeration,            ParamDesc,      0,  %InterruptModeration%
HKR,Ndi\Params\*InterruptModeration,            Type,           0,  "enum"
HKR,Ndi\Params\*InterruptModeration\enum,       "0",            0,  %IMDisabled%
HKR,Ndi\Params\*InterruptModeration\enum,       "1",            0,  %IMEnabled%
HKR,Ndi\Params\*InterruptModeration,            Default,        0,  "1"

[InterruptModerationLevel.kw]
HKR,Ndi\Params\InterruptModerationLevel,        ParamDesc,      0,  %InterruptModerationLevel%
HKR,Ndi\Params\InterruptModerationLevel,        Type,           0,  "enum"
HKR,Ndi\Params\InterruptModerationLevel\enum,   "0",            0,  %IMLow%
HKR,Ndi\Params\InterruptModerationLevel\enum,   "1",            0,  %IMMedium%
HKR,Ndi\Params\InterruptModerationLevel,        Default,        0,  "0"
HKR,Ndi\params\InterruptModerationLevel,        Optional,       0,  "1"
HKR,,*InterruptModeration,0,"1"

[OffloadChecksum.kw]
HKR,Ndi\params\*IPChecksumOffloadIPv4,          ParamDesc,      0,  %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,          default,        0,  "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,          type,           0,  "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,     "0",            0,  %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,     "1",            0,  %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,     "2",            0,  %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,     "3",            0,  %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,         ParamDesc,      0,  %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,         default,        0,  "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,         type,           0,  "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,    "0",            0,  %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,    "1",            0,  %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,    "2",            0,  %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,    "3",            0,  %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,         ParamDesc,      0,  %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,         default,        0,  "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,         type,           0,  "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,    "0",            0,  %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,    "1",            0,  %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,    "2",            0,  %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,    "3",            0,  %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv6,         ParamDesc,      0,  %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,         default,        0,  "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,         type,           0,  "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,    "0",            0,  %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,    "1",            0,  %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,    "2",            0,  %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,    "3",            0,  %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,         ParamDesc,      0,  %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,         default,        0,  "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,         type,           0,  "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,    "0",            0,  %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,    "1",            0,  %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,    "2",            0,  %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,    "3",            0,  %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

[OffloadLsoV2.kw]
HKR,Ndi\params\*LsoV2IPv4,                      ParamDesc,      0,  %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,                      default,        0,  "1"
HKR,Ndi\params\*LsoV2IPv4,                      type,           0,  "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,                 "0",            0,  %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,                 "1",            0,  %Enabled%
HKR,,*LsoV2IPv4,0,"1"

HKR,Ndi\params\*LsoV2IPv6,                      ParamDesc,      0,  %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,                      default,        0,  "1"
HKR,Ndi\params\*LsoV2IPv6,                      type,           0,  "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,                 "0",            0,  %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,                 "1",            0,  %Enabled%
HKR,,*LsoV2IPv6,0,"1"

[Rsc.kw]
HKR, Ndi\params\*RscIPv4,                       ParamDesc,  0, %RscIPv4%
HKR, Ndi\params\*RscIPv4,                       Default,    0, "0"
HKR, Ndi\params\*RscIPv4,                       Type,       0, "enum"
HKR, Ndi\params\*RscIPv4\enum,                  "0",        0, %Disabled%
HKR, Ndi\params\*RscIPv4\enum,                  "1",        0, %Enabled%
HKR,,*RscIPv4,0,"0"

HKR, Ndi\params\*RscIPv6,                       ParamDesc,  0, %RscIPv6%
HKR, Ndi\params\*RscIPv6,                       Default,    0, "0"
HKR, Ndi\params\*RscIPv6,                       Type,       0, "enum"
HKR, Ndi\params\*RscIPv6\enum,                  "0",        0, %Disabled%
HKR, Ndi\params\*RscIPv6\enum,                  "1",        0, %Enabled%
HKR,,*RscIPv6,0,"0"

[PriorityVlanTag.kw]
HKR,Ndi\Params\*PriorityVlanTag,                ParamDesc,      0,  %PriorityVLAN%
HKR,Ndi\Params\*PriorityVlanTag,                Default,        0,  "3"
HKR,Ndi\Params\*PriorityVlanTag,                Type,           0,  "enum"
HKR,Ndi\Params\*PriorityVlanTag\enum,           "0",            0,  %PriorityVLANDisabled%
HKR,Ndi\Params\*PriorityVlanTag\enum,           "1",            0,  %PriorityEnabled%
HKR,Ndi\Params\*PriorityVlanTag\enum,           "2",            0,  %VLANEnabled%
HKR,Ndi\Params\*PriorityVlanTag\enum,           "3",            0,  %PriorityVLANEnabled%
HKR,,*PriorityVlanTag,0,"3"

[TxRxBuf.kw]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "32"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "8"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "32"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "8"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[TxRxBuf8125.kw]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "32"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "8"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "512"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "64"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "4096"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "8"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"512"

[Jumboframe9k.kw]
HKR,Ndi\params\*JumboPacket,                    ParamDesc,      0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,                    default,        0, "1514"
HKR,Ndi\params\*JumboPacket,                    type,           0, "enum"
HKR,Ndi\params\*JumboPacket\enum,               "1514",         0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,               "4088",         0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,               "9014",         0, %9KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe16k.kw]
HKR,Ndi\params\*JumboPacket\enum,               "16128",        0, %16KBMTU%

[Rss.kw]
HKR,Ndi\params\*RSS,                            ParamDesc,      0, %RSS%
HKR,Ndi\params\*RSS,                            default,        0, "1"
HKR,Ndi\params\*RSS,                            type,           0, "enum"
HKR,Ndi\params\*RSS\enum,                       "0",            0, %Disabled%
HKR,Ndi\params\*RSS\enum,                       "1",            0, %Enabled%
HKR,,*RSS,0,"1"

[Rss4Q.kw]
HKR, Ndi\Params\*NumRssQueues,                  ParamDesc,      0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,                  default,        0, "4"
HKR, Ndi\Params\*NumRssQueues,                  type,           0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,             "1",            0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,             "2",            0, %2Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,             "4",            0, %4Queue%
HKR,,*NumRssQueues,0,"4"

[Rss4Q_2Q.kw]
HKR, Ndi\Params\*NumRssQueues,                  ParamDesc,      0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,                  default,        0, "2"
HKR, Ndi\Params\*NumRssQueues,                  type,           0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,             "1",            0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,             "2",            0, %2Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,             "4",            0, %4Queue%
HKR,,*NumRssQueues,0,"2"

[WolShutdownLinkSpeed.kw]
HKR,Ndi\params\WolShutdownLinkSpeed,           ParamDesc,       0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,           default,         0, "0"
;HKR,Ndi\params\WolShutdownLinkSpeed,          optional,        0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,           type,            0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,      "0",             0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,      "1",             0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,      "2",             0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"0"

[s5wol.kw]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
;HKR,Ndi\params\S5WakeOnLan,      optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[s5woldefaultdisable.kw]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "0"
;HKR,Ndi\params\S5WakeOnLan,       optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"0"

[s5wolhideenable.kw]
HKR,,S5WakeOnLan,0,"1"

[s5wolhidedisable.kw]
HKR,,S5WakeOnLan,0,"0"

[IdleRestriction.kw]
HKR,Ndi\params\*IdleRestriction,        ParamDesc,  0, %IdleRestriction%
HKR,Ndi\params\*IdleRestriction,        default,    0, "0"
HKR,Ndi\params\*IdleRestriction,        type,       0, "enum"
HKR,Ndi\params\*IdleRestriction\enum,   "0",        0, %RestrictionDisable%
HKR,Ndi\params\*IdleRestriction\enum,   "1",        0, %RestrictionEnable%
HKR,,*IdleRestriction,0,"0"

[PDPllEnabled.kw]
HKR,,PowerDownPll,0,"1"

[GPPSWEnabled.kw]
HKR,,GPPSW,0,"1"

[S0MgcPktEnabled.kw]
HKR,,S0MgcPkt,0,"1"

[FiberMode1.kw]
HKR,,HwFiberModeVer,0x00010001,1
HKR,,HwFiberStat,0,"0"

[DrvOption.reg]
HKR,Parameters,DrvOption,0x00010001,0

[DrvMode.reg]
HKR,Parameters,DrvMode,0x00010001,0

[DMAr.reg]
HKR,Parameters,DmaRemappingCompatible,0x00010001,2
;1 = opt-in, 2 = opt-in only for external devices

[del.reg]
HKR,Ndi\params

HKR,,*RSS
HKR,,*NumRssQueues
HKR,,*RscIPv4
HKR,,*RscIPv6
HKR,,InterruptModerationLevel

HKR,,ForceMode
HKR,,DisablePBA
HKR,,PowerDownPll
HKR,,ForceEnableClkReq
HKR,,JumboFrame
HKR,,AIPSMode
HKR,,S3S4WolPowerSaving
HKR,,LimitCbJumboFrame
HKR,,DeviceRemovable
HKR,,HwParaMask
HKR,,HwPciOtherFunDevMask
HKR,,HwOptimize
HKR,,HwOption
HKR,,HwWolCrcVal
HKR,,LogDisconnectEvent
HKR,,EnableEDT
HKR,,RIACP
HKR,,S5NicKeepOverrideMacAddr
HKR,,S5NicKeepOverrideMacAddrV2
HKR,,PPSW
HKR,,GPPSW
HKR,,S0MgcPkt
HKR,,HwFPSM
HKR,,SwIML
HKR,,SwIML100
HKR,,SwIMLV2
HKR,,SwIML100V2
HKR,,ENPWMode
HKR,,Diskless
HKR,,DisklessOption
HKR,,TxOptimizeThreshold
HKR,,RxOptimizeThreshold
HKR,,CFHTime
HKR,,LDWTime
HKR,,RMPT
HKR,,CRSPDThreshold
HKR,,ComboPerfAdjust
HKR,,CHNLWTime
HKR,,CHNLWCnt
HKR,,L1L0sLT
HKR,,MRRSize
HKR,,TDBSize
HKR,,RDBSize
HKR,,HwOptionV2
HKR,,HwOptionV3
HKR,,HwOptionV4
HKR,,HwBpMask
HKR,,MonitorModeEnabled
HKR,,UCEM
HKR,,HwFiberModeVer
HKR,,HwFiberStat
HKR,,FactoryMode

[del.default.reg]
HKR,,*SpeedDuplex
HKR,,NetworkAddress
HKR,,*FlowControl
HKR,,*PriorityVLANTag
HKR,,*InterruptModeration
HKR,,InterruptModerationLevel
HKR,,*ReceiveBuffers
HKR,,*TransmitBuffers
HKR,,*JumboPacket
HKR,,*TCPChecksumOffloadIPv4
HKR,,*TCPChecksumOffloadIPv6
HKR,,*UDPChecksumOffloadIPv4
HKR,,*UDPChecksumOffloadIPv6
HKR,,*IPChecksumOffloadIPv4
HKR,,*LsoV1IPv4
HKR,,*LsoV2IPv4
HKR,,*LsoV2IPv6
HKR,,*RscIPv4
HKR,,*RscIPv6
HKR,,*RSS
HKR,,*NumRssQueues
HKR,,*WakeOnPattern
HKR,,*WakeOnMagicPacket
HKR,,*PMARPOffload
HKR,,*PMNSOffload
HKR,,*SelectiveSuspend
HKR,,*SSIdleTimeout
HKR,,*EEE
HKR,,EEE
HKR,,*HeaderDataSplit
HKR,,*IPSecOffloadV2
HKR,,*IdleRestriction
HKR,,AutoCrossoverDet
HKR,,S5WakeOnLan
HKR,,S5ARPOffload
HKR,,WolShutdownLinkSpeed
HKR,,AutoDisableGigabit
HKR,,AutoLinkDownPcieMacOff
HKR,,EnableGreenEthernet
HKR,,AdvancedEEE
HKR,,GigaLite
HKR,,WakeOnLinkUp
HKR,,WolCap
HKR,,PowerSavingMode
HKR,,EEEMaxSupportSpeed

;
; Localized strings
;
[Strings]
Provider                 = "Realtek"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
RSS                      = "Receive Side Scaling"
PriorityEnabled          = "Priority Enabled"
VLANEnabled              = "VLAN Enabled"
10MbFirst                = "10 Mbps First"
100MbFirst               = "100 Mbps First"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy-Efficient Ethernet"
NumRssQueues             = "Maximum Number of RSS Queues"
1Queue                   = "1 Queue"
2Queue                   = "2 Queues"
4Queue                   = "4 Queues"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Arabic_UAX
[Strings.3801]
Provider                 = "Realtek"
AutoDetect               = "التفاوض التلقائي"
SpeedDuplex              = "السرعة والازدواج"
10Mb-Half-Duplex         = "نصف المزدوج 10 ميجا بايت في الثانية"
10Mb-Full-Duplex         = "كامل الازدواج 10 ميجا بايت في الثانية"
100Mb-Half-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية"
100Mb-Full-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية"
1000Mb-Full-Duplex       = "كامل الازدواج 1000 ميجا بايت في الثانية"
2.5Gb-Full-Duplex        = "كامل الازدواج 2500 ميجا بايت في الثانية"
NetworkAddress           = "عنوان الشبكة"
IPChksumOffv4            = "تحميل المجموع الاختباري IPv4"
TCPChksumOffv4           = "تحميل المجموع الاختباري IPv4) TCP)"
UDPChksumOffv4           = "تحميل المجموع الاختباري IPv4) UDP)"
TCPChksumOffv6           = "تحميل المجموع الاختباري IPv6) TCP)"
UDPChksumOffv6           = "تحميل المجموع الاختباري IPv6) UDP)"
Enabled                  = "قيد التمكين"
Disabled                 = "قيد التعطيل"
TxEnabled                = "Tx قيد التمكين"
RxEnabled                = "Rx قيد التمكين"
RxTxEnabled              = "Rx & Tx قيد التمكين"
LSOv2v4                  = "تحميل الإرسال الكبير IPv4) v2)"
LSOv2v6                  = "تحميل الإرسال الكبير IPv6) v2)"
FlowControl              = "التحكم بالانسياب"
PriorityVLAN             = "الأولوية وVLAN"
PriorityVLANDisabled     = "الأولوية وVLAN قيد التعطيل"
PriorityVLANEnabled      = "الأولوية وVLAN قيد التمكين"
InterruptModeration      = "قطع التوسط"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "استقبال المخزنات المؤقتة"
TransmitBuffers          = "نقل المخزنات المؤقتة"
JumboFrame               = "الإطار الضخم"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "إغلاق معيار Wake-On-Lan"
RSS                      = "استلام تحديد مقياس الجانب"
PriorityEnabled          = "الأولوية قيد التمكين"
VLANEnabled              = "VLAN قيد التمكين"
10MbFirst                = "10 ميجا بايت في الثانية أولا"
100MbFirst               = "100 ميجا بايت في الثانية أولا"
WolShutdownLinkSpeed     = "رابط السرعة للإغلاق وWOL"
NotSpeedDown             = "عدم تخفيض السرعة"
GreenEthernet            = "إيثرنت أخضر"
WakeOnPtn                = "التنبيه عند مطابقة النقش"
WakeOnMagPkt             = "لتنبيه عند الحزمة السحرية"
ARPOffload               = "ARP توزيع نقل بيانات "
NsOffload                = " توزيع نقل بيانات NS"
EEE                      = " تقنية إيثرنت لحفظ الطاقة "
NumRssQueues             = "RSS لعدد الأقصى لقوائم انتظار "
1Queue                   = "قائمة انتظار واحدة"
2Queue                   = "قائمتا انتظار"
4Queue                   = " 4 قوائم انتظار"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Bulgarian
[Strings.0402]
Provider                 = "Realtek"
AutoDetect               = "Автоматични преговори"
SpeedDuplex              = "Скорост и дуплекс"
10Mb-Half-Duplex         = "10 Mbps полудуплекс"
10Mb-Full-Duplex         = "10 Mbps пълен дуплекс"
100Mb-Half-Duplex        = "100 Mbps полудуплекс"
100Mb-Full-Duplex        = "100 Mbps пълен дуплекс"
1000Mb-Full-Duplex       = "1,0 Gbps пълен дуплекс"
2.5Gb-Full-Duplex        = "2,5 Gbps пълен дуплекс"
NetworkAddress           = "Мрежов адрес"
IPChksumOffv4            = "Контролна сума IPv4 при разтоварване"
TCPChksumOffv4           = "Контролна сума TCP при разтоварване (IPv4)"
UDPChksumOffv4           = "Контролна сума UDP при разтоварване (IPv4)"
TCPChksumOffv6           = "Контролна сума TCP при разтоварване (IPv6)"
UDPChksumOffv6           = "Контролна сума UDP при разтоварване (IPv6)"
Enabled                  = "Разрешено"
Disabled                 = "Забранено"
TxEnabled                = "Tx разрешен"
RxEnabled                = "Rx разрешен"
RxTxEnabled              = "Rx & Tx Разрешено"
LSOv2v4                  = "Голямо разтоварване на изпращане в2 (IPv4)"
LSOv2v6                  = "Голямо разтоварване на изпращане в2 (IPv6)"
FlowControl              = "Управление на потока"
PriorityVLAN             = "Приоритет и VLAN"
PriorityVLANDisabled     = "Приоритет и VLAN забранени"
PriorityVLANEnabled      = "Приоритет и VLAN разрешени"
InterruptModeration      = "Прекъсване на наблюдаване"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Буфери при получаване"
TransmitBuffers          = "Буфери при прехвърляне"
JumboFrame               = "Jumbo рамка"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Изключване на събуждане при LAN"
RSS                      = "Получаване на мащабиране на страните"
PriorityEnabled          = "Разрешен приоритет"
VLANEnabled              = "VLAN разрешена"
10MbFirst                = "10 Mbps първо"
100MbFirst               = "100 Mbps първо"
WolShutdownLinkSpeed     = "WOL & скорост на връзката при изключване"
NotSpeedDown             = "Няма намаляване на скоростта"
GreenEthernet            = "Зелена Ethernet мрежа"
WakeOnPtn                = "Събуждане при съвпадение на модел"
WakeOnMagPkt             = "Събуждане при Magic Packet"
ARPOffload               = "ARP офлоуд"
NsOffload                = "NS офлоуд"
EEE                      = "Енергийно ефективен Етернет"
NumRssQueues             = "Максимален брой на RSS редица"
1Queue                   = "1 редица"
2Queue                   = "2 редици"
4Queue                   = "4 редици"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Chinese_Taiwan
[Strings.0404]
Provider                 = "Realtek"
AutoDetect               = "自動偵測"
SpeedDuplex              = "連線速度與雙工模式"
10Mb-Half-Duplex         = "10 Mbps 半雙工"
10Mb-Full-Duplex         = "10 Mbps 全雙工"
100Mb-Half-Duplex        = "100 Mbps 半雙工"
100Mb-Full-Duplex        = "100 Mbps 全雙工"
1000Mb-Full-Duplex       = "1.0 Gbps 全雙工"
2.5Gb-Full-Duplex        = "2.5 Gbps 全雙工"
NetworkAddress           = "網路卡位址"
IPChksumOffv4            = "IPv4 檢查總和值卸載"
TCPChksumOffv4           = "TCP 檢查總和卸載 (IPv4)"
UDPChksumOffv4           = "UDP 檢查總和卸載 (IPv4)"
TCPChksumOffv6           = "TCP 檢查總和卸載 (IPv6)"
UDPChksumOffv6           = "UDP 檢查總和卸載 (IPv6)"
Enabled                  = "開啟"
Disabled                 = "關閉"
TxEnabled                = "Tx 開啟"
RxEnabled                = "Rx 開啟"
RxTxEnabled              = "Rx & Tx 開啟"
LSOv2v4                  = "大量傳送卸載 v2 (IPv4)"
LSOv2v6                  = "大量傳送卸載 v2 (IPv6)"
FlowControl              = "流量控制"
PriorityVLAN             = "優先權 & VLAN"
PriorityVLANDisabled     = "優先權 & VLAN 關閉"
PriorityVLANEnabled      = "優先權 & VLAN 開啟"
InterruptModeration      = "中斷調整合適化"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "接收緩衝區"
TransmitBuffers          = "傳送緩衝區"
JumboFrame               = "巨大訊框"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "關機網路喚醒"
RSS                      = "接收端調整"
PriorityEnabled          = "優先權開啟"
VLANEnabled              = "VLAN 開啟"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL & 關機連線速度"
NotSpeedDown             = "不降速"
GreenEthernet            = "環保節能"
WakeOnPtn                = "樣式比對喚醒"
WakeOnMagPkt             = "魔術封包喚醒"
ARPOffload               = "ARP 卸載"
NsOffload                = "NS 卸載"
EEE                      = "節能乙太網路"
NumRssQueues             = "接收端調整最大佇列"
1Queue                   = "1個佇列"
2Queue                   = "2個佇列"
4Queue                   = "4個佇列"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Chinese (PRC)
[Strings.0804]
Provider                 = "Realtek"
AutoDetect               = "自动侦测"
SpeedDuplex              = "连接速度和双工模式"
10Mb-Half-Duplex         = "10 Mbps 半双工"
10Mb-Full-Duplex         = "10 Mbps 全双工"
100Mb-Half-Duplex        = "100 Mbps 半双工"
100Mb-Full-Duplex        = "100 Mbps 全双工"
1000Mb-Full-Duplex       = "1.0 Gbps 全双工"
2.5Gb-Full-Duplex        = "2.5 Gbps 全双工"
NetworkAddress           = "网络地址"
IPChksumOffv4            = "IPv4 硬件校验和"
TCPChksumOffv4           = "TCP 硬件校验和 (IPv4)"
UDPChksumOffv4           = "UDP 硬件校验和 (IPv4)"
TCPChksumOffv6           = "TCP 硬件校验和 (IPv6)"
UDPChksumOffv6           = "UDP 硬件校验和 (IPv6)"
Enabled                  = "开启"
Disabled                 = "关闭"
TxEnabled                = "Tx 开启"
RxEnabled                = "Rx 开启"
RxTxEnabled              = "Rx & Tx 开启"
LSOv2v4                  = "大量传送减负 v2 (IPv4)"
LSOv2v6                  = "大量传送减负 v2 (IPv6)"
FlowControl              = "流控制"
PriorityVLAN             = "优先级和VLAN"
PriorityVLANDisabled     = "优先级和VLAN 关闭"
PriorityVLANEnabled      = "优先级和VLAN 开启"
InterruptModeration      = "中断调整"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "接收缓冲区"
TransmitBuffers          = "传送缓冲区"
JumboFrame               = "巨型帧"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "关机 网络唤醒"
RSS                      = "接收端调整"
PriorityEnabled          = "优先级开启"
VLANEnabled              = "VLAN 开启"
10MbFirst                = "10 Mbps 优先"
100MbFirst               = "100 Mbps 优先"
WolShutdownLinkSpeed     = "网络唤醒和关机连接速度"
NotSpeedDown             = "不降速"
GreenEthernet            = "环保节能"
WakeOnPtn                = "样式比对唤醒"
WakeOnMagPkt             = "魔术封包唤醒"
ARPOffload               = "ARP 减负"
NsOffload                = "NS 减负"
EEE                      = "节能乙太网路"
NumRssQueues             = "接收端调整最大伫列"
1Queue                   = "1个伫列"
2Queue                   = "2个伫列"
4Queue                   = "4个伫列"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Croatian
[Strings.041a]
Provider                 = "Realtek"
AutoDetect               = "Automatsko prilagođivanje"
SpeedDuplex              = "Brzina i dupleks"
10Mb-Half-Duplex         = "10 Mb/s poludupleks"
10Mb-Full-Duplex         = "10 Mb/s puni dupleks"
100Mb-Half-Duplex        = "100 Mb/s poludupleks"
100Mb-Full-Duplex        = "100 Mb/s puni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s puni dupleks"
2.5Gb-Full-Duplex        = "2.5 Gb/s puni dupleks"
NetworkAddress           = "Mrežna adresa"
IPChksumOffv4            = "IPv4 kontrolni zbroj bez opterećenja"
TCPChksumOffv4           = "TCP kontrolni zbroj na periferiju (IPv4)"
UDPChksumOffv4           = "UDP kontrolni zbroj na periferiju (IPv4)"
TCPChksumOffv6           = "TCP kontrolni zbroj na periferiju (IPv6)"
UDPChksumOffv6           = "UDP kontrolni zbroj na periferiju (IPv6)"
Enabled                  = "Omogućeno"
Disabled                 = "Onemogućeno"
TxEnabled                = "Tx omogućeno"
RxEnabled                = "Rx omogućeno"
RxTxEnabled              = "Rx & Tx omogućeno"
LSOv2v4                  = "Slanje velikog na periferiju v2 (IPv4)"
LSOv2v6                  = "Slanje velikog na periferiju v2 (IPv6)"
FlowControl              = "Kontrola protoka"
PriorityVLAN             = "Prioritet i VLAN"
PriorityVLANDisabled     = "Prioritet i VLAN onemogućen"
PriorityVLANEnabled      = "Prioritet i VLAN omogućeni"
InterruptModeration      = "Moderacija prekida"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Spremnici prijema"
TransmitBuffers          = "Spremnici prijenosa"
JumboFrame               = "Jumbo okvir"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Isključivanje funkcije Probudi se na mreži nakon isključivanja"
RSS                      = "Smanjivanje na strani prijema"
PriorityEnabled          = "Prioritet omogućen"
VLANEnabled              = "VLAN omogućen"
10MbFirst                = "Prvo 10 Mb/s"
100MbFirst               = "Prvo 100 Mb/s"
WolShutdownLinkSpeed     = "Brzina veze za WOL i isključivanje"
NotSpeedDown             = "Nema smanjivanja brzine"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Odgovarajući uzorak izlaska iz stanja mirovanja"
WakeOnMagPkt             = "Čarobni paket izlaska iz stanja mirovanja"
ARPOffload               = "ARP rasterećenje"
NsOffload                = "NS rasterećenje"
EEE                      = "Energetski učinkovit Ethernet"
NumRssQueues             = "Maksimalni broj RSS redova čekanja"
1Queue                   = "1 red čekanja"
2Queue                   = "2 reda čekanja"
4Queue                   = "4 reda čekanja"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; CZ
[Strings.0405]
Provider                 = "Realtek"
AutoDetect               = "Automatické nastavení režimu provozu"
SpeedDuplex              = "Rychlost a přenosový režim"
10Mb-Half-Duplex         = "Poloduplexní 10 Mbps"
10Mb-Full-Duplex         = "Plně duplexní 10 Mbps"
100Mb-Half-Duplex        = "Poloduplexní 100 Mbps"
100Mb-Full-Duplex        = "Plně duplexní 100 Mbps"
1000Mb-Full-Duplex       = "Plně duplexní 1,0 Gbps"
2.5Gb-Full-Duplex        = "Plně duplexní 2,5 Gbps"
NetworkAddress           = "Síťová adresa"
IPChksumOffv4            = "Výpočet kontrolních součtů protokolu IPv4"
TCPChksumOffv4           = "Výpočet kontrolních součtů protokolu TCP (IPv4)"
UDPChksumOffv4           = "Výpočet kontrolních součtů protokolu UDP (IPv4)"
TCPChksumOffv6           = "Výpočet kontrolních součtů protokolu TCP (IPv6)"
UDPChksumOffv6           = "Výpočet kontrolních součtů protokolu UDP (IPv6)"
Enabled                  = "Povoleno"
Disabled                 = "Zakázáno"
TxEnabled                = "Odesílání povoleno"
RxEnabled                = "Příjem povolen"
RxTxEnabled              = "Příjem a odesílání povoleno"
LSOv2v4                  = "Zpracování velkých segmentů LSO v2 (IPv4)"
LSOv2v6                  = "Zpracování velkých segmentů LSO v2 (IPv6)"
FlowControl              = "Řízení toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN zakázána"
PriorityVLANEnabled      = "Priorita a VLAN povolena"
InterruptModeration      = "Tlumení přerušení"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Zásobníky příjmu"
TransmitBuffers          = "Zásobníky odesílání"
JumboFrame               = "Jumbo rámec"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
RSS                      = "Škálování na straně příjmu"
PriorityEnabled          = "Priorita povolena"
VLANEnabled              = "VLAN povolena"
10MbFirst                = "Nejdříve 10 Mbps"
100MbFirst               = "Nejdříve 100 Mbps"
WolShutdownLinkSpeed     = "Rychlost linky pro WOL a vypnutí"
NotSpeedDown             = "Bez zpomalení"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Probuzení porovnávacím vzorkem"
WakeOnMagPkt             = "Probuzení paketem Magic"
ARPOffload               = "Snižování zatížení ARP"
NsOffload                = "Snižování zatížení NS"
EEE                      = "Úsporná síť Ethernet"
NumRssQueues             = "Maximální počet front RSS"
1Queue                   = "1 fronta"
2Queue                   = "2 fronty"
4Queue                   = "4 fronty"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Danish
[Strings.0406]
Provider                 = "Realtek"
AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighed og duplex"
10Mb-Half-Duplex         = "10 Mbps halv duplex"
10Mb-Full-Duplex         = "10 Mbps fuld duplex"
100Mb-Half-Duplex        = "100 Mbps halv duplex"
100Mb-Full-Duplex        = "100 Mbps fuld duplex"
1000Mb-Full-Duplex       = "1.0 Gbps fuld duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps fuld duplex"
NetworkAddress           = "Netværksadresse"
IPChksumOffv4            = "Aflastning af IPv4 kontrolsum"
TCPChksumOffv4           = "Aflastning af TCP kontrolsum (IPv4)"
UDPChksumOffv4           = "Aflastning af UDP kontrolsum (IPv4)"
TCPChksumOffv6           = "Aflastning af TCP kontrolsum (IPv6)"
UDPChksumOffv6           = "Aflastning af UDP kontrolsum (IPv6)"
Enabled                  = "Aktiveret"
Disabled                 = "Deaktiveret"
TxEnabled                = "Tx aktiveret"
RxEnabled                = "Rx aktiveret"
RxTxEnabled              = "Rx og Tx aktiveret"
LSOv2v4                  = "Aflastning af stor forsendelse v2 (IPv4)"
LSOv2v6                  = "Aflastning af stor forsendelse v2 (IPv6)"
FlowControl              = "Flow-kontrol"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktiveret"
PriorityVLANEnabled      = "Prioritet og VLAN aktiveret"
InterruptModeration      = "Interruptindstilling"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Modtagelsesbuffer"
TransmitBuffers          = "Afsendelsesbuffere"
JumboFrame               = "Jumboramme"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Nedluk Wake-On-Lan"
RSS                      = "Skalering, modtagelsesside"
PriorityEnabled          = "Prioritet aktiveret"
VLANEnabled              = "VLAN aktiveret"
10MbFirst                = "10 Mbps først"
100MbFirst               = "100 Mbps først"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Grøn Ethernet"
WakeOnPtn                = "Vågn op ved mønstergenkendelse"
WakeOnMagPkt             = "Vågn op ved Magisk pakke"
ARPOffload               = "ARP-aflastning"
NsOffload                = "NS-aflastning"
EEE                      = "Energibesparende Ethernet"
NumRssQueues             = "Maksimal antal RSS-køer"
1Queue                   = "1 kø"
2Queue                   = "2 køer"
4Queue                   = "4 køer"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Dutch
[Strings.0413]
Provider                 = "Realtek"
AutoDetect               = "Automatisch onderhandelen"
SpeedDuplex              = "Snelheid & duplex"
10Mb-Half-Duplex         = "10 Mbps Half duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Half duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Netwerkadres"
IPChksumOffv4            = "IPv4-checksum-offload"
TCPChksumOffv4           = "TCP-checksum-offload (IPv4)"
UDPChksumOffv4           = "UDP-checksum-offload (IPv4)"
TCPChksumOffv6           = "TCP-checksum-offload (IPv6)"
UDPChksumOffv6           = "UDP-checksum-offload (IPv6)"
Enabled                  = "Ingeschakeld"
Disabled                 = "Uitgeschakeld"
TxEnabled                = "Tx ingeschakeld"
RxEnabled                = "Rx ingeschakeld"
RxTxEnabled              = "Rx & Tx ingeschakeld"
LSOv2v4                  = "Grote verzendings-Offload v2 (IPv4)"
LSOv2v6                  = "Grote verzendings-Offload v2 (IPv6)"
FlowControl              = "Datatransportbesturing"
PriorityVLAN             = "Prioriteit & VLAN"
PriorityVLANDisabled     = "Prioriteit & VLAN uitgeschakeld"
PriorityVLANEnabled      = "Prioriteit & VLAN ingeschakeld"
InterruptModeration      = "Interrupt-controle"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Buffers ontvangst"
TransmitBuffers          = "Buffers verzending"
JumboFrame               = "Jumbo frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-On-LAN uitschakelen"
RSS                      = "Schaling ontvangstzijde"
PriorityEnabled          = "Prioriteit ingeschakeld"
VLANEnabled              = "VLAN ingeschakeld"
10MbFirst                = "10 Mbps eerst"
100MbFirst               = "100 Mbps eerst"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Groen Ethernet"
WakeOnPtn                = "Ontwaken bij overeenkomend patroon"
WakeOnMagPkt             = "Ontwaken door Magic Packet"
ARPOffload               = "ARP-ontlading"
NsOffload                = "NS-ontlading"
EEE                      = "Energie-efficiënt Ethernet"
NumRssQueues             = "Maximaal aantal RSS-wachtrijen"
1Queue                   = "1 wachtrij"
2Queue                   = "2 wachtrijen"
4Queue                   = "4 wachtrijen"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Finnish
[Strings.040B]
Provider                 = "Realtek"
AutoDetect               = "Automaattinen neuvottelu"
SpeedDuplex              = "Nopeus & Duplex"
10Mb-Half-Duplex         = "10 Mbps puolikas Duplex"
10Mb-Full-Duplex         = "10 Mbps täysi Duplex"
100Mb-Half-Duplex        = "100 Mbps puolikas Duplex"
100Mb-Full-Duplex        = "100 Mbps täysi Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps täysi Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps täysi Duplex"
NetworkAddress           = "Verkon osoite"
IPChksumOffv4            = "IPv4 Pura tarkistussumma"
TCPChksumOffv4           = "TCP Pura tarkistussumma (IPv4)"
UDPChksumOffv4           = "UDP Pura tarkistussumma (IPv4)"
TCPChksumOffv6           = "TCP Pura tarkistussumma (IPv6)"
UDPChksumOffv6           = "UDP Pura tarkistussumma (IPv6)"
Enabled                  = "Käytössä"
Disabled                 = "Poistettu käytöstä"
TxEnabled                = "Tx Käytössä"
RxEnabled                = "Rx Käytössä"
RxTxEnabled              = "Rx & Tx Käytössä"
LSOv2v4                  = "Pura isot lähetykset v2 (IPv4)"
LSOv2v6                  = "Pura isot lähetykset v2 (IPv6)"
FlowControl              = "Datavuon ohjaus"
PriorityVLAN             = "Etusija & VLAN"
PriorityVLANDisabled     = "Etusija & VLAN poistettu käytöstä"
PriorityVLANEnabled      = "Etusija & VLAN käytössä"
InterruptModeration      = "Keskeytyksen hidastaminen"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Vastaanota puskureita"
TransmitBuffers          = "Siirrä puskureita"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Sammuta herätystoiminto Lanin kautta"
RSS                      = "RSS-verkkosyötemuodot"
PriorityEnabled          = "Etusija käytössä"
VLANEnabled              = "VLAN käytössä"
10MbFirst                = "10 Mbps ensin"
100MbFirst               = "100 Mbps ensin"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Vihreä Ethernet"
WakeOnPtn                = "Herätys vastaavalla kuviolla"
WakeOnMagPkt             = "Herätys Magic Packet -sovelluksella"
ARPOffload               = "ARP-purkaminen"
NsOffload                = "NS-purkaminen"
EEE                      = "Energiatehokas Ethernet"
NumRssQueues             = "RSS-jonojen maksimimäärä"
1Queue                   = "1 jono"
2Queue                   = "2 jonoa"
4Queue                   = "4 jonoa"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; French
[Strings.040c]
Provider                 = "Realtek"
AutoDetect               = "Négociation auto"
SpeedDuplex              = "Vitesse & Duplex"
10Mb-Half-Duplex         = "10 Mbps Semi-duplex"
10Mb-Full-Duplex         = "10 Mbps Duplex intégral"
100Mb-Half-Duplex        = "100 Mbps Semi-duplex"
100Mb-Full-Duplex        = "100 Mbps Duplex intégral"
1000Mb-Full-Duplex       = "1.0 Gbps Duplex intégral"
2.5Gb-Full-Duplex        = "2.5 Gbps Duplex intégral"
NetworkAddress           = "Adresse de réseau"
IPChksumOffv4            = "IPv4 Somme de contrôle hors charge"
TCPChksumOffv4           = "TCP Somme de contrôle hors charge (IPv4)"
UDPChksumOffv4           = "UDP Somme de contrôle hors charge (IPv4)"
TCPChksumOffv6           = "TCP Somme de contrôle hors charge (IPv6)"
UDPChksumOffv6           = "UDP Somme de contrôle hors charge (IPv6)"
Enabled                  = "Activé"
Disabled                 = "Désactivé"
TxEnabled                = "Tx activé"
RxEnabled                = "Rx activé"
RxTxEnabled              = "Rx & Tx activé"
LSOv2v4                  = "Grand envoi hors charge v2 (IPv4)"
LSOv2v6                  = "Grand envoi hors charge v2 (IPv6)"
FlowControl              = "Contrôle de flux"
PriorityVLAN             = "Priorité & VLAN"
PriorityVLANDisabled     = "Priorité & VLAN désactivé"
PriorityVLANEnabled      = "Priorité & VLAN activé"
InterruptModeration      = "Modération interruption"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Mémoires tampon de réception"
TransmitBuffers          = "Mémoires tampon de transmission"
JumboFrame               = "Cadre jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Arrêter Réveil par réseau"
RSS                      = "Echelle coté réception"
PriorityEnabled          = "Priorité activé"
VLANEnabled              = "VLAN activé"
10MbFirst                = "10 Mbps en premier"
100MbFirst               = "100 Mbps en premier"
WolShutdownLinkSpeed     = "WoL / Arrêt vitesse réseau"
NotSpeedDown             = "Pas vitesse ralentie"
GreenEthernet            = "Ethernet vert"
WakeOnPtn                = "Avertir lors de correspondance de motif"
WakeOnMagPkt             = "Réveil sur Magic Packet"
ARPOffload               = "Décharge ARP"
NsOffload                = "Décharge NS"
EEE                      = "Ethernet à économie d’énergie"
NumRssQueues             = "Nombre maximum de files d’attente RSS"
1Queue                   = "1 file d’attente"
2Queue                   = "2 files d’attente"
4Queue                   = "4 files d’attente"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; German
[Strings.0407]
Provider                 = "Realtek"
AutoDetect               = "Autom. Aushandlung"
SpeedDuplex              = "Geschwindigkeit & Duplex"
10Mb-Half-Duplex         = "10 Mbit/s Halbduplex"
10Mb-Full-Duplex         = "10 Mbit/s Vollduplex"
100Mb-Half-Duplex        = "100 Mbit/s Halbduplex"
100Mb-Full-Duplex        = "100 Mbit/s Vollduplex"
1000Mb-Full-Duplex       = "1.0 Gbit/s Vollduplex"
2.5Gb-Full-Duplex        = "2.5 Gbit/s Vollduplex"
NetworkAddress           = "Netzwerkadresse"
IPChksumOffv4            = "IPv4 Prüfsummenabladung"
TCPChksumOffv4           = "TCP Prüfsummenabladung (IPv4)"
UDPChksumOffv4           = "UDP Prüfsummenabladung (IPv4)"
TCPChksumOffv6           = "TCP Prüfsummenabladung (IPv6)"
UDPChksumOffv6           = "UDP-Prüfsummenabladung (IPv6)"
Enabled                  = "Aktiviert"
Disabled                 = "Deaktiviert"
TxEnabled                = "Tx aktiviert"
RxEnabled                = "Rx deaktiviert"
RxTxEnabled              = "Rx & Tx aktiviert"
LSOv2v4                  = "Abladung großer Übertragung V2 (IPv4)"
LSOv2v6                  = "Abladung großer Übertragung V2 (IPv6)"
FlowControl              = "Fließkontrolle"
PriorityVLAN             = "Priorität & VLAN"
PriorityVLANDisabled     = "Priorität & VLAN deaktiviert"
PriorityVLANEnabled      = "Priorität & VLAN aktiviert"
InterruptModeration      = "Interrupt-Moderation"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Puffer empfangen"
TransmitBuffers          = "Puffer übertragen"
JumboFrame               = "Jumbo-Rahmen"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-On-Lan herunterfahren"
RSS                      = "Seitenskalierung empfangen"
PriorityEnabled          = "Priorität aktiviert"
VLANEnabled              = "VLAN aktiviert"
10MbFirst                = "10 Mbit/s zuerst"
100MbFirst               = "100 Mbit/s zuerst"
WolShutdownLinkSpeed     = "WoL / Link-Geschwindigkeit reduzieren"
NotSpeedDown             = "Nicht verlangsamen"
GreenEthernet            = "Green-Ethernet"
WakeOnPtn                = "Bei Musterübereinstimmung aufwecken"
WakeOnMagPkt             = "Bei Magic Packet aufwecken"
ARPOffload               = "ARP-Abladen"
NsOffload                = "NS-Abladen"
EEE                      = "Energy-Efficient Ethernet (LAN-Energiesparen, EEE)"
NumRssQueues             = "Maximale RSS-Warteschlangenanzahl"
1Queue                   = "1 Warteschlange"
2Queue                   = "2 Warteschlangen"
4Queue                   = "4 Warteschlangen"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Greek
[Strings.0408]
Provider                 = "Realtek"
AutoDetect               = "Αυτόματη διαπραγμάτευση"
SpeedDuplex              = "Ταχύτητα & Αμφίδρομη"
10Mb-Half-Duplex         = "10Mbps/Ημι-αμφίδρομη"
10Mb-Full-Duplex         = "10Mbps/Πλήρως αμφίδρομη"
100Mb-Half-Duplex        = "100Mbps/Ημι-αμφίδρομη"
100Mb-Full-Duplex        = "100Mbps/Πλήρως αμφίδρομη"
1000Mb-Full-Duplex       = "1.0Gbps/Πλήρως αμφίδρομη"
2.5Gb-Full-Duplex        = "2.5Gbps/Πλήρως αμφίδρομη"
NetworkAddress           = "Διεύθυνση δικτύου"
IPChksumOffv4            = "Μείωση φόρτου αθροίσματος ελέγχου IPv4"
TCPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv4)"
UDPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
TCPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
UDPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv6)"
Enabled                  = "Ενεργοποιημένο"
Disabled                 = "Απενεργοποιημένο"
TxEnabled                = "Ενεργοποιημένο Tx"
RxEnabled                = "Ενεργοποιημένο Rx"
RxTxEnabled              = "Ενεργοποιημένο Rx & Tx"
LSOv2v4                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv4)"
LSOv2v6                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv6)"
FlowControl              = "Έλεγχος ροής"
PriorityVLAN             = "Προτεραιότητα & VLAN"
PriorityVLANDisabled     = "Απενεργοποίηση προτεραιότητας & VLAN"
PriorityVLANEnabled      = "Ενεργοποίηση προτεραιότητας & VLAN"
InterruptModeration      = "Διακοπή επόπτευσης"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Προσωρινοί χώροι παραλαβής"
TransmitBuffers          = "Προσωρινοί χώροι μετάδοσης"
JumboFrame               = "Πλαίσιο Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-on-LAN τερματισμού"
RSS                      = "Παραλαβή πλευρικής κλιμάκωσης"
PriorityEnabled          = "Ενεργοποίηση προτεραιότητας"
VLANEnabled              = "Ενεργοποίηση VLAN"
10MbFirst                = "Πρώτα 10 Mbps"
100MbFirst               = "Πρώτα 100 Mbps"
WolShutdownLinkSpeed     = "Ταχύτητα σύνδεσης τερματισμού & WOL"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Ενεργοποίηση με αντιστοίχιση μοτίβου"
WakeOnMagPkt             = "Ενεργοποίηση με Μαγικό πακέτο"
ARPOffload               = "Μείωση φόρτου ARP"
NsOffload                = "Μείωση φόρτου NS"
EEE                      = "Ethernet με αποτελεσματική χρήση ενέργειας"
NumRssQueues             = "Μέγιστος αριθμός ουρών RSS"
1Queue                   = "1 ουρά"
2Queue                   = "2 ουρές"
4Queue                   = "4 ουρές"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Hebrew
[Strings.040D]
Provider                 = "Realtek"
AutoDetect               = "משא ומתן אוטומטי"
SpeedDuplex              = "מהירות וכיווניות"
10Mb-Half-Duplex         = "10Mbps חד כיווני"
10Mb-Full-Duplex         = "10Mbps דו כיווני"
100Mb-Half-Duplex        = "100Mbps חד כיווני"
100Mb-Full-Duplex        = "100Mbps דו כיווני"
1000Mb-Full-Duplex       = "1000Mbps דו כיווני"
2.5Gb-Full-Duplex        = "2500Mbps דו כיווני"
NetworkAddress           = "כתובת רשת"
IPChksumOffv4            = "העברת סיכום ביקורת IPv4"
TCPChksumOffv4           = "העברת סיכום ביקורת IPv4) TCP)"
UDPChksumOffv4           = "העברת סיכום ביקורת IPv4) UDP)"
TCPChksumOffv6           = "העברת סיכום ביקורת IPv6) TCP)"
UDPChksumOffv6           = "העברת סיכום ביקורת IPv6) UDP)"
Enabled                  = "מאופשר"
Disabled                 = "מבוטל"
TxEnabled                = "שידור מאופשר"
RxEnabled                = "קליטה מאופשרת"
RxTxEnabled              = "שידור וקליטה מאופשרים"
LSOv2v4                  = "העברת שליחה גדולה IPv4) v2)"
LSOv2v6                  = "העברת שליחה גדולה IPv6) v2)"
FlowControl              = "בקרת זרימה"
PriorityVLAN             = "עדיפות ו-VLAN"
PriorityVLANDisabled     = "עדיפות ו-VLAN מבוטלות"
PriorityVLANEnabled      = "עדיפות ו-VLAN מאופשרות"
InterruptModeration      = "צמצום פסיקות"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "מאגרי קליטה"
TransmitBuffers          = "מאגרי שידור"
JumboFrame               = "מסגרת Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "כיבוי Wake-On-Lan"
RSS                      = "התאמת גודל בצד הקליטה"
PriorityEnabled          = "עדיפות מאופשרת"
VLANEnabled              = "VLAN מאופשר"
10MbFirst                = "10Mbps ראשון"
100MbFirst               = "100Mbps ראשון"
WolShutdownLinkSpeed     = "מהירות קישור כיבוי ו-WOL"
NotSpeedDown             = "ללא האטה"
GreenEthernet            = "ירוקEthernet"
WakeOnPtn                = "התאמת תבנית התעוררות"
WakeOnMagPkt             = "Magic Packet של התעוררות"
ARPOffload               = "העברת פרוטוקול ARP (פרוטוקול מציאת כתובת)"
NsOffload                = "העברת בקשת NS (בקשת זיהוי של שכן)"
EEE                      = "אתרנט חסכוני בחשמל"
NumRssQueues             = "המספר המרבי של תורי RSS (שינוי קנה מידה של הצד המקבל)"
1Queue                   = "תור אחד"
2Queue                   = "2 תורים"
4Queue                   = "4 תורים"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Hungarian
[Strings.040e]
Provider                 = "Realtek"
AutoDetect               = "Automatikus sebesség- és duplexitás-felismerés"
SpeedDuplex              = "Sebesség és duplex"
10Mb-Half-Duplex         = "10 Mbps Félduplex"
10Mb-Full-Duplex         = "10 Mbps Teljes duplex"
100Mb-Half-Duplex        = "100 Mbps Mbps Félduplex"
100Mb-Full-Duplex        = "100 Mbps Teljes duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Teljes duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Teljes duplex"
NetworkAddress           = "Hálózati cím"
IPChksumOffv4            = "IPv4 Ellenőrzőösszeg tehermentesítése"
TCPChksumOffv4           = "TCP Ellenőrzőösszeg tehermentesítése (IPv4)"
UDPChksumOffv4           = "UDP Ellenőrzőösszeg tehermentesítése (IPv4)"
TCPChksumOffv6           = "TCP Ellenőrzőösszeg tehermentesítése (IPv6)"
UDPChksumOffv6           = "UDP Ellenőrzőösszeg tehermentesítése (IPv6)"
Enabled                  = "Engedélyezve"
Disabled                 = "Letiltva"
TxEnabled                = "Tx Engedélyezve"
RxEnabled                = "Rx Engedélyezve"
RxTxEnabled              = "Rx és Tx Engedélyezve"
LSOv2v4                  = "Nagyobb küldemény tehermentesítése v2 (IPv4)"
LSOv2v6                  = "Nagyobb küldemény tehermentesítése v2 (IPv6)"
FlowControl              = "Áramlásszabályozás"
PriorityVLAN             = "Prioritás és VLAN"
PriorityVLANDisabled     = "Prioritás és VLAN letiltva"
PriorityVLANEnabled      = "Prioritás és VLAN engedélyezve"
InterruptModeration      = "Megszakítás visszatartása"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Vételi pufferek"
TransmitBuffers          = "Átviteli pufferek"
JumboFrame               = "Jumbo Frame (Óriás keret)"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Felélesztés leállítás után hálózaton keresztül"
RSS                      = "Vételoldali skálázás"
PriorityEnabled          = "Prioritás engedélyezve"
VLANEnabled              = "VLAN engedélyezve"
10MbFirst                = "10 Mbps/Első"
100MbFirst               = "100 Mbps/Első"
WolShutdownLinkSpeed     = "WOL és leállítás kapcsolati sebessége"
NotSpeedDown             = "Nincs lassítás"
GreenEthernet            = "Energiatakarékos Ethernet"
WakeOnPtn                = "Ébresztés egyező mintára"
WakeOnMagPkt             = "Ébresztés Magic Packetre"
ARPOffload               = "ARP lerakodás"
NsOffload                = "NS lerakodás"
EEE                      = "Energia-hatékony Ethernet"
NumRssQueues             = "RSS várakozási sorok maximális száma"
1Queue                   = "1 sor"
2Queue                   = "2 sor"
4Queue                   = "4 sor"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Italian
[Strings.0410]
Provider                 = "Realtek"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Velocità e duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Indirizzo di rete"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Abilitato"
Disabled                 = "Disabilitato"
TxEnabled                = "Tx Abilitata"
RxEnabled                = "Rx Abilitata"
RxTxEnabled              = "Rx & Tx Abilitata"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Controllo flusso"
PriorityVLAN             = "Priorità e VLAN"
PriorityVLANDisabled     = "Priorità e VLAN disabilitata"
PriorityVLANEnabled      = "Priorità e VLAN abilitata"
InterruptModeration      = "Interrupt Moderation"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Ricevi buffer"
TransmitBuffers          = "Trasmetti buffer"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
RSS                      = "Ricevi side scaling"
PriorityEnabled          = "Priorità abilitata"
VLANEnabled              = "VLAN abilitata"
10MbFirst                = "Prima 10 Mbps"
100MbFirst               = "Prima 100 Mbps"
WolShutdownLinkSpeed     = "WOL & Shutdown velocità collegamento"
NotSpeedDown             = "Non rallentamento"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Corrispondenza motivo per riattivazione"
WakeOnMagPkt             = "Magic Packet per riattivazione"
ARPOffload               = "Offload ARP"
NsOffload                = "Offload NS"
EEE                      = "Ethernet a risparmio energetico"
NumRssQueues             = "Numero massimo code RSS"
1Queue                   = "1 coda"
2Queue                   = "2 code"
4Queue                   = "4 code"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Japanese
[Strings.0411]
Provider                 = "Realtek"
AutoDetect               = "自動ネゴシエーション"
SpeedDuplex              = "速度とデュプレックス"
10Mb-Half-Duplex         = "10 Mbps ハーフデュプレックス"
10Mb-Full-Duplex         = "10 Mbps フルデュプレックス"
100Mb-Half-Duplex        = "100 Mbps ハーフデュプレックス"
100Mb-Full-Duplex        = "100 Mbps フルデュプレックス"
1000Mb-Full-Duplex       = "1.0 Gbps フルデュプレックス"
2.5Gb-Full-Duplex        = "2.5 Gbps フルデュプレックス"
NetworkAddress           = "ネットワークアドレス"
IPChksumOffv4            = "IPv4 チェックサムオフロード"
TCPChksumOffv4           = "TCP チェックサムオフロード (IPv4)"
UDPChksumOffv4           = "UDP チェックサムオフロード (IPv4)"
TCPChksumOffv6           = "TCP チェックサムオフロード (IPv6)"
UDPChksumOffv6           = "UDP チェックサムオフロード (IPv6)"
Enabled                  = "有効"
Disabled                 = "無効"
TxEnabled                = "Tx 有効"
RxEnabled                = "Rx 有効"
RxTxEnabled              = "受信と伝送有効"
LSOv2v4                  = "一括送信オフロード v2 (IPv4)"
LSOv2v6                  = "一括送信オフロード v2 (IPv6)"
FlowControl              = "フローコントロール"
PriorityVLAN             = "優先度およびVLAN"
PriorityVLANDisabled     = "優先度およびVLAN 無効"
PriorityVLANEnabled      = "優先度およびVLAN 有効"
InterruptModeration      = "割込みモデレーション"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "受信バッファ"
TransmitBuffers          = "伝送バッファ"
JumboFrame               = "ジャンボフレーム"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "LAN 上のウェークアップのシャットダウン"
RSS                      = "受信側スケーリング"
PriorityEnabled          = "優先度有効"
VLANEnabled              = "VLAN 有効"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL とシャットダウンリンク速度"
NotSpeedDown             = "速度低下ではない"
GreenEthernet            = "グリーンイーサネット"
WakeOnPtn                = "ウェイク・オン・パターン・マッチ"
WakeOnMagPkt             = "ウェイク・オン・マジック・パケット"
ARPOffload               = "ARP オフロード"
NsOffload                = "NS オフロード"
EEE                      = "省電力型イーサネット(EEE)"
NumRssQueues             = "RSSキューの最大数"
1Queue                   = "1キュー"
2Queue                   = "2キュー"
4Queue                   = "4キュー"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Korean
[Strings.0412]
Provider                 = "Realtek"
AutoDetect               = "자동 교섭"
SpeedDuplex              = "속도 및 이중"
10Mb-Half-Duplex         = "10 Mbps 반이중"
10Mb-Full-Duplex         = "10 Mbps 전이중"
100Mb-Half-Duplex        = "100 Mbps 반이중"
100Mb-Full-Duplex        = "100 Mbps 전이중"
1000Mb-Full-Duplex       = "1.0 Gbps 전이중"
2.5Gb-Full-Duplex        = "2.5 Gbps 전이중"
NetworkAddress           = "네트워크 주소"
IPChksumOffv4            = "IPv4 체크섬 오프로드"
TCPChksumOffv4           = "TCP 체크섬 오프로드(IPv4)"
UDPChksumOffv4           = "UDP 체크섬 오프로드(IPv4)"
TCPChksumOffv6           = "TCP 체크섬 오프로드(IPv6)"
UDPChksumOffv6           = "UDP 체크섬 오프로드(IPv6)"
Enabled                  = "사용"
Disabled                 = "사용 안 함"
TxEnabled                = "Tx 사용"
RxEnabled                = "Rx 사용"
RxTxEnabled              = "Rx/Tx 사용"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "흐름 제어"
PriorityVLAN             = "우선 순위 및 VLAN"
PriorityVLANDisabled     = "우선 순위 및 VLAN 사용 안 함"
PriorityVLANEnabled      = "우선 순위 및 VLAN 사용"
InterruptModeration      = "인터럽트 완화"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "수신 버퍼"
TransmitBuffers          = "송신 버퍼"
JumboFrame               = "점보 프레임"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "웨이크 온 랜 종료"
RSS                      = "수신측 조정"
PriorityEnabled          = "우선 순위 사용"
VLANEnabled              = "VLAN 사용"
10MbFirst                = "10 Mbps 먼저"
100MbFirst               = "100 Mbps 먼저"
WolShutdownLinkSpeed     = "WOL 및 종료 링크 속도"
NotSpeedDown             = "속도 저하 안 함"
GreenEthernet            = "절전형 이더넷"
WakeOnPtn                = "패턴 일치 웨이크 온"
WakeOnMagPkt             = "매직 패킷 웨이크 온"
ARPOffload               = "ARP 오프로드"
NsOffload                = "NS 오프로드"
EEE                      = "에너지 효율적인 이더넷"
NumRssQueues             = "RSS 대기행렬의 최대 수"
1Queue                   = "1개의 대기행렬"
2Queue                   = "2개의 대기행렬"
4Queue                   = "4개의 대기행렬"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Norwegian_Bokmal
[Strings.0414]
Provider                 = "Realtek"
AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighet og dupleks"
10Mb-Half-Duplex         = "10Mbps Halv dupleks"
10Mb-Full-Duplex         = "10Mbps Full dupleks"
100Mb-Half-Duplex        = "100Mbps Halv dupleks"
100Mb-Full-Duplex        = "100Mbps Full dupleks"
1000Mb-Full-Duplex       = "1.0Gbps Full dupleks"
2.5Gb-Full-Duplex        = "2.5Gbps Full dupleks"
NetworkAddress           = "Nettverksadresse"
IPChksumOffv4            = "IPv4 Sjekksum avlastning"
TCPChksumOffv4           = "TCP Sjekksum avlastning (IPv4)"
UDPChksumOffv4           = "UDP Sjekksum avlastning (IPv4)"
TCPChksumOffv6           = "TCP Sjekksum avlastning (Ipv6)"
UDPChksumOffv6           = "UDP Sjekksum avlastning (Ipv6)"
Enabled                  = "Aktivert"
Disabled                 = "Deaktivert"
TxEnabled                = "Tx aktivert"
RxEnabled                = "Rx aktivert"
RxTxEnabled              = "Rx og Tx aktivert"
LSOv2v4                  = "Stor sending avlastning v2 (IPv4)"
LSOv2v6                  = "Stor sending avlastning v2 (Ipv6)"
FlowControl              = "Flytkontroll"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktivert"
PriorityVLANEnabled      = "Prioritet og VLAN aktivert"
InterruptModeration      = "Avbruddsmoderering"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Mottaksbuffere"
TransmitBuffers          = "Sendebuffere"
JumboFrame               = "Jumbo-ramme"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Avslutningsaktivering på nettverk"
RSS                      = "Mottak sideskalering"
PriorityEnabled          = "Prioritet aktivert"
VLANEnabled              = "VLAN aktivert"
10MbFirst                = "10 Mbps Først"
100MbFirst               = "100 Mbps Først"
WolShutdownLinkSpeed     = "WOL og avslutningslinjehastighet"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Grønt Ethernet"
WakeOnPtn                = "Reaktiver når mønster samsvarer"
WakeOnMagPkt             = "Reaktivert etter magisk pakke"
ARPOffload               = "ARP-avlasting"
NsOffload                = "NS-avlasting"
EEE                      = "Energy-Efficient Ethernet"
NumRssQueues             = "Maksimalt antall RSS-køer"
1Queue                   = "1 kø"
2Queue                   = "2 køer"
4Queue                   = "4 køer"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Polish
[Strings.0415]
Provider                 = "Realtek"
AutoDetect               = "Automatyczne negocjacje"
SpeedDuplex              = "Szybkość i dupleks"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Adres sieciowy"
IPChksumOffv4            = "Suma kontrolna bez obciążenia IPv4"
TCPChksumOffv4           = "Suma kontrolna bez obciążenia TCP (IPv4)"
UDPChksumOffv4           = "Suma kontrolna bez obciążenia UDP (IPv4)"
TCPChksumOffv6           = "Suma kontrolna bez obciążenia TCP (IPv6)"
UDPChksumOffv6           = "Suma kontrolna bez obciążenia UDP (IPv6)"
Enabled                  = "Włączone"
Disabled                 = "Wyłączone"
TxEnabled                = "Włączone Tx"
RxEnabled                = "Włączone Rx"
RxTxEnabled              = "Włączone Rx i Tx"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Sterowanie przepływem"
PriorityVLAN             = "Priorytet i VLAN"
PriorityVLANDisabled     = "Wyłączony Priorytet i VLAN"
PriorityVLANEnabled      = "Włączony Priorytet i VLAN"
InterruptModeration      = "Moderacja przerwania"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Bufory odbioru"
TransmitBuffers          = "Bufory transmisji"
JumboFrame               = "Ramka Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Zamknięcie Wybudzanie przy uaktywnieniu sieci"
RSS                      = "Receive Side Scaling"
PriorityEnabled          = "Włączony priorytet"
VLANEnabled              = "Włączona sieć VLAN"
10MbFirst                = "Najpierw 10 Mbps"
100MbFirst               = "Najpierw 100 Mbps"
WolShutdownLinkSpeed     = "WOL i szybkość zamykania łącza"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Energooszczędny Ethernet"
WakeOnPtn                = "Dopasowanie do wzorca wybudzania"
WakeOnMagPkt             = "Pakiet wybudzania Magic Packet"
ARPOffload               = "Rozładowanie ARP"
NsOffload                = "Rozładowanie NS"
EEE                      = "Ethernet efektywny energetycznie"
NumRssQueues             = "Maksymalna liczba kolejek RSS"
1Queue                   = "1 kolejka"
2Queue                   = "2 kolejki"
4Queue                   = "4 kolejki"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Portuguese_Brazilian
[Strings.0416]
Provider                 = "Realtek"
AutoDetect               = "Auto Negociação"
SpeedDuplex              = "Velocidade & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Endereço de Rede"
IPChksumOffv4            = "IPv4 Descarga de Checksum"
TCPChksumOffv4           = "TCP Descarga de Checksum (IPv4)"
UDPChksumOffv4           = "UDP Descarga de Checksum (IPv4)"
TCPChksumOffv6           = "TCP Descarga de Checksum (IPv6)"
UDPChksumOffv6           = "UDP Descarga de Checksum (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx Activado"
RxEnabled                = "Rx Activado"
RxTxEnabled              = "Rx & Tx Activados"
LSOv2v4                  = "Descarga Large Send v2 (IPv4)"
LSOv2v6                  = "Descarga Large Send v2 (IPv6)"
FlowControl              = "Controlo de Fluxo"
PriorityVLAN             = "Prioridade & VLAN"
PriorityVLANDisabled     = "Prioridade & VLAN Desactivados"
PriorityVLANEnabled      = "Prioridade & VLAN Activados"
InterruptModeration      = "Moderação de Interrupção"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Receber Memórias Intermédias"
TransmitBuffers          = "Transmitir Memórias Intermédias"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Desligar Despertar Aquando de Lan"
RSS                      = "Receber Side Scaling"
PriorityEnabled          = "Prioridade Activada"
VLANEnabled              = "VLAN Activada"
10MbFirst                = "10 Mbps Primeiro"
100MbFirst               = "100 Mbps Primeiro"
WolShutdownLinkSpeed     = "WOL & Desligar Velocidade Ligação"
NotSpeedDown             = "Não reduzir velocidade"
GreenEthernet            = "Ethernet Verde"
WakeOnPtn                = "Combinação do padrão Wake on"
WakeOnMagPkt             = "Pacote Wake on Magic"
ARPOffload               = "Transferência ARP"
NsOffload                = "Transferência NS"
EEE                      = "Energia Eficiente Ethernet"
NumRssQueues             = "Número Máximo de Filas RSS"
1Queue                   = "1 Fila"
2Queue                   = "2 Filas"
4Queue                   = "4 Filas"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Portuguese_Standard
[Strings.0816]
Provider                 = "Realtek"
AutoDetect               = "Auto negociação"
SpeedDuplex              = "Velocidade e modo duplex"
10Mb-Half-Duplex         = "10 Mbps modo semi duplex"
10Mb-Full-Duplex         = "10 Mbps modo full-duplex"
100Mb-Half-Duplex        = "100 Mbps modo semi duplex"
100Mb-Full-Duplex        = "100 Mbps modo full-duplex"
1000Mb-Full-Duplex       = "1,0 Gbps modo full-duplex"
2.5Gb-Full-Duplex        = "2,5 Gbps modo full-duplex"
NetworkAddress           = "Endereço de rede"
IPChksumOffv4            = "Soma de verificação offload IPv4"
TCPChksumOffv4           = "Soma de verificação offload TCP (IPv4)"
UDPChksumOffv4           = "Soma de verificação offload UDP (IPv4)"
TCPChksumOffv6           = "Soma de verificação offload TCP (IPv6)"
UDPChksumOffv6           = "Soma de verificação offload UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Transmissão activada"
RxEnabled                = "Recepção activada"
RxTxEnabled              = "Recepção e transmissão activada"
LSOv2v4                  = "Envio grande de offload v2 (IPv4)"
LSOv2v6                  = "Envio grande de offload v2 (IPv6)"
FlowControl              = "Controlo do fluxo"
PriorityVLAN             = "Prioridade e VLAN"
PriorityVLANDisabled     = "Prioridade e VLAN desactivada"
PriorityVLANEnabled      = "Prioridade e VLAN activada"
InterruptModeration      = "Moderação de interrupção"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Memória de recepção"
TransmitBuffers          = "Memória de transmissão"
JumboFrame               = "Estrutura jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Encerrar Wake-On-Lan"
RSS                      = "Receive Side Scaling"
PriorityEnabled          = "Prioridade activada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps primeiro"
100MbFirst               = "100 Mbps primeiro"
WolShutdownLinkSpeed     = "WOL e encerrar velocidade de ligação"
NotSpeedDown             = "Não diminuir velocidade"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Reactivação por correspondência de padrões"
WakeOnMagPkt             = "Reactivação por Magic Packet"
ARPOffload               = "Descarga de ARP"
NsOffload                = "Descarga de NS"
EEE                      = "Ethernet de Consumo de Energia Eficiente"
NumRssQueues             = "Número máximo de filas RSS"
1Queue                   = "1 Fila"
2Queue                   = "2 Filas"
4Queue                   = "4 Filas"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Romanian
[Strings.0418]
Provider                 = "Realtek"
AutoDetect               = "Negociere automată"
SpeedDuplex              = "Viteză şi duplex"
10Mb-Half-Duplex         = "10 Mbps semiduplex"
10Mb-Full-Duplex         = "10 Mbps duplex"
100Mb-Half-Duplex        = "100 Mbps semiduplex"
100Mb-Full-Duplex        = "100 Mbps duplex"
1000Mb-Full-Duplex       = "1,0 Gbps duplex"
2.5Gb-Full-Duplex        = "2,5 Gbps duplex"
NetworkAddress           = "Adresă de reţea"
IPChksumOffv4            = "Preluare sarcină de verificare erori de transmisie IPv4"
TCPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie TCP (IPv4)"
UDPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie UDP(IPv4)"
TCPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie TCP(IPv6)"
UDPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie UDP (IPv6)"
Enabled                  = "Activat"
Disabled                 = "Dezactivat"
TxEnabled                = "Tx activat"
RxEnabled                = "Rx activat"
RxTxEnabled              = "Rx şi Tx activate"
LSOv2v4                  = "Preluare sarcină de trimitere pachete mari v2 (IPv4)"
LSOv2v6                  = "Preluare sarcină de trimitere pachete mari v2 (IPv6)"
FlowControl              = "Control debit"
PriorityVLAN             = "Prioritate şi VLAN"
PriorityVLANDisabled     = "Prioritate şi VLAN dezactivate"
PriorityVLANEnabled      = "Prioritate şi VLAN activate"
InterruptModeration      = "Moderare întrerupere"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Zone tampon de primire"
TransmitBuffers          = "Zone tampon de trimitere"
JumboFrame               = "Cadru jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Închidere Trezire prin LAN"
RSS                      = "Primire scalare laterală"
PriorityEnabled          = "Prioritate activată"
VLANEnabled              = "VLAN activată"
10MbFirst                = "10 Mbps iniţial"
100MbFirst               = "100 Mbps iniţial"
WolShutdownLinkSpeed     = "WOL şi dezactivare viteză legătură"
NotSpeedDown             = "Fără reducere viteză"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Activare la potrivire model"
WakeOnMagPkt             = "Potrivire la pachet magic"
ARPOffload               = "Reducere sarcină protocol rezolvare adresă"
NsOffload                = "Reducere sarcină solicitare vecin"
EEE                      = "Ethernet eficient energetic"
NumRssQueues             = "Număr maxim de cozi pentru scalare la primire"
1Queue                   = "1 coadă"
2Queue                   = "2 cozi"
4Queue                   = "4 cozi"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Russian
[Strings.0419]
Provider                 = "Realtek"
AutoDetect               = "Автосогласование"
SpeedDuplex              = "Скорость и дуплекс"
10Mb-Half-Duplex         = "10 Мбит/с полудуплекс"
10Mb-Full-Duplex         = "10 Мбит/с дуплекс"
100Mb-Half-Duplex        = "100 Мбит/с полудуплекс"
100Mb-Full-Duplex        = "100 Мбит/с дуплекс"
1000Mb-Full-Duplex       = "1 Гбит/с дуплекс"
2.5Gb-Full-Duplex        = "2.5 Гбит/с дуплекс"
NetworkAddress           = "Сетевой адрес"
IPChksumOffv4            = "Контрольная сумма разгрузки IPv4"
TCPChksumOffv4           = "Контрольная сумма разгрузки TCP (IPv4)"
UDPChksumOffv4           = "Контрольная сумма разгрузки UDP (IPv4)"
TCPChksumOffv6           = "Контрольная сумма разгрузки TCP (IPv6)"
UDPChksumOffv6           = "Контрольная сумма разгрузки UDP (IPv6)"
Enabled                  = "Вкл"
Disabled                 = "Выкл"
TxEnabled                = "Tx вкл"
RxEnabled                = "Rx вкл"
RxTxEnabled              = "Rx & Tx вкл"
LSOv2v4                  = "Разгрузка при большой отправке v2 (IPv4)"
LSOv2v6                  = "Разгрузка при большой отправке v2 (IPv6)"
FlowControl              = "Управление потоком"
PriorityVLAN             = "Приоритет & VLAN"
PriorityVLANDisabled     = "Приоритет & VLAN выкл"
PriorityVLANEnabled      = "Приоритет & VLAN вкл"
InterruptModeration      = "Модерация прерывания"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Буферы приема"
TransmitBuffers          = "Буферы передачи"
JumboFrame               = "Большой кадр"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Включение по локальной сети после отключения"
RSS                      = "Получение бокового масштабирования"
PriorityEnabled          = "Приоритет вкл"
VLANEnabled              = "VLAN вкл"
10MbFirst                = "Сначала 10 Mбит/с"
100MbFirst               = "Сначала 100 Mбит/с"
WolShutdownLinkSpeed     = "Скорость при включении по локальной сети после отключения"
NotSpeedDown             = "Не использовать автопонижение скорости"
GreenEthernet            = "Зеленый Ethernet"
WakeOnPtn                = "Включить при совпадении шаблона"
WakeOnMagPkt             = "Включить при срабатывании функции Magic Packet"
ARPOffload               = "Выгрузка протокола ARP"
NsOffload                = "Выгрузка протокола NS"
EEE                      = "Энергосберегающий Ethernet"
NumRssQueues             = "Максимальное число очередей RSS"
1Queue                   = "1 очередь"
2Queue                   = "2 очереди"
4Queue                   = "4 очереди"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Slovak
[Strings.041b]
Provider                 = "Realtek"
AutoDetect               = "Automatické vyjednávanie"
SpeedDuplex              = "Rýchlosť a duplexný režim"
10Mb-Half-Duplex         = "10 Mbps polovične duplexný"
10Mb-Full-Duplex         = "10 Mbps plne duplexný"
100Mb-Half-Duplex        = "100 Mbps polovične duplexný"
100Mb-Full-Duplex        = "100 Mbps plne duplexný"
1000Mb-Full-Duplex       = "1,0 Gbps plne duplexný"
2.5Gb-Full-Duplex        = "2,5 Gbps plne duplexný"
NetworkAddress           = "Sieťová adresa"
IPChksumOffv4            = "Kontrolný súčet zníženej záťaže IPv4"
TCPChksumOffv4           = "Kontrolný súčet zníženej záťaže TCP (IPv4)"
UDPChksumOffv4           = "Kontrolný súčet zníženej záťaže UDP (IPv4)"
TCPChksumOffv6           = "Kontrolný súčet zníženej záťaže TCP (IPv6)"
UDPChksumOffv6           = "Kontrolný súčet zníženej záťaže UDP (IPv6)"
Enabled                  = "Aktivovaný"
Disabled                 = "Deaktivovaný"
TxEnabled                = "Tx aktivovaný"
RxEnabled                = "Rx aktivovaný"
RxTxEnabled              = "Rx a Tx aktivované"
LSOv2v4                  = "Veľká odoslaná znížená záťaž v2 (IPv4)"
LSOv2v6                  = "Veľká odoslaná znížená záťaž v2 (IPv6)"
FlowControl              = "Ovládanie toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN sú deaktivované"
PriorityVLANEnabled      = "Priorita a VLAN sú aktivované"
InterruptModeration      = "Prerušiť moderovanie"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Medzipamäte pre príjem"
TransmitBuffers          = "Medzipamäte pre prenos"
JumboFrame               = "Jumbo rámček"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Vypnutie po pripojení k LAN"
RSS                      = "Prijať bočnú zmenu mierky"
PriorityEnabled          = "Priorita je aktivovaná"
VLANEnabled              = "VLAN je aktivovaná"
10MbFirst                = "Najprv 10 Mbps"
100MbFirst               = "Najprv 100 Mbps"
WolShutdownLinkSpeed     = "Rýchlosť WOL a vypnutia spojenia"
NotSpeedDown             = "Neznížiť rýchlosť"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Funkcia Wake on pattern match (Zapnúť funkciu Zhoda vzoru)"
WakeOnMagPkt             = "Nástroj Wake on Magic Packet (Zapnúť aplikáciu Kúzelný balík)"
ARPOffload               = "Nepriame zavádzanie ARP"
NsOffload                = "Nepriame zavádzanie NS"
EEE                      = "Energeticky účinný Ethernet"
NumRssQueues             = "Maximálny počet frontov RSS"
1Queue                   = "1 front "
2Queue                   = "2 fronty"
4Queue                   = "4 fronty"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Slovenian
[Strings.0424]
Provider                 = "Realtek"
AutoDetect               = "Samopogajanje"
SpeedDuplex              = "Hitrost in dupleks"
10Mb-Half-Duplex         = "10 Mb/s Polovični dupleks"
10Mb-Full-Duplex         = "10 Mb/s Polni dupleks"
100Mb-Half-Duplex        = "100 Mb/s Polovični dupleks"
100Mb-Full-Duplex        = "100 Mb/s Polni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s Polni dupleks"
2.5Gb-Full-Duplex        = "2.5 Gb/s Polni dupleks"
NetworkAddress           = "Omrežni naslov"
IPChksumOffv4            = "IPv4 Razbremenitev kontrolne vsote"
TCPChksumOffv4           = "TCP Razbremenitev kontrolne vsote (IPv4)"
UDPChksumOffv4           = "UDP Razbremenitev kontrolne vsote (IPv4)"
TCPChksumOffv6           = "TCP Razbremenitev kontrolne vsote (IPv6)"
UDPChksumOffv6           = "UDP Razbremenitev kontrolne vsote (IPv6)"
Enabled                  = "Omogočeno"
Disabled                 = "Onemogočeno"
TxEnabled                = "Tx Omogočeno"
RxEnabled                = "Rx Omogočeno"
RxTxEnabled              = "Rx in Tx omogočeno"
LSOv2v4                  = "Razbremenitev velikega prenosa v2 (IPv4)"
LSOv2v6                  = "Razbremenitev velikega prenosa v2 (IPv6)"
FlowControl              = "Kontrola pretoka"
PriorityVLAN             = "Prednost in VLAN"
PriorityVLANDisabled     = "Prednost in VLAN onemogočena"
PriorityVLANEnabled      = "Prednost in VLAN omogočena"
InterruptModeration      = "Prekinjena moderacija"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Prejmi medpomnilnike"
TransmitBuffers          = "Prenesi medpomnilnike"
JumboFrame               = "Jumbo okvir"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Zaustavitev Bujenje-na-Lan"
RSS                      = "Sprejmi stransko merilo"
PriorityEnabled          = "Prednost omogočena"
VLANEnabled              = "VLAN omogočen"
10MbFirst                = "10 Mb/s Najprej"
100MbFirst               = "100 Mb/s Najprej"
WolShutdownLinkSpeed     = "Hitrost zaustavitve povezave in WOL"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Zbudi ob enakem vzorcu"
WakeOnMagPkt             = "Zbudi ob paketu Magic"
ARPOffload               = "Prelaganje ARP"
NsOffload                = "Prelaganje NS"
EEE                      = "Energijsko učinkovit ethernet"
NumRssQueues             = "Največje število čakalnih vrst RSS"
1Queue                   = "1 čakalna vrsta"
2Queue                   = "2 čakalni vrsti"
4Queue                   = "4 čakalne vrste"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Spanish
[Strings.040A]
Provider                 = "Realtek"
AutoDetect               = "Negociación automática"
SpeedDuplex              = "Velocidad y Dúplex"
10Mb-Half-Duplex         = "10 Mbps Half Dúplex"
10Mb-Full-Duplex         = "10 Mbps Full Dúplex"
100Mb-Half-Duplex        = "100 Mbps Half Dúplex"
100Mb-Full-Duplex        = "100 Mbps Full Dúplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Dúplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Dúplex"
NetworkAddress           = "Dirección de red"
IPChksumOffv4            = "Descarga de suma de comprobación IPv4"
TCPChksumOffv4           = "Descarga de suma de comprobación TCP (IPv4)"
UDPChksumOffv4           = "Descarga de suma de comprobación UDP (IPv4)"
TCPChksumOffv6           = "Descarga de suma de comprobación TCP (IPv6)"
UDPChksumOffv6           = "Descarga de suma de comprobación UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx activada"
RxEnabled                = "Rx activada"
RxTxEnabled              = "Rx y Tx activado"
LSOv2v4                  = "Descarga de gran envío v2 (IPv4)"
LSOv2v6                  = "Descarga de gran envío v2 (IPv6)"
FlowControl              = "Control de flujo"
PriorityVLAN             = "Prioridad y VLAN"
PriorityVLANDisabled     = "Prioridad y VLAN desactivada"
PriorityVLANEnabled      = "Prioridad y VLAN activada"
InterruptModeration      = "Moderación de interrupción"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Búferes de recepción"
TransmitBuffers          = "Búferes de transmisión"
JumboFrame               = "Trama Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Activación con LAN de apagado"
RSS                      = "Escalado lateral de recepción"
PriorityEnabled          = "Prioridad habilitada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps Primero"
100MbFirst               = "100 Mbps Primero"
WolShutdownLinkSpeed     = "Velocidad de enlace WOL y Apagado"
NotSpeedDown             = "Sin reducción de velocidad"
GreenEthernet            = "Ethernet ecológico"
WakeOnPtn                = "Reactivar en coincidencia de patrones"
WakeOnMagPkt             = "Reactivar en Magic Packet"
ARPOffload               = "Descarga ARP"
NsOffload                = "Descarga NS"
EEE                      = "Ethernet de consumo eficiente de energía"
NumRssQueues             = "Número máximo de colas de RSS"
1Queue                   = "1 Cola"
2Queue                   = "2 Colas"
4Queue                   = "4 Colas"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Swedish
[Strings.041D]
Provider                 = "Realtek"
AutoDetect               = "Automatisk förhandling"
SpeedDuplex              = "Hastighet & duplex"
10Mb-Half-Duplex         = "10 Mbps Halv duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Halv duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Nätverksadress"
IPChksumOffv4            = "IPv4 Avbelasta kontrollsumma"
TCPChksumOffv4           = "TCP avbelasta kontrollsumma (IPv4)"
UDPChksumOffv4           = "UDP avbelasta kontrollsumma (IPv4)"
TCPChksumOffv6           = "TCP avbelasta kontrollsumma (IPv6)"
UDPChksumOffv6           = "UDP avbelasta kontrollsumma (IPv6)"
Enabled                  = "Aktiverad"
Disabled                 = "Inaktiverad"
TxEnabled                = "Tx aktiverad"
RxEnabled                = "Rx aktiverad"
RxTxEnabled              = "Rx & Tx aktiverad"
LSOv2v4                  = "Avbelastning för stor överföring v2 (IPv4)"
LSOv2v6                  = "Avbelastning för stor överföring v2 (IPv6)"
FlowControl              = "Flödeskontroll"
PriorityVLAN             = "Prioritet & VLAN"
PriorityVLANDisabled     = "Prioritet & VLAN inaktiverad"
PriorityVLANEnabled      = "Prioritet & VLAN aktiverad"
InterruptModeration      = "Gruppering av avbrott"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Mottagningsbuffertar"
TransmitBuffers          = "Överföringsbuffertar"
JumboFrame               = "Jumboram"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Avsluta Wake-on-LAN"
RSS                      = "Ta emot sidskalning"
PriorityEnabled          = "Prioritet aktiverad"
VLANEnabled              = "VLAN aktiverat"
10MbFirst                = "10 Mbps först"
100MbFirst               = "100 Mbps först"
WolShutdownLinkSpeed     = "WOL och länkhastighet vid avslutning"
NotSpeedDown             = "Not Speed Down"
GreenEthernet            = "Grönt Ethernet"
WakeOnPtn                = "Vakna vid matchat mönster"
WakeOnMagPkt             = "Vakna vid Magiskt paket"
ARPOffload               = "ARP-avlastning"
NsOffload                = "NS-avlastning"
EEE                      = "Energieffektivt Ethernet"
NumRssQueues             = "Maximalt antal RSS-köer"
1Queue                   = "1 Kö"
2Queue                   = "2 Köer"
4Queue                   = "4 Köer"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Thai
[Strings.041E]
Provider                 = "Realtek"
AutoDetect               = "การปรับอัตโนมัติ"
SpeedDuplex              = "ความเร็ว & ดูเพล็กซ์"
10Mb-Half-Duplex         = "10 Mbps ฮาล์ฟดูเพล็กซ์"
10Mb-Full-Duplex         = "10 Mbps ฟุลดูเพล็กซ์"
100Mb-Half-Duplex        = "100 Mbps ฮาล์ฟดูเพล็กซ์"
100Mb-Full-Duplex        = "100 Mbps ฟุลดูเพล็กซ์"
1000Mb-Full-Duplex       = "1.0 Gbps ฟุลดูเพล็กซ์"
2.5Gb-Full-Duplex        = "2.5 Gbps ฟุลดูเพล็กซ์"
NetworkAddress           = "เน็ตเวิร์กแอดเดรส"
IPChksumOffv4            = "IPv4 เช็คซัม ออฟโหลด"
TCPChksumOffv4           = "TCP เช็คซัม ออฟโหลด (IPv4)"
UDPChksumOffv4           = "UDP เช็คซัม ออฟโหลด (IPv4)"
TCPChksumOffv6           = "TCP เช็คซัม ออฟโหลด (IPv6)"
UDPChksumOffv6           = "UDP เช็คซัม ออฟโหลด (IPv6)"
Enabled                  = "เปิดทำงาน"
Disabled                 = "ปิดทำงาน"
TxEnabled                = "Tx เปิดทำงาน"
RxEnabled                = "Rx เปิดทำงาน"
RxTxEnabled              = "Rx & Tx เปิดทำงาน"
LSOv2v4                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv4)"
LSOv2v6                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv6)"
FlowControl              = "โฟลว์คอนโทรล"
PriorityVLAN             = "ลำดับความสำคัญ & VLAN "
PriorityVLANDisabled     = "ลำดับความสำคัญ & VLAN ปิดทำงาน"
PriorityVLANEnabled      = "ลำดับความสำคัญ & VLAN เปิดทำงาน"
InterruptModeration      = "ขัดจังหวะโมเดอเรชัน"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "บัฟเฟอร์รับ"
TransmitBuffers          = "บัฟเฟอร์รับส่ง"
JumboFrame               = "จัมโบ เฟรม"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "การปลุกแลนหลังปิดเครื่อง"
RSS                      = "การเปลี่ยนขนาดด้านที่ได้รับ"
PriorityEnabled          = "ลำดับความสำคัญเปิดทำงาน"
VLANEnabled              = "VLAN เปิดทำงาน"
10MbFirst                = "10 Mbps ก่อน"
100MbFirst               = "100 Mbps ก่อน"
WolShutdownLinkSpeed     = "ความเร็วลิงค์การปลุกแลน & ปิดเครื่อง"
NotSpeedDown             = "ไม่ลดความเร็ว"
GreenEthernet            = "กรีนอีเธอร์เน็ต"
WakeOnPtn                = "เปิดเมื่อรูปแบบตรงกัน"
WakeOnMagPkt             = "เปิดด้วย Magic Packet"
ARPOffload               = "ARP ออฟโหลด"
NsOffload                = "NS ออฟโหลด"
EEE                      = "อีเธอร์เน็ตประหยัดพลังงาน"
NumRssQueues             = "จำนวนสูงสุดของคิว RSS"
1Queue                   = "1 คิว"
2Queue                   = "2 คิว"
4Queue                   = "4 คิว"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Turkish
[Strings.041F]
Provider                 = "Realtek"
AutoDetect               = "Otomatik Görüşme"
SpeedDuplex              = "Hız & İkili"
10Mb-Half-Duplex         = "10 Mbps Yarım İkili"
10Mb-Full-Duplex         = "10 Mbps Tam İkili"
100Mb-Half-Duplex        = "100 Mbps Yarım İkili"
100Mb-Full-Duplex        = "100 Mbps Tam İkili"
1000Mb-Full-Duplex       = "1.0 Gbps Tam İkili"
2.5Gb-Full-Duplex        = "2.5 Gbps Tam İkili"
NetworkAddress           = "Ağ Adresi"
IPChksumOffv4            = "IPv4 Boşaltmayı Sağla"
TCPChksumOffv4           = "TCP Boşaltmayı Sağla (IPv4)"
UDPChksumOffv4           = "UDP Boşaltmayı Sağla (IPv4)"
TCPChksumOffv6           = "TCP Boşaltmayı Sağla (IPv6)"
UDPChksumOffv6           = "UDP Boşaltmayı Sağla (IPv6)"
Enabled                  = "Etkinleştirildi"
Disabled                 = "Devre Dışı Bırakıldı"
TxEnabled                = "Tx Etkinleştirildi"
RxEnabled                = "Rx Etkinleştirildi"
RxTxEnabled              = "Rx & Tx Etkinleştirildi"
LSOv2v4                  = "Boşaltmayı Geniş Gönder v2 (IPv4)"
LSOv2v6                  = "Boşaltmayı Geniş Gönder v2 (IPv6)"
FlowControl              = "Akış Denetimi"
PriorityVLAN             = "Öncelik & VLAN"
PriorityVLANDisabled     = "Öncelik & VLAN Devre Dışı Bırakıldı"
PriorityVLANEnabled      = "Öncelik & VLAN Etkinleştirildi"
InterruptModeration      = "Hafifletmeyi Kes"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Arabellekleri Al"
TransmitBuffers          = "Arabellekleri İlet"
JumboFrame               = "Jumbo Çerçeve"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Yerel Ağ Üzerinden Kapat"
RSS                      = "Yan Ölçüyü Al"
PriorityEnabled          = "Öncelik Etkinleştirildi"
VLANEnabled              = "VLAN Etkinleştirildi"
10MbFirst                = "10 Mbps Önce"
100MbFirst               = "100 Mbps Önce"
WolShutdownLinkSpeed     = "WOL & Kapatma Bağlantı Hızı"
NotSpeedDown             = "Yavaşlatma Değil"
GreenEthernet            = "Yeşil Ethernet"
WakeOnPtn                = "Desen eşleştirme uyanması"
WakeOnMagPkt             = "Sihirli Paket Eşleştirme Uyanması"
ARPOffload               = "ARP Yük Boşaltma"
NsOffload                = "NS Yük Boşaltma"
EEE                      = "Enerji Tasarruflu Ethernet"
NumRssQueues             = "En Fazla RSS Sırası Sayısı"
1Queue                   = "1 Sıra"
2Queue                   = "2 Sıra"
4Queue                   = "4 Sıra"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

;Ukrainian
[Strings.0422]
Provider                 = "Realtek"
AutoDetect               = "Автоматичне узгодження"
SpeedDuplex              = "Швидкість і дуплексний режим"
10Mb-Half-Duplex         = "10 Мб/с — півдуплексний"
10Mb-Full-Duplex         = "10 Мб/с — повнодуплексний"
100Mb-Half-Duplex        = "100 Мб/с — півдуплексний"
100Mb-Full-Duplex        = "100 Мб/с — повнодуплексний"
1000Mb-Full-Duplex       = "1,0 Гб/с — повнодуплексний"
2.5Gb-Full-Duplex        = "2,5 Гб/с — повнодуплексний"
NetworkAddress           = "Мережева адреса"
IPChksumOffv4            = "Розвантаження контрольної суми IPv4"
TCPChksumOffv4           = "Розвантаження контрольної суми TCP (IPv4)"
UDPChksumOffv4           = "Розвантаження контрольної суми UDP (IPv4)"
TCPChksumOffv6           = "Розвантаження контрольної суми TCP (IPv6)"
UDPChksumOffv6           = "Розвантаження контрольної суми UDP (IPv6)"
Enabled                  = "Увімкнено"
Disabled                 = "Вимкнено"
TxEnabled                = "Tx увімкнено"
RxEnabled                = "Rx увімкнено"
RxTxEnabled              = "Rx і Tx увімкнено"
LSOv2v4                  = "Розвантаження великого надсилання верс. 2 (IPv4)"
LSOv2v6                  = "Розвантаження великого надсилання верс. 2 (IPv6)"
FlowControl              = "Регулятор потоку"
PriorityVLAN             = "Пріоритетність та віртуальна локальна мережа"
PriorityVLANDisabled     = "Пріоритетність та віртуальну локальну мережу вимкнено"
PriorityVLANEnabled      = "Пріоритетність та віртуальну локальну мережу увімкнено"
InterruptModeration      = "Переривання черги завершення для керування "
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Отримати буфери"
TransmitBuffers          = "Передати буфери"
JumboFrame               = "Jumbo-кадр"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Вимкнути дистанційне ввімкнення через локальну мережу"
RSS                      = "Receive Side Scaling"
PriorityEnabled          = "Пріоритетність увімкнено"
VLANEnabled              = "Віртуальну локальну мережу ввімкнено"
10MbFirst                = "Спершу 10 Мб/с"
100MbFirst               = "Спершу 100 Мб/с"
WolShutdownLinkSpeed     = "Дистанційне ввімкнення через мережу та швидкість з'єднання під час вимкнення"
NotSpeedDown             = "Без зниження швидкості"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Увімкнення в разі збігу послідовності "
WakeOnMagPkt             = "Увімкнення в разі пакетів Magic Packet"
ARPOffload               = "Розвантаження ARP"
NsOffload                = "Розвантаження NS"
EEE                      = "Energy-Efficient Ethernet"
NumRssQueues             = "Максимальна кількість черг RSS"
1Queue                   = "1 Черга"
2Queue                   = "2 Черги"
4Queue                   = "4 Черги"
AdvancedEEE              = "Розширені параметри EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"

; Vietnamese
[Strings.042A]
Provider                 = "Realtek"
AutoDetect               = "Tự động thỏa thuận"
SpeedDuplex              = "Tốc độ & Song công"
10Mb-Half-Duplex         = "10 Mb/giây bán song công"
10Mb-Full-Duplex         = "10 Mb/giây song công hoàn toàn"
100Mb-Half-Duplex        = "100 Mb/giây bán song công"
100Mb-Full-Duplex        = "100 Mb/giây song công hoàn toàn"
1000Mb-Full-Duplex       = "1 Gb/giây song công hoàn toàn"
2.5Gb-Full-Duplex        = "2.5 Gb/giây song công hoàn toàn"
NetworkAddress           = "Địa chỉ mạng"
IPChksumOffv4            = "Tải kiểm tra tổng IPv4"
TCPChksumOffv4           = "Tải kiểm tra tổng TCP (IPv4)"
UDPChksumOffv4           = "Tải kiểm tra tổng UDP (IPv4)"
TCPChksumOffv6           = "Tải kiểm tra tổng TCP (IPv6)"
UDPChksumOffv6           = "Tải kiểm tra tổng UDP (IPv6)"
Enabled                  = "Bật"
Disabled                 = "Tắt"
TxEnabled                = "Tx bật"
RxEnabled                = "Rx bật"
RxTxEnabled              = "Rx & Tx bật"
LSOv2v4                  = "Tải nội dung lớn v2 (IPv4)"
LSOv2v6                  = "Tải nội dung lớn v2 (IPv6)"
FlowControl              = "Kiểm soát lưu lượng"
PriorityVLAN             = "Ưu tiên & VLAN"
PriorityVLANDisabled     = "Ưu tiên & VLAN tắt"
PriorityVLANEnabled      = "Ưu tiên & VLAN bật"
InterruptModeration      = "Ngắt kiểm soát"
InterruptModerationLevel = "Interrupt Moderation Level"
IMDisabled               = "Disabled"
IMEnabled                = "Enabled"
IMLow                    = "Low"
IMMedium                 = "Medium"
ReceiveBuffers           = "Bộ nhớ đệm nhận"
TransmitBuffers          = "Bộ nhớ đệm gửi"
JumboFrame               = "Khung mở rộng"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "LAN hiện hành khi tắt máy"
RSS                      = "Tỷ lệ bên nhận"
PriorityEnabled          = "Ưu tiên bật"
VLANEnabled              = "VLAN bật"
10MbFirst                = "10 Mb/giây trước"
100MbFirst               = "100 Mb/giây trước"
WolShutdownLinkSpeed     = "LAN hiện hành & Tắt tốc độ kết nối"
NotSpeedDown             = "Không giảm tốc độ"
GreenEthernet            = "Ethernet xanh"
WakeOnPtn                = "Khởi động trùng kiểu"
WakeOnMagPkt             = "Khởi động gói dữ liệu đặc biệt"
ARPOffload               = "Dỡ tải ARP"
NsOffload                = "Giỡ tải NS"
EEE                      = "Ethernet hiệu năng"
NumRssQueues             = "Số chuỗi RSS tối đa"
1Queue                   = "1 chuỗi"
2Queue                   = "2 chuỗi"
4Queue                   = "4 chuỗi"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
RegVlanid                = "VLAN ID"
RscIPv4                  = "Recv Segment Coalescing (IPv4)"
RscIPv6                  = "Recv Segment Coalescing (IPv6)"
IdleRestriction          = "idle power down restriction"
RestrictionDisable       = "No Restriction"
RestrictionEnable        = "Only idle when user is not present"

RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"
RTL81xx.DeviceDesc       = "Realtek(R) PCI(e) Ethernet Controller"

ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

Service.DisplayName      = "Realtek NetAdapter Driver"

DiskDescription          = "Realtek Driver Disk 1"

; TODO: Give your driver service a unique name. (Usually the same as the .sys file)
ServiceName              = "rt68cx21"
;#8128

