// Support SubsystemID
// Driver Version
// MHI (For PCIe mode) - v1.0.0.5 (LE1.2 POST-CS8 based. WHQL)
// UDE - v1.0.0.4 (r0035.1 based. WHQL)
// Modem (QUD) - v1.0.0.2 (r1.00.70 based. WHQL)
// Diagnostic (QUD) - v1.0.0.2 (r1.00.70 based. WHQL)
// Location GNSS Qmux (GNSS) - v1.0.0.7 (LE1.2 POST-CS8 based. SIM Service V1.0.0.38. WHQL)
// Location GNSS (GNSS) - v1.0.0.7 (LE1.2 POST-CS8 based. WHQL)
// FOTA - v1.0.2.1 (F0.1.0.0.9(AP063). WHQL)

// Procedure
1. Install PCIe device with MHI driver(MhiHost.inf) (set driver search path \MHI)
2. Replace MHI child node to UDE driver(qcude.inf) (\UDE)
3. Update all Unknown UDE Client device with QUD driver (\QUD_GNSS)
