;****************************************************************************************************
; Netwtw04.INF
;
;MPCIEX INF
;
; Intel Wireless WiFi Link Adapters
; Installation Script for Windows Blue 64 bit
;
; Copyright (C) 1997-2011 Intel Corporation. All rights reserved.
;
; The information and source code contained herein is the exclusive
; property of Intel Corporation and may not be disclosed, examined
; or reproduced in whole or in part without explicit written authorization
; from the company.
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[version]
Signature   = "$Windows NT$"
Compatible  = 1
Class       = net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %PROVIDER_NAME%
DriverVer   = 03/29/2023,22.220.0.4 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY
PnpLockdown = 1

CatalogFile = Netwtw04.cat


;****************************************************************************************************
; Manufacturer
;----------------------------------------------------------------------------------------------------

[Manufacturer]
%COMPANY_NAME% = Device, NTamd64.10.0

;[ControlFlags]
;ExcludeFromSelect = \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_10108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_10108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50028086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50028086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_500A8086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_500A8086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50128086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50128086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50208086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50208086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_502A8086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_502A8086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50908086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50908086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51028086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51028086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51908086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51908086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54128086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54128086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54208086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54208086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54908086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54908086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55908086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55908086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5C108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5C108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_79 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_69 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_71 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_900A8086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_900A8086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_69 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90128086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90128086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_69 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_95108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_95108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_B9 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_99 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52028086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52028086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_520A8086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_520A8086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_99 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52128086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52128086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52908086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52908086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53028086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53028086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92008086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92008086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_93108086&REV_59 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_93108086&REV_61 , \ 
;        PCI\VEN_8086&DEV_24FB&SUBSYS_20108086 , \ 
;        PCI\VEN_8086&DEV_24FB&SUBSYS_20508086 , \ 
;        PCI\VEN_8086&DEV_24FB&SUBSYS_21108086 , \ 
;        PCI\VEN_8086&DEV_24FB&SUBSYS_21508086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_40108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_40128086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_41108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_44108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_45108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_80108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_81108086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_42108086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_42128086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_43108086 , \ 

;****************************************************************************************************
;Device
;****************************************************************************************************

;****************************************************************************************************
;Device WINT_64
;----------------------------------------------------------------------------------------------------
[Device.NTamd64.10.0]

%NIC_7265_2x2_AC% = Install_MPCIEX_GEN_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_10108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GEN_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_10108086&REV_61 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50008086&REV_61 ; AGN

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50028086&REV_59 ; BGN15

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50028086&REV_61 ; BGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_500A8086&REV_59 ; AGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_500A8086&REV_61 ; AGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50108086&REV_61 ; AC

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50128086&REV_59 ; AC15

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50128086&REV_61 ; AC15

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50208086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50208086&REV_61 ; AGN

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_502A8086&REV_59 ; AGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_502A8086&REV_61 ; AGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50908086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50908086&REV_61 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSARM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSARM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51008086&REV_61 ; AGN

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENSARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51028086&REV_59 ; BGN15

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENSARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51028086&REV_61 ; BGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51908086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51908086&REV_61 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54008086&REV_61 ; AGN

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54108086&REV_61 ; AC

%NIC_7265_2x2_AC15% = Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54128086&REV_59 ; AC15

%NIC_7265_2x2_AC15% = Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54128086&REV_61 ; AC15

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54208086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54208086&REV_61 ; AGN

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54908086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54908086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55908086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55908086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_ASUSM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5C108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_ASUSM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5C108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_SKLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_SKLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_SKLSARM2_D_REV_79_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5F108086&REV_79 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_61 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSD_D_REV_69_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_69 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENSD_D_REV_71_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90008086&REV_71 ; AGN

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_900A8086&REV_59 ; AGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_900A8086&REV_61 ; AGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90108086&REV_69 ; AC

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90128086&REV_59 ; AC15

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90128086&REV_61 ; AC15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENSARSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_91108086&REV_69 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_DELLSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94008086&REV_61 ; AGN

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_95108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_DELLSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_95108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GooSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GooSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GooSD_D_REV_B9_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_9E108086&REV_B9 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_61 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENUIM2_D_REV_99_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52008086&REV_99 ; AGN

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENUIM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52028086&REV_59 ; BGN15

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENUIM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52028086&REV_61 ; BGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_520A8086&REV_59 ; AGN15

%NIC_7265_2x2_AGN15% = Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_520A8086&REV_61 ; AGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUIM2_D_REV_99_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52108086&REV_99 ; AC

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52128086&REV_59 ; AC15

%NIC_7265_2x2_AC15% = Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52128086&REV_61 ; AC15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUIM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52908086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUIM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52908086&REV_61 ; AC

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENUISARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53028086&REV_59 ; BGN15

%NIC_7265_2x2_BGN15% = Install_MPCIEX_GENUISARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53028086&REV_61 ; BGN15

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53108086&REV_61 ; AC

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENUISD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92008086&REV_59 ; AGN

%NIC_7265_2x2_AGN% = Install_MPCIEX_GENUISD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92008086&REV_61 ; AGN

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92108086&REV_61 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_93108086&REV_59 ; AC

%NIC_7265_2x2_AC% = Install_MPCIEX_GENUISARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_93108086&REV_61 ; AC

%NIC_3168_1x1_AC% = Install_MPCIEX_GENSARM2_3168_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_24FB&SUBSYS_20108086 ; AC

%NIC_3168_1x1_AC% = Install_MPCIEX_DELLSARM2_3168_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_24FB&SUBSYS_20508086 ; AC

%NIC_3168_1x1_AC% = Install_MPCIEX_GENM2_3168_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_24FB&SUBSYS_21108086 ; AC

%NIC_3168_1x1_AC% = Install_MPCIEX_DELLM2_3168_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_24FB&SUBSYS_21508086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_40108086 ; AC

%NIC_3165_1x1_AC15% = Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_3165&SUBSYS_40128086 ; AC15

%NIC_3165_1x1_AC% = Install_MPCIEX_GENSARM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_41108086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_DELLM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_44108086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_45108086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_GENSD_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_80108086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_GENSARSD_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_81108086 ; AC

%NIC_3165_1x1_AC% = Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3166&SUBSYS_42108086 ; AC

%NIC_3165_1x1_AC15% = Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC15    ,   PCI\VEN_8086&DEV_3166&SUBSYS_42128086 ; AC15

%NIC_3165_1x1_AC% = Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINT_64_AC    ,   PCI\VEN_8086&DEV_3166&SUBSYS_43108086 ; AC



;****************************************************************************************************
;INSTALL WINT_64
;----------------------------------------------------------------------------------------------------

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2NBT_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2NBT_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUSM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUSM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUSM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUSM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUSM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUSM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SKLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SKLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SKLSARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SKLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SKLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SKLSARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SKLSARM2_D_REV_79_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SKLSARM2_D_REV_79_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SKLSARM2_D_REV_79_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_69_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_69_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_69_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_71_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_71_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_71_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_D_REV_69_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GooSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GooSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GooSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GooSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GooSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GooSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GooSD_D_REV_B9_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GooSD_D_REV_B9_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GooSD_D_REV_B9_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_99_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2WG_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2WG_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_BGN, Reg_7265_2x2_BGN15, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_BGN_2x2_HMC_WINT_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_D_REV_59_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AGN, Reg_7265_2x2_AGN, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_D_REV_61_7265_AGN_2x2_HMC_WINT_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARSD_D_REV_59_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_7265_2x2_AC, Reg_NDIS_WINT_64, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARSD_D_REV_61_7265_AC_2x2_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_3168_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3168_1x1_AC, Reg_NDIS_WINT_64, Reg_SDP, Reg_NDI, Reg_NDI_SDP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_3168_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_3168_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_3168_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3168_1x1_AC, Reg_NDIS_WINT_64, Reg_SDP, Reg_NDI, Reg_NDI_SDP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_3168_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_3168_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_3168_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3168_1x1_AC, Reg_NDIS_WINT_64, Reg_SDP, Reg_NDI, Reg_NDI_SDP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_3168_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_3168_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_3168_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3168_1x1_AC, Reg_NDIS_WINT_64, Reg_SDP, Reg_NDI, Reg_NDI_SDP, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_3168_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_3168_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC15, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_3165_AC_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC15]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC15, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINT_64_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINT_64_AC]
FeatureScore    = 0xFC
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINT_64, Reg_IHV_Router, Reg_AC, Reg_3165_1x1_AC, Reg_NDIS_WINT_64, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINT_64, CopyFiles_IHV_Router
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINT_64_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration.HW
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINT_64_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = Netwtw04, 2, NIC_Service_WINT_64, Common_EventLog_WINT_64

[DelReg_Common]
HKR,,ChannelWidth24
HKR,,ChannelWidth52
HKR,,TGeEnableBits
HKR,,uAPSDSupport
HKR,,CtsToItself
HKR, Ndi\

[Reg_Common]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,CardType,0x00010001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,BTOnThreshold,0x10001,0x4
HKR,,APMMode,0x10001,0x0
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,BaEnable,0x10001,0x0
HKR,,PanTimeoutForResetTxFailCnt,0x10001,0x64
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1
HKR,,uAPSDSupport,0x10001,0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, GUID, 0x00000000, {9296FE7F-CE24-497C-99C9-5795A7E23610}
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, FileMax, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, MaxFileSize, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, LogFileMode, 0x00010001, 0x10000400
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, ClockType, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, BufferSize, 0x00010001, 0x64
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, MinimumBuffers, 0x00010001, 0x9
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, MaximumBuffers, 0x00010001, 0x16
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableFlags, 0x00010001, 0xf
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableFlags, 0x00010001, 0x3ff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableFlags, 0x00010001, 0x1ff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableFlags, 0x00010001, 0x7f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableFlags, 0x00010001, 0x7
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableFlags, 0x00010001, 0x7
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableFlags, 0x00010001, 0x1f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableFlags, 0x00010001, 0x3f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableFlags, 0x00010001, 0x1fff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableFlags, 0x00010001, 0x3f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableFlags, 0x00010001, 0xf
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableFlags, 0x00010001, 0xf
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableFlags, 0x00010001, 0x3f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableFlags, 0x00010001, 0x3f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableFlags, 0x00010001, 0x7
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableFlags, 0x00010001, 0x3f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableFlags, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableFlags, 0x00010001, 0x1f
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableFlags, 0x00010001, 0x7
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, EnableLevel, 0x00010001, 0xf
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, EnableFlags, 0x00010001, 0xC0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverSession\{1F243412-D185-4C47-8B2E-805F9B0833F3}, Status, 0x00010001, 0x0

; following registry keys define the Advanced Property Page (NDI) values. they are common, and the defult values vary between the different reg sections.
[Reg_NDI_BGN]
HKR, Ndi\Params\WirelessMode,			ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode, 			Type, 	    0, "enum",
HKR, Ndi\params\WirelessMode, 			Default,    0, "32" ;bg
HKR, Ndi\Params\WirelessMode, 			Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"0",  	    0, "1. "%WIRELESS_MODE_B%
HKR, Ndi\params\WirelessMode\enum, 		"16", 	    0, "2. "%WIRELESS_MODE_G%
HKR, Ndi\params\WirelessMode\enum, 		"32", 	    0, "3. "%WIRELESS_MODE_BG%

[Reg_NDI_AGN]                                               
HKR, Ndi\Params\WirelessMode,               	ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      		Default,    0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"17",       0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\params\WirelessMode\enum, 		"0",        0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\params\WirelessMode\enum, 		"16",       0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\params\WirelessMode\enum, 		"32",       0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\params\WirelessMode\enum, 		"18",       0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\params\WirelessMode\enum, 		"34",       0, "6. "%WIRELESS_MODE_ABG%

HKR, Ndi\params\RoamingPreferredBandType,     	ParamDesc,  0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	Default,    0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	"0",        0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	"1",        0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,  "2",        0x00000000, "3. "%PREFER_52_BAND_STR%

HKR, Ndi\params\ChannelWidth52,			ParamDesc,  0,  %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,			Type,       0,  "enum"
HKR, Ndi\params\ChannelWidth52,			Default,    0,  "1"
HKR, Ndi\params\ChannelWidth52,			Optional,   0,  "0"
HKR, Ndi\params\ChannelWidth52\enum, 		"0",        0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 		"1",        0,  %CHANNELWIDTHAUTO%

[Reg_NDI_AC]                                                
HKR, Ndi\Params\WirelessMode,               	ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      		Default,    0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"17",       0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\params\WirelessMode\enum, 		"0",        0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\params\WirelessMode\enum, 		"16",       0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\params\WirelessMode\enum, 		"32",       0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\params\WirelessMode\enum, 		"18",       0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\params\WirelessMode\enum, 		"34",       0, "6. "%WIRELESS_MODE_ABG%

HKR, Ndi\params\RoamingPreferredBandType,     	ParamDesc,  0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	Default,    0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	"0",        0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	"1",        0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,  "2",        0x00000000, "3. "%PREFER_52_BAND_STR%

HKR, Ndi\params\ChannelWidth52,			ParamDesc,  0,  %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,			Type,       0,  "enum"
HKR, Ndi\params\ChannelWidth52,			Default,    0,  "1"
HKR, Ndi\params\ChannelWidth52,			Optional,   0,  "0"
HKR, Ndi\params\ChannelWidth52\enum, 		"0",        0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 		"1",        0,  %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,			ParamDesc,  0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,			Type,       0, "enum"
HKR, Ndi\params\IEEE11nMode,			Default,    0, "2"
HKR, Ndi\params\IEEE11nMode,			Optional,   0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 		"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"1",        0, %HT_ENABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"2",        0, %VHT_ENABLED_STR%

[Reg_NDI]                                       
HKR, Ndi\params\ThroughputBoosterEnabled,	ParamDesc,  0x00000000, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\params\ThroughputBoosterEnabled,	Type,  	    0x00000002, "enum"
HKR, Ndi\params\ThroughputBoosterEnabled,	Default,    0x00000002, "0"
HKR, Ndi\params\ThroughputBoosterEnabled,	Optional,   0x00000002, "0"
HKR, Ndi\params\ThroughputBoosterEnabled\enum,  "0",  	    0x00000000, %DISABLED_STR%
HKR, Ndi\params\ThroughputBoosterEnabled\enum,  "1",  	    0x00000000, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth24,			ParamDesc,  0, 	%CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,			Type,       0, 	"enum"
HKR, Ndi\params\ChannelWidth24,			Default,    0, 	"1"
HKR, Ndi\params\ChannelWidth24,			Optional,   0, 	"0"
HKR, Ndi\params\ChannelWidth24\enum, 		"0",        0, 	%CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 		"1",        0, 	%CHANNELWIDTHAUTO%

HKR, Ndi\params\IbssTxPower,      	     	ParamDesc,  0x00000000, %IBSS_TX_POWER_STR%
HKR, Ndi\params\IbssTxPower,      	     	Type,       0x00000002, "enum"
HKR, Ndi\params\IbssTxPower,      	     	Default,    0x00000002, "100"
HKR, Ndi\params\IbssTxPower,      	     	Optional,   0x00000002, "0"
HKR, Ndi\params\IbssTxPower\enum, 	     	"0",        0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"25",       0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"50",       0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"75",       0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"100",      0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RoamAggressiveness,     	ParamDesc,  0x00000000, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\params\RoamAggressiveness,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamAggressiveness,     	Default,    0x00000002, "2"
HKR, Ndi\params\RoamAggressiveness,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamAggressiveness\enum,	"0",        0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"1",        0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"2",        0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"3", 	    0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\RoamAggressiveness\enum,    	"4",        0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\CtsToItself,			ParamDesc,  0x00000000, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\params\CtsToItself,			Type,  	    0x00000002, "enum"
HKR, Ndi\params\CtsToItself,			Default,    0x00000002, "0"
HKR, Ndi\params\CtsToItself,			Optional,   0x00000002, "0"
HKR, Ndi\params\CtsToItself\enum, 		"0",  	    0x00000000, %RTS_CTS_ENABLED_STR%
HKR, Ndi\params\CtsToItself\enum, 		"1",  	    0x00000000, %CTS_TO_SELF_ENABLED_STR%

HKR, Ndi\params\FatChannelIntolerant, 	    	ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	    0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,    0, "0"
HKR, Ndi\params\FatChannelIntolerant, 		Optional,   0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	    0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	    0, %ENABLED_STR%

HKR, Ndi\params\uAPSDSupport, 	    		ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\params\uAPSDSupport, 			Type,	    0, "enum"
HKR, Ndi\params\uAPSDSupport, 			Optional,   0, "0"
HKR, Ndi\params\uAPSDSupport,			Default,    0, "0"
HKR, Ndi\params\uAPSDSupport\enum,  		"0",	    0, %DISABLED_STR%
HKR, Ndi\params\uAPSDSupport\enum,  		"1",	    0, %ENABLED_STR%


HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"

HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"

HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"

HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"

HKR, Ndi\params\MIMOPowerSaveMode,              ParamDesc,  0x00000000, %MIMO_POWER_SAVE_MODE_STR% 
HKR, Ndi\params\MIMOPowerSaveMode,              Type,       0x00000002, "enum" 
HKR, Ndi\params\MIMOPowerSaveMode,              Default,    0x00000002, "0" 
HKR, Ndi\params\MIMOPowerSaveMode,              Optional,   0x00000002, "0" 
HKR, Ndi\params\MIMOPowerSaveMode\enum,         "0",        0x00000000, %MIMO_AUTO_STR% 
HKR, Ndi\params\MIMOPowerSaveMode\enum,         "1",        0x00000000, %NO_MIMO_STR% 
HKR, Ndi\params\MIMOPowerSaveMode\enum,         "2",        0x00000000, %RTS_BEFORE_MIMO_STR% 
HKR, Ndi\params\MIMOPowerSaveMode\enum,         "3",        0x00000000, %NO_RTS_BEFORE_MIMO_STR%


[Reg_NDI_STP]
HKR,,CLSGUID,0,"{15520CF2-F2F6-44eb-97D4-039BC10BEA1D}"

[Reg_NDI_STP1]
HKR,,CLSGUID,0,"{15520CF2-F2F6-44eb-97D4-039BC10BEA1D}"

[Reg_NDI_SDP]
HKR,,CLSGUID,0,"{6C22ABA3-3000-4471-A9BF-622484507292}"

[Reg_NDI_11N]                                   
HKR, Ndi\params\IEEE11nMode,			ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,			Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,			Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,			Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 		"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"1",        	0, %HT_ENABLED_STR%

HKR, Ndi\params\FatChannelIntolerant, 	    	ParamDesc,	0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 	0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,	0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 	0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%


[Reg_NDIS_WINT_64]
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5,wifipro,intel_psm"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet,wlan,vwifi"
HKR, Ndi,             Service,      0, "Netwtw04"

; =========================
; Registry settings by HW
; =========================
[Reg_STP]
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,CtdpSupported,0x10001,1
HKR,,LowLinearitySupported,0x10001,1
HKR,,OtpMode,0x00010001,0x0

[Reg_STP1]
;This section is full copy from STP, if you think it should be changed, go ahead
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,CtdpSupported,0x10001,1
HKR,,LowLinearitySupported,0x10001,1
HKR,,VhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,OtpMode,0x00010001,0x0
HKR,,IbmMutualAuthDisabled,0x00010001,0x1

[Reg_SDP]
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,CtdpSupported,0x10001,1
HKR,,LowLinearitySupported,0x10001,1
HKR,,VhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,OtpMode,0x00010001,0x0

; =========================
; Registry settings by OS
; =========================

[Reg_Common_WINT_64]
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x0
HKR,,CalibrationActiveUcode,0x10001,0x0


; =========================
; Registry settings by Regulatory
; =========================

[Reg_AC]
HKR,,SKU_CAP,0x10001,0xf

[Reg_AGN]
HKR,,SKU_CAP,0x10001,0x7

[Reg_BGN]
HKR,,SKU_CAP,0x10001,0x5


; =============================
; Registry settings for Binding
; =============================

[MSI_NDIS.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

; ===============================
; Registry settings for EventLogs
; ===============================

[Reg_CommonAddEventLog_WINT_64]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwtw04.sys"
HKR,, TypesSupported,   0x00010001, 7



[Reg_7265_2x2_AC]
HKR,,AdapterModel,0,%NIC_7265_2x2_AC%
HKR,,DriverDesc,0,%NIC_7265_2x2_AC%

[Reg_7265_2x2_AGN]
HKR,,AdapterModel,0,%NIC_7265_2x2_AGN%
HKR,,DriverDesc,0,%NIC_7265_2x2_AGN%

[Reg_7265_2x2_BGN15]
HKR,,AdapterModel,0,%NIC_7265_2x2_BGN15%
HKR,,DriverDesc,0,%NIC_7265_2x2_BGN15%

[Reg_7265_2x2_AGN15]
HKR,,AdapterModel,0,%NIC_7265_2x2_AGN15%
HKR,,DriverDesc,0,%NIC_7265_2x2_AGN15%

[Reg_7265_2x2_AC15]
HKR,,AdapterModel,0,%NIC_7265_2x2_AC15%
HKR,,DriverDesc,0,%NIC_7265_2x2_AC15%

[Reg_3168_1x1_AC]
HKR,,AdapterModel,0,%NIC_3168_1x1_AC%
HKR,,DriverDesc,0,%NIC_3168_1x1_AC%

[Reg_3165_1x1_AC]
HKR,,AdapterModel,0,%NIC_3165_1x1_AC%
HKR,,DriverDesc,0,%NIC_3165_1x1_AC%

[Reg_3165_1x1_AC15]
HKR,,AdapterModel,0,%NIC_3165_1x1_AC15%
HKR,,DriverDesc,0,%NIC_3165_1x1_AC15%

[Reg_IHV_Router]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\system32\IntelIHVRouter04.dll"

[NIC_Service_WINT_64]
DisplayName = "___" %NIC_Service_DispName_WINT_64%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\Netwtw04.sys
LoadOrderGroup  = NDIS

[Common_EventLog_WINT_64]
AddReg = Reg_CommonAddEventLog_WINT_64

;----------------------------------------------------------------------------------------------------
; DestinationDirs
;----------------------------------------------------------------------------------------------------

[CopyFiles_Driver_WINT_64]
Netwtw04.sys,,,2
Netwfw04.dat,,,2

[CopyFiles_IHV_Router]
IntelIHVRouter04.dll,,,2

[SourceDisksNames]
1=%SOURCEDISK1%,,

[SourceDisksFiles]
Netwtw04.sys = 1,,
Netwfw04.dat = 1,,
IntelIHVRouter04.dll = 1,,

[DestinationDirs]
DefaultDestDir = 11 ; Windows\System32
CopyFiles_Driver_WINT_64=12;Windows\System32\Drivers
CopyFiles_IHV_Router = 11 ; Windows\System32

[Strings]
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless Adapter Driver for Windows 10 - 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	= "Transmit Power"
ROAMING_AGGRESSIVENESS_STR	= "Roaming Aggressiveness"
MIXED_MODE_PROTECTION_STR   	= "Mixed Mode Protection"
WIRELESS_MODE_STR           	= "802.11a/b/g Wireless Mode"
WIRELESS_MODE_A                 = "5GHz  802.11a"
WIRELESS_MODE_B                 = "2.4GHz 802.11b"
WIRELESS_MODE_G                 = "2.4GHz 802.11g"
WIRELESS_MODE_BG                = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG                = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG               = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	= "Preferred Band"
CHANNELWIDTH52              	= "Channel Width for 5GHz"
CHANNELWIDTH24              	= "Channel Width for 2.4GHz"
TGnMode                     	= "802.11n/ac Wireless Mode"
VHT_ENABLED_STR			= "802.11ac"
HT_ENABLED_STR			= "802.11n"
FAT_CHANNEL_TOLERANT		= "Fat Channel Intolerant"
LOWEST_STR			= "Lowest"
MEDIUM_LOW_STR			= "Medium-low"
MEDIUM_STR			= "Medium"
MEDIUM_HIGH_STR			= "Medium-High"
HIGHEST_STR			= "Highest"
DISABLED_STR			= "Disabled"
ENABLED_STR 			= "Enabled"
CTS_TO_SELF_ENABLED_STR     	= "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR         	= "RTS/CTS Enabled"
CHANNELWIDTH20ONLY          	= "20 MHz Only"
CHANNELWIDTHAUTO            	= "Auto"
NO_PREFERECE_STR            	= "No Preference"
PREFER_24_BAND_STR          	= "Prefer 2.4GHz band"
PREFER_52_BAND_STR          	= "Prefer 5GHz band"
WAKE_ON_MAGIC_PACKET        	= "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	= "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	= "GTK rekeying for WoWLAN"
PM_ARP_OFFLOAD			= "ARP offload for WoWLAN"
PM_NS_OFFLOAD			= "NS offload for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	= "Sleep on WoWLAN Disconnect"
PACKET_COALESCING               = "Packet Coalescing"
U_APSD_SUPPORT			= "U-APSD support"
THROUGHPUTBOOSTER_STR   	= "Throughput Booster"
MIMO_POWER_SAVE_MODE_STR        = "MIMO Power Save Mode" 
MIMO_AUTO_STR                   = "Auto SMPS" 
NO_MIMO_STR                     = "Static SMPS" 
RTS_BEFORE_MIMO_STR             = "Dynamic SMPS" 
NO_RTS_BEFORE_MIMO_STR          = "No SMPS" 

SOURCEDISK1                     = "Intel(R) Wireless Install Disk"

[Strings.0401] ; Arabic (Saudi Arabia)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="برنامج تشغيل محول Intel(R) Wireless لنظام Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="طاقة الإرسال"
ROAMING_AGGRESSIVENESS_STR	="نشاط التجوال"
MIXED_MODE_PROTECTION_STR   	="حماية الوضع المختلط"
WIRELESS_MODE_STR           	="الوضع اللاسلكي 802.11a/b/g"
WIRELESS_MODE_A                 ="5 جيجاهرتز 802.11a"
WIRELESS_MODE_B                 ="2.4  جيجاهرتز 802.11b"
WIRELESS_MODE_G                 ="2.4  جيجاهرتز 802.11g"
WIRELESS_MODE_BG                ="2.4 جيجاهرتز 802.11b/g"
WIRELESS_MODE_AG                ="نطاق مزدوج 802.11a/g"
WIRELESS_MODE_ABG               ="نطاق مزدوج 802.11a/b/g"
PREFERRED_BAND_STR          	="مدى الموجات المفضل"
CHANNELWIDTH52              	="عرض القناة للّتردد 5 غيغاهرتز"
CHANNELWIDTH24              	="عرض القناة للّتردد 2.4 غيغاهرتز"
TGnMode                     	="الوضع اللاسلكي 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="غير متوافق مع قناة 40 ميجاهيرتز"
LOWEST_STR			="الأدنى"
MEDIUM_LOW_STR			="متوسط-منخفض"
MEDIUM_STR			="متوسط"
MEDIUM_HIGH_STR			="متوسط-مرتفع"
HIGHEST_STR			="الأعلى"
DISABLED_STR			="معطل"
ENABLED_STR 			="ممكَّن"
CTS_TO_SELF_ENABLED_STR     	="تمكين CTS الذاتي"
RTS_CTS_ENABLED_STR         	="تمكين RTS/CTS"
CHANNELWIDTH20ONLY          	="20 ميجاهيرتز"
CHANNELWIDTHAUTO            	="تلقائي"
NO_PREFERECE_STR            	="بلا تفضيل"
PREFER_24_BAND_STR          	="يفضل مدى موجات 2.4 جيجاهيرتز"
PREFER_52_BAND_STR          	="أفضّل مدى موجات 5 جيجاهرتز"
WAKE_ON_MAGIC_PACKET        	="التنبيه عند الحزمة السحرية"
WAKE_ON_PATTERN_MATCH       	="التنبيه عند مطابقة النقش"
PM_WIFI_REKEY_OFFLOAD	    	="إعادة إنشاء مفتاح GTK لتنبيه WLAN"
PM_ARP_OFFLOAD			="توزيع نقل البيانات باستخدام ARP لتنبيه WLAN"
PM_NS_OFFLOAD			="توزيع نقل البيانات باستخدام NS لتنبيه WLAN"
DEVICE_SLEEP_ON_DISCONNECT	="السكون عند فصل تنبيه WLAN"
PACKET_COALESCING               ="إدماج الحزمة"
U_APSD_SUPPORT			="دعم U-APSD"
THROUGHPUTBOOSTER_STR   	="معزز معدل النقل"
MIMO_POWER_SAVE_MODE_STR        ="وضع توفير الطاقة لـ MIMO" 
MIMO_AUTO_STR                   ="SMPS التلقائي" 
NO_MIMO_STR                     ="SMPS الثابت" 
RTS_BEFORE_MIMO_STR             ="SMPS الديناميكي" 
NO_RTS_BEFORE_MIMO_STR          ="ما من SMPS" 

SOURCEDISK1                     ="قرص تثبيت مجموعة Intel(R) Wireless"

[Strings.0804] ; Chinese (Simplified)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless 适配器驱动程序（适用于 Windows 10 64 位）"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="传输电源"
ROAMING_AGGRESSIVENESS_STR	="漫游主动性"
MIXED_MODE_PROTECTION_STR   	="混合模式保护"
WIRELESS_MODE_STR           	="802.11a/b/g 无线模式"
WIRELESS_MODE_A                 ="5GHz 802.11a"
WIRELESS_MODE_B                 ="2.4GHz 802.11b"
WIRELESS_MODE_G                 ="2.4GHz 802.11g"
WIRELESS_MODE_BG                ="2.4GHz 802.11b/g"
WIRELESS_MODE_AG                ="双频带 802.11a/g"
WIRELESS_MODE_ABG               ="双频带 802.11a/b/g"
PREFERRED_BAND_STR          	="首选频带"
CHANNELWIDTH52              	="5GHz 信道宽度"
CHANNELWIDTH24              	="2.4GHz 信道宽度"
TGnMode                     	="802.11n/ac 无线模式"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="与 40Mhz 信道不兼容"
LOWEST_STR			="最低值"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中间"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高值"
DISABLED_STR			="已禁用"
ENABLED_STR 			="已启用"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self 已启用"
RTS_CTS_ENABLED_STR         	="RTS/CTS 已启用"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自动"
NO_PREFERECE_STR            	="无首选项"
PREFER_24_BAND_STR          	="首选 2.4 GHz 频带"
PREFER_52_BAND_STR          	="首选 5GHz 频带"
WAKE_ON_MAGIC_PACKET        	="唤醒幻数据包"
WAKE_ON_PATTERN_MATCH       	="唤醒模式匹配"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN 的 GTK 重新生成密钥"
PM_ARP_OFFLOAD			="WoWLAN 的 ARP 卸载"
PM_NS_OFFLOAD			="WoWLAN 的 NS 卸载"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 断开连接时睡眠"
PACKET_COALESCING               ="数据包合并"
U_APSD_SUPPORT			="支持 U-APSD "
THROUGHPUTBOOSTER_STR   	="吞吐量助推器"
MIMO_POWER_SAVE_MODE_STR        ="MIMO 节能模式" 
MIMO_AUTO_STR                   ="自动 SMPS" 
NO_MIMO_STR                     ="静态 SMPS" 
RTS_BEFORE_MIMO_STR             ="动态 SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="无 SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless 系列安装盘"

[Strings.0404] ; Chinese (Traditional)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="用於 Windows 10 64 Bit 的 Intel(R) Wireless 介面卡驅動程式"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="傳輸電源"
ROAMING_AGGRESSIVENESS_STR	="漫遊積極度"
MIXED_MODE_PROTECTION_STR   	="混合模式保護"
WIRELESS_MODE_STR           	="802.11a/b/g 無線模式"
WIRELESS_MODE_A                 ="5GHz 802.11a"
WIRELESS_MODE_B                 ="2.4GHz 802.11b"
WIRELESS_MODE_G                 ="2.4GHz 802.11g"
WIRELESS_MODE_BG                ="2.4GHz 802.11b/g"
WIRELESS_MODE_AG                ="雙頻 802.11a/g"
WIRELESS_MODE_ABG               ="雙頻 802.11a/b/g"
PREFERRED_BAND_STR          	="偏好的頻帶"
CHANNELWIDTH52              	="5GHz 的通道寬度"
CHANNELWIDTH24              	="2.4GHz 的通道寬度"
TGnMode                     	="802.11n/ac 無線模式"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="不容大量通道"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="停用"
ENABLED_STR 			="啟用"
CTS_TO_SELF_ENABLED_STR     	="啟用 CTS-to-self"
RTS_CTS_ENABLED_STR         	="啟用 RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
NO_PREFERECE_STR            	="無偏好設定"
PREFER_24_BAND_STR          	="喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR          	="偏好 5GHz 頻帶"
WAKE_ON_MAGIC_PACKET        	="收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH       	="收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD			="WoWLAN ARP 卸載"
PM_NS_OFFLOAD			="WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 中斷連線時睡眠"
PACKET_COALESCING               ="封包聯合"
U_APSD_SUPPORT			="U-APSD 支援"
THROUGHPUTBOOSTER_STR   	="傳輸加速"
MIMO_POWER_SAVE_MODE_STR        ="MIMO 省電模式" 
MIMO_AUTO_STR                   ="自動 SMPS" 
NO_MIMO_STR                     ="靜態 SMPS" 
RTS_BEFORE_MIMO_STR             ="動態 SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="無 SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless 系列安裝磁碟"

[Strings.0C04] ; Chinese (Hong Kong)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="用於 Windows 10 64 Bit 的 Intel(R) Wireless 介面卡驅動程式"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="傳輸電源"
ROAMING_AGGRESSIVENESS_STR	="漫遊積極度"
MIXED_MODE_PROTECTION_STR   	="混合模式保護"
WIRELESS_MODE_STR           	="802.11a/b/g 無線模式"
WIRELESS_MODE_A                 ="5GHz 802.11a"
WIRELESS_MODE_B                 ="2.4GHz 802.11b"
WIRELESS_MODE_G                 ="2.4GHz 802.11g"
WIRELESS_MODE_BG                ="2.4GHz 802.11b/g"
WIRELESS_MODE_AG                ="雙頻 802.11a/g"
WIRELESS_MODE_ABG               ="雙頻 802.11a/b/g"
PREFERRED_BAND_STR          	="偏好的頻帶"
CHANNELWIDTH52              	="5GHz 的通道寬度"
CHANNELWIDTH24              	="2.4GHz 的通道寬度"
TGnMode                     	="802.11n/ac 無線模式"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="不容大量通道"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="停用"
ENABLED_STR 			="啟用"
CTS_TO_SELF_ENABLED_STR     	="啟用 CTS-to-self"
RTS_CTS_ENABLED_STR         	="啟用 RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
NO_PREFERECE_STR            	="無偏好設定"
PREFER_24_BAND_STR          	="喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR          	="偏好 5GHz 頻帶"
WAKE_ON_MAGIC_PACKET        	="收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH       	="收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD			="WoWLAN ARP 卸載"
PM_NS_OFFLOAD			="WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 中斷連線時睡眠"
PACKET_COALESCING               ="封包聯合"
U_APSD_SUPPORT			="U-APSD 支援"
THROUGHPUTBOOSTER_STR   	="傳輸加速"
MIMO_POWER_SAVE_MODE_STR        ="MIMO 省電模式" 
MIMO_AUTO_STR                   ="自動 SMPS" 
NO_MIMO_STR                     ="靜態 SMPS" 
RTS_BEFORE_MIMO_STR             ="動態 SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="無 SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless 系列安裝磁碟"

[Strings.0405] ; Czech (Czechia)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Ovladač adaptéru Intel(R) Wireless pro systém Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Vysílací energie"
ROAMING_AGGRESSIVENESS_STR	="Agresivita roamingu"
MIXED_MODE_PROTECTION_STR   	="Ochrana smíšeného režimu"
WIRELESS_MODE_STR           	="Bezdrátový režim 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Upřednostňované pásmo"
CHANNELWIDTH52              	="Šířka kanálu pro 5 GHz"
CHANNELWIDTH24              	="Šířka kanálu pro 2,4 GHz"
TGnMode                     	="Bezdrátový režim 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Nekompatibilní s šířkou kanálu 40 MHz"
LOWEST_STR			="Nejnižší"
MEDIUM_LOW_STR			="Středně nízký"
MEDIUM_STR			="Střední"
MEDIUM_HIGH_STR			="Středně vysoký"
HIGHEST_STR			="Nejvyšší"
DISABLED_STR			="Zakázáno"
ENABLED_STR 			="Povoleno"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self povoleno"
RTS_CTS_ENABLED_STR         	="RTS/CTS povoleno"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaticky"
NO_PREFERECE_STR            	="Žádná předvolba"
PREFER_24_BAND_STR          	="Upřednostňovat pásmo 2,4 GHz"
PREFER_52_BAND_STR          	="Dát přednost pásmu 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Probuzení paketem Magic"
WAKE_ON_PATTERN_MATCH       	="Probuzení porovnávacím vzorkem"
PM_WIFI_REKEY_OFFLOAD	    	="Vystavování nových klíčů GTK pro technologii WoWLAN"
PM_ARP_OFFLOAD			="Snižování zatížení ARP pro technologii WoWLAN"
PM_NS_OFFLOAD			="Snižování zatížení NS pro technologii WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Režim spánku při odpojení technologie WoWLAN"
PACKET_COALESCING               ="Slučování paketů"
U_APSD_SUPPORT			="Podpora U-APSD"
THROUGHPUTBOOSTER_STR   	="Podpora průchodnosti"
MIMO_POWER_SAVE_MODE_STR        ="Režim úspory energie MIMO" 
MIMO_AUTO_STR                   ="Automatický režim SMPS" 
NO_MIMO_STR                     ="Statický režim SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamický režim SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Žádný režim SMPS" 

SOURCEDISK1                     ="Instalační disk adaptéru řady Intel(R) Wireless"

[Strings.0406] ; Danish (Denmark)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless adapter driver til Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Sendeeffekt"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
MIXED_MODE_PROTECTION_STR   	="Beskyttelse til blandet miljø"
WIRELESS_MODE_STR           	="802.11a/b/g trådløs tilstand"
WIRELESS_MODE_A                 ="5GHz 802.11a"
WIRELESS_MODE_B                 ="2,4GHz 802.11b"
WIRELESS_MODE_G                 ="2,4GHz 802.11g"
WIRELESS_MODE_BG                ="2,4GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="Kanalbredde for 5 GHz"
CHANNELWIDTH24              	="Kanalbredde for 2,4 GHz"
TGnMode                     	="802.11n/ac trådløs tilstand"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="40Mhz kanal intolerant"
LOWEST_STR			="Laveste"
MEDIUM_LOW_STR			="Mellem-lav"
MEDIUM_STR			="Mellem"
MEDIUM_HIGH_STR			="Mellem-høj"
HIGHEST_STR			="Højeste"
DISABLED_STR			="Deaktiveret"
ENABLED_STR 			="Aktiveret"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self aktiveret "
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiveret "
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Ingen indstilling"
PREFER_24_BAND_STR          	="Foretræk 2,4 GHz bånd"
PREFER_52_BAND_STR          	="Foretræk 5GHz-båndet"
WAKE_ON_MAGIC_PACKET        	="Vækning ved magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Vækning ved mønstermatch"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nøglefornyelse til WoWLAN"
PM_ARP_OFFLOAD			="ARP-aflastning til WoWLAN"
PM_NS_OFFLOAD			="NS-aflastning til WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slumring ved afbrydelse af WoWLAN"
PACKET_COALESCING               ="Pakke-samling"
U_APSD_SUPPORT			="U-APSD Support"
THROUGHPUTBOOSTER_STR   	="Gennemløbsforstærker"
MIMO_POWER_SAVE_MODE_STR        ="MIMO-strømsparetilstand" 
MIMO_AUTO_STR                   ="Auto-SMPS" 
NO_MIMO_STR                     ="Statisk SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamisk SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Ingen SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless installationsdisk"

[Strings.0407] ; German (Germany)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless Adaptertreiber für Windows 10 64-Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Übertragungsleistung"
ROAMING_AGGRESSIVENESS_STR	="Roaming-Dynamik"
MIXED_MODE_PROTECTION_STR   	="Schutz f. gemischte Umgebungen"
WIRELESS_MODE_STR           	="Wireless-Modus 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Bevorzugtes Band"
CHANNELWIDTH52              	="Kanalbreite für 5 GHz"
CHANNELWIDTH24              	="Kanalbreite für 2,4 GHz"
TGnMode                     	="Wireless-Modus 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Fat Kanal Intolerant"
LOWEST_STR			="Am niedrigsten"
MEDIUM_LOW_STR			="Mittel-niedrig"
MEDIUM_STR			="Mittel"
MEDIUM_HIGH_STR			="Mittel-hoch"
HIGHEST_STR			="Am höchsten"
DISABLED_STR			="Deaktiviert"
ENABLED_STR 			="Aktiviert"
CTS_TO_SELF_ENABLED_STR     	="'CTS-to-self' aktiviert"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiviert"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Keine Einstellung"
PREFER_24_BAND_STR          	="2,4-GHz-Band bevorzugen"
PREFER_52_BAND_STR          	="5 GHz-Band bevorzugt"
WAKE_ON_MAGIC_PACKET        	="Aktivierung durch Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivierung durch Musterübereinstimmung"
PM_WIFI_REKEY_OFFLOAD	    	="GTK führt Neuverschlüsselung für WoWLAN durch"
PM_ARP_OFFLOAD			="ARP-Offload für WoWLAN"
PM_NS_OFFLOAD			="NS-Offload für WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Medientrennung beim Aufrechterhalten des Energiesparmodus von WoWLAN"
PACKET_COALESCING               ="Paketzusammenfügung"
U_APSD_SUPPORT			="U-APSD-Unterstützung"
THROUGHPUTBOOSTER_STR   	="Durchsatzbooster"
MIMO_POWER_SAVE_MODE_STR        ="MIMO-Energiesparmodus" 
MIMO_AUTO_STR                   ="Auto-SMPS" 
NO_MIMO_STR                     ="Statische SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamische SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Keine SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless - Installationsdiskette"

[Strings.0408] ; Greek (Greece)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Πρόγραμμα οδήγησης προσαρμογέα Intel(R) Wireless για Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Ισχύς μετάδοσης"
ROAMING_AGGRESSIVENESS_STR	="Δυναμικότητα περιαγωγής"
MIXED_MODE_PROTECTION_STR   	="Προστασία μεικτής λειτουργίας"
WIRELESS_MODE_STR           	="Ασύρματη λειτουργία 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Διπλή ζώνη 802.11a/g"
WIRELESS_MODE_ABG               ="Διπλή ζώνη 802.11a/b/g"
PREFERRED_BAND_STR          	="Προτιμώμενη ζώνη"
CHANNELWIDTH52              	="Εύρος καναλιού για 5GHz"
CHANNELWIDTH24              	="Εύρος καναλιού για 2,4GHz"
TGnMode                     	="Ασύρματη λειτουργία 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Μη συμβατό με ισχυρά κανάλια"
LOWEST_STR			="Χαμηλότερη"
MEDIUM_LOW_STR			="Μεσαία-Χαμηλή"
MEDIUM_STR			="Μεσαία"
MEDIUM_HIGH_STR			="Μεσαία-Υψηλή"
HIGHEST_STR			="Υψηλότερη"
DISABLED_STR			="Απενεργοποιημένη"
ENABLED_STR 			="Ενεργοποιημένη"
CTS_TO_SELF_ENABLED_STR     	="Ενεργοποιημένο CTS-to-self"
RTS_CTS_ENABLED_STR         	="Ενεργοποιημένο RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Αυτόματα"
NO_PREFERECE_STR            	="Καμία προτίμηση"
PREFER_24_BAND_STR          	="Προτίμηση ζώνη 2,4 GHz"
PREFER_52_BAND_STR          	="Προτίμηση ζώνης 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Ενεργοποίηση με Μαγικό πακέτο"
WAKE_ON_PATTERN_MATCH       	="Ενεργοποίηση με αντιστοίχιση μοτίβου"
PM_WIFI_REKEY_OFFLOAD	    	="Το GTK ζητά τη δημιουργία νέου κλειδιού για WoWLAN"
PM_ARP_OFFLOAD			="Μείωση φόρτου ARP για WoWLAN"
PM_NS_OFFLOAD			="Μείωση φόρτου NS για WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Αναστολή λειτουργίας κατά την αποσύνδεση του WoWLAN"
PACKET_COALESCING               ="Ενοποίηση πακέτων"
U_APSD_SUPPORT			="Υποστήριξη U-APSD"
THROUGHPUTBOOSTER_STR   	="Ενισχυτής μετάδοσης"
MIMO_POWER_SAVE_MODE_STR        ="Λειτουργία εξοικονόμησης ενέργειας MIMO" 
MIMO_AUTO_STR                   ="Αυτόματο SMPS" 
NO_MIMO_STR                     ="Στατικό SMPS" 
RTS_BEFORE_MIMO_STR             ="Δυναμικό SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Χωρίς SMPS" 

SOURCEDISK1                     ="Δισκέτα εγκατάστασης Intel(R) Wireless"

[Strings.0C0A] ; Spanish (Spain)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Controlador del adaptador Intel(R) Wireless para Windows 10 de 64 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Potencia de transmisión"
ROAMING_AGGRESSIVENESS_STR	="Agresividad de itinerancia"
MIXED_MODE_PROTECTION_STR   	="Protección de modo mixto"
WIRELESS_MODE_STR           	="Modo inalámbrico 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Doble banda 802.11a/g"
WIRELESS_MODE_ABG               ="Doble banda 802.11a/b/g"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Ancho de canal para 5 GHz"
CHANNELWIDTH24              	="Ancho de canal para 2,4GHz"
TGnMode                     	="Modo inalámbrico 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="No compatible con canal de 40 MHz"
LOWEST_STR			="Mínimo"
MEDIUM_LOW_STR			="Bajo"
MEDIUM_STR			="Mediano"
MEDIUM_HIGH_STR			="Alto"
HIGHEST_STR			="Máximo"
DISABLED_STR			="Desactivado"
ENABLED_STR 			="Activado"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS activado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automático"
NO_PREFERECE_STR            	="Sin preferencias"
PREFER_24_BAND_STR          	="Preferir la banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferencia de banda 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet de reactivación"
WAKE_ON_PATTERN_MATCH       	="Coincidencia de patrones de reactivación"
PM_WIFI_REKEY_OFFLOAD	    	="Regeneración de clave GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspensión al desconectar WoWLAN"
PACKET_COALESCING               ="Fusión de paquetes"
U_APSD_SUPPORT			="Soporte de U-APSD"
THROUGHPUTBOOSTER_STR   	="Impulsar la capacidad de proceso"
MIMO_POWER_SAVE_MODE_STR        ="Modo de ahorro de energía MIMO" 
MIMO_AUTO_STR                   ="SMPS automático" 
NO_MIMO_STR                     ="SMPS estático" 
RTS_BEFORE_MIMO_STR             ="SMPS dinámico" 
NO_RTS_BEFORE_MIMO_STR          ="Sin SMPS" 

SOURCEDISK1                     ="Disco de instalación de Intel(R) Wireless"

[Strings.040B] ; Finnish (Finland)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless -sovitinohjain Windows 10 64-bit -käyttöjärjestelmään"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Lähetysteho"
ROAMING_AGGRESSIVENESS_STR	="Solukonpäivitysaktiivisuus"
MIXED_MODE_PROTECTION_STR   	="Sekatilan Suojaus"
WIRELESS_MODE_STR           	="802.11a/b/g Langaton tila"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Kaksikaistainen 802.11a/g"
WIRELESS_MODE_ABG               ="Kaksikaistainen 802.11a/b/g"
PREFERRED_BAND_STR          	="Ensisijainen kaista"
CHANNELWIDTH52              	="5 GHz:n kanavaleveys"
CHANNELWIDTH24              	="2,4 GHz:n kanavaleveys"
TGnMode                     	="802.11n/ac Langaton tila"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Fat Channel -esto"
LOWEST_STR			="Pienin"
MEDIUM_LOW_STR			="Kohtalainen-pieni"
MEDIUM_STR			="Kohtalainen"
MEDIUM_HIGH_STR			="Kohtalainen-suuri"
HIGHEST_STR			="Suurin"
DISABLED_STR			="Poissa käytöstä"
ENABLED_STR 			="Käytössä"
CTS_TO_SELF_ENABLED_STR     	="CTS itselle käytössä"
RTS_CTS_ENABLED_STR         	="RTS/CTS käytössä"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaattinen"
NO_PREFERECE_STR            	="Ei ensisijaisuutta"
PREFER_24_BAND_STR          	="2,4 GHz:n kaista ensisijainen"
PREFER_52_BAND_STR          	="5 GHz:n kaista"
WAKE_ON_MAGIC_PACKET        	="Aktivointi Magic-paketilla"
WAKE_ON_PATTERN_MATCH       	="Aktivointi mallivastaavuudella"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN-toiminnon GTK-uudelleenavainnus "
PM_ARP_OFFLOAD			="WoWLAN-toiminnon ARP-purku"
PM_NS_OFFLOAD			="WoWLAN-toiminnon NS-purku"
DEVICE_SLEEP_ON_DISCONNECT	="Lepotilaan, kun WoWLAN-yhteys katkaistu"
PACKET_COALESCING               ="Pakettien yhdistäminen"
U_APSD_SUPPORT			="U-APSD-tuki"
THROUGHPUTBOOSTER_STR   	="Siirtomäärän tehostus"
MIMO_POWER_SAVE_MODE_STR        ="MIMO-virransäästötila" 
MIMO_AUTO_STR                   ="AutomaattinenSMPS" 
NO_MIMO_STR                     ="Staattinen SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynaaminen SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Ei SMPS:ää" 

SOURCEDISK1                     ="Intel(R) Wireless asennuslevy"

[Strings.040C] ; French (France)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Pilote de carte Intel(R) Wireless pour Windows 10 64 bits "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Puissance de transmission"
ROAMING_AGGRESSIVENESS_STR	="Agressivité de l’itinérance"
MIXED_MODE_PROTECTION_STR   	="Protection en mode mixte"
WIRELESS_MODE_STR           	="Mode sans fil 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Bande privilégiée"
CHANNELWIDTH52              	="Largeur de canal pour 5 GHz"
CHANNELWIDTH24              	="Largeur de canal pour 2,4 GHz"
TGnMode                     	="Mode sans fil 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Incompatible avec canaux de 40 MHz"
LOWEST_STR			="Min."
MEDIUM_LOW_STR			="Faible"
MEDIUM_STR			="Moyenne"
MEDIUM_HIGH_STR			="Élevée"
HIGHEST_STR			="Max."
DISABLED_STR			="Désactivé(e)"
ENABLED_STR 			="Activé(e)"
CTS_TO_SELF_ENABLED_STR     	="Auto-CTS activée"
RTS_CTS_ENABLED_STR         	="RTS/CTS activée"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Aucune préférence"
PREFER_24_BAND_STR          	="Préférer bande 2,4 GHz"
PREFER_52_BAND_STR          	="Préférer la bande 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondance au modèle WOL"
PM_WIFI_REKEY_OFFLOAD	    	="Régénération des clés GTK pour WoWLAN"
PM_ARP_OFFLOAD			="Délestage ARP pour WoWLAN"
PM_NS_OFFLOAD			="Délestage NS pour WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Veille à la déconnexion WoWLAN"
PACKET_COALESCING               ="Fusion des paquets"
U_APSD_SUPPORT			="Assistance U-APSD"
THROUGHPUTBOOSTER_STR   	="Multiplicateur de débit"
MIMO_POWER_SAVE_MODE_STR        ="MIMO – Mode économie d'énergie" 
MIMO_AUTO_STR                   ="SMPS auto" 
NO_MIMO_STR                     ="SMPS statique" 
RTS_BEFORE_MIMO_STR             ="SMPS dynamique" 
NO_RTS_BEFORE_MIMO_STR          ="SMPS désactivé" 

SOURCEDISK1                     ="Disque d'installation de Intel(R) Wireless"

[Strings.040D] ; Hebrew (Israel)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="מנהל התקן של מתאם Intel(R) Wireless עבור Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="עוצמת שידור"
ROAMING_AGGRESSIVENESS_STR	="תוקפנות נדידה"
MIXED_MODE_PROTECTION_STR   	="הגנת מצב מעורב"
WIRELESS_MODE_STR           	="מצב אלחוטי 802.11a/b/g"
WIRELESS_MODE_A                 ="5GHz ‏802.11a"
WIRELESS_MODE_B                 ="2.4GHz ‏802.11b"
WIRELESS_MODE_G                 ="2.4GHz ‏802.11g"
WIRELESS_MODE_BG                ="2.4GHz ‏802.11b/g"
WIRELESS_MODE_AG                ="פס כפול 802.11a/g"
WIRELESS_MODE_ABG               ="פס כפול 802.11a/b/g"
PREFERRED_BAND_STR          	="פס מועדף"
CHANNELWIDTH52              	="רוחב פס עבור 5GHz"
CHANNELWIDTH24              	="רוחב פס עבור 2.4GHz"
TGnMode                     	="מצב אלחוטי 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="לא תואם לערוץ 40Mhz"
LOWEST_STR			="נמוך ביותר"
MEDIUM_LOW_STR			="בינוני-נמוך"
MEDIUM_STR			="בינוני"
MEDIUM_HIGH_STR			="בינוני-גבוה"
HIGHEST_STR			="גבוה ביותר"
DISABLED_STR			="מנוטרל"
ENABLED_STR 			="זמין"
CTS_TO_SELF_ENABLED_STR     	="מאופשר CTS-אל-עצמו"
RTS_CTS_ENABLED_STR         	="מאופשר RTS/CTS"
CHANNELWIDTH20ONLY          	="‎20 MHz"
CHANNELWIDTHAUTO            	="אוטומטי"
NO_PREFERECE_STR            	="אין העדפה"
PREFER_24_BAND_STR          	="העדפת פס ‎2.4GHz"
PREFER_52_BAND_STR          	="העדפת פס ‎5GHz"
WAKE_ON_MAGIC_PACKET        	="התעורר בעת מנת Magic"
WAKE_ON_PATTERN_MATCH       	="התעורר בעת התאמת תבנית"
PM_WIFI_REKEY_OFFLOAD	    	="החלפת מפתחות GTK עבור WoWLAN"
PM_ARP_OFFLOAD			="העברת ARP עבור WoWLAN"
PM_NS_OFFLOAD			="העברת NS עבור WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="כניסה למצב שינה עם ניתוק WoWLAN"
PACKET_COALESCING               ="מיזוג מנה"
U_APSD_SUPPORT			="תמיכה ב- U-APSD"
THROUGHPUTBOOSTER_STR   	="הגברת תפוקה"
MIMO_POWER_SAVE_MODE_STR        ="מצב חיסכון בחשמל MIMO" 
MIMO_AUTO_STR                   ="SMPS אוטומטי" 
NO_MIMO_STR                     ="SMPS סטטי" 
RTS_BEFORE_MIMO_STR             ="SMPS דינמי" 
NO_RTS_BEFORE_MIMO_STR          ="ללא SMPS" 

SOURCEDISK1                     ="דיסק התקנה של Intel(R) Wireless"

[Strings.040E] ; Hungarian (Hungary)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless adapter illesztőprogram 64 bites Windows 10"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Sugárzási teljesítmény"
ROAMING_AGGRESSIVENESS_STR	="A barangolás intenzitása"
MIXED_MODE_PROTECTION_STR   	="Vegyes üzemmódú védelem"
WIRELESS_MODE_STR           	="802.11a/b/g Vezeték nélküli üzemmód"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Preferált frekvenciasáv"
CHANNELWIDTH52              	="Csatorna sávszélessége 5 GHz értékre"
CHANNELWIDTH24              	="Csatorna sávszélessége 2,4 GHz értékre"
TGnMode                     	="802.11n/ac Vezeték nélküli üzemmód"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Csökkentett sávszélességen működik"
LOWEST_STR			="Legalacsonyabb"
MEDIUM_LOW_STR			="Közepes - alacsony"
MEDIUM_STR			="Közepes"
MEDIUM_HIGH_STR			="Közepes - magas"
HIGHEST_STR			="Legmagasabb"
DISABLED_STR			="Letiltva"
ENABLED_STR 			="Engedélyezve"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self engedélyezve"
RTS_CTS_ENABLED_STR         	="RTS/CTS engedélyezve"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Nincs preferencia"
PREFER_24_BAND_STR          	="2,4 GHz-es sáv preferálása"
PREFER_52_BAND_STR          	="A 5 GHz-es sáv előnyben részesítése"
WAKE_ON_MAGIC_PACKET        	="Ébresztés magic-csomaggal"
WAKE_ON_PATTERN_MATCH       	="Ébresztés mintaegyezésre"
PM_WIFI_REKEY_OFFLOAD	    	="GTK újrakulcsolás WoWLAN hálózathoz"
PM_ARP_OFFLOAD			="ARP tehermentesítés WoWLAN hálózathoz"
PM_NS_OFFLOAD			="NS tehermentesítés WoWLAN hálózathoz"
DEVICE_SLEEP_ON_DISCONNECT	="Alvó állapot WoWLAN hálózati szétkapcsolás esetén"
PACKET_COALESCING               ="Csomagegyesítés"
U_APSD_SUPPORT			="U-APSD támogatás"
THROUGHPUTBOOSTER_STR   	="Átviteli sebesség növelés "
MIMO_POWER_SAVE_MODE_STR        ="MIMO energiatakarékos üzemmód" 
MIMO_AUTO_STR                   ="Auto. SMPS" 
NO_MIMO_STR                     ="Statikus SMPS" 
RTS_BEFORE_MIMO_STR             ="Dinamikus SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Nincs SMPS" 

SOURCEDISK1                     ="Intel(R) Wireless telepítő lemez"

[Strings.0410] ; Italian (Italy)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Driver scheda Intel(R) Wireless per Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Potenza di trasmissione"
ROAMING_AGGRESSIVENESS_STR	="Efficacia roaming"
MIXED_MODE_PROTECTION_STR   	="Protezione a modalità mista"
WIRELESS_MODE_STR           	="Modalità wireless 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802311b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Banda preferita"
CHANNELWIDTH52              	="Larghezza canale per 5 GHz"
CHANNELWIDTH24              	="Larghezza canale per 2,4 GHz"
TGnMode                     	="Modalità wireless 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Fat Channel incompatibile"
LOWEST_STR			="Minimo"
MEDIUM_LOW_STR			="Medio-basso"
MEDIUM_STR			="Medio"
MEDIUM_HIGH_STR			="Medio-alto"
HIGHEST_STR			="Massimo"
DISABLED_STR			="Disattivata"
ENABLED_STR 			="Attivata"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self attivato"
RTS_CTS_ENABLED_STR         	="Attivato RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Nessuna preferenza"
PREFER_24_BAND_STR          	="Preferenza a banda a 2,4 GHz"
PREFER_52_BAND_STR          	="Banda a 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet per riattivazione"
WAKE_ON_PATTERN_MATCH       	="Corrispondenza motivo per riattivazione"
PM_WIFI_REKEY_OFFLOAD	    	="Rigenerazione delle chiavi GTK per WoWLAN"
PM_ARP_OFFLOAD			="Offload ARP per WoWLAN"
PM_NS_OFFLOAD			="Offload NS per WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Sospensione attiva alla disconnessione da WoWLAN"
PACKET_COALESCING               ="Unione pacchetti"
U_APSD_SUPPORT			="Supporto U-APSD"
THROUGHPUTBOOSTER_STR   	="Incremento del throughput"
MIMO_POWER_SAVE_MODE_STR        ="Modalità risparmio energia MIMO" 
MIMO_AUTO_STR                   ="SMPS automatico" 
NO_MIMO_STR                     ="SMPS statico" 
RTS_BEFORE_MIMO_STR             ="SMPS dinamico" 
NO_RTS_BEFORE_MIMO_STR          ="Senza SMPS" 

SOURCEDISK1                     ="Disco di installazione per Intel(R) Wireless"

[Strings.0411] ; Japanese (Japan)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Windows 10 64 ビット用 Intel(R) Wireless アダプタードライバー"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="送信パワー"
ROAMING_AGGRESSIVENESS_STR	="ローミングの積極性"
MIXED_MODE_PROTECTION_STR   	="混在モード保護"
WIRELESS_MODE_STR           	="802.11a/b/g ワイヤレスモード"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2.4 GHz 802.11b"
WIRELESS_MODE_G                 ="2.4 GHz 802.11g"
WIRELESS_MODE_BG                ="2.4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="デュアルバンド 802.11a/b/g"
PREFERRED_BAND_STR          	="優先バンド"
CHANNELWIDTH52              	="チャネル幅 (5GHz 用)"
CHANNELWIDTH24              	="チャネル幅 (2.4GHz 用)"
TGnMode                     	="802.11n/ac ワイヤレスモード"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="40Mhz チャネル幅非互換"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="無効"
ENABLED_STR 			="有効"
CTS_TO_SELF_ENABLED_STR     	="個別 CTS 有効"
RTS_CTS_ENABLED_STR         	="RTS/CTS 有効"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
NO_PREFERECE_STR            	="優先順位なし"
PREFER_24_BAND_STR          	="2.4 GHz バンドの優先"
PREFER_52_BAND_STR          	="5 GHz バンドを優先"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN の GTK Rekey"
PM_ARP_OFFLOAD			="WoWLAN の ARP オフロード"
PM_NS_OFFLOAD			="WoWLAN の NS オフロード"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN のスリープ状態の解除"
PACKET_COALESCING               ="パケット結合"
U_APSD_SUPPORT			="U-APSD 対応"
THROUGHPUTBOOSTER_STR   	="スループット・ブースター"
MIMO_POWER_SAVE_MODE_STR        ="MIMO 省電力モード" 
MIMO_AUTO_STR                   ="自動 SMPS" 
NO_MIMO_STR                     ="静的 SMPS" 
RTS_BEFORE_MIMO_STR             ="動的 SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="SMPS なし" 

SOURCEDISK1                     ="Intel(R) Wireless インストール・ディスク"

[Strings.0412] ; Korean (Korea)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Windows 10 64비트용 Intel(R) Wireless 어댑터 드라이버"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="전송 전원"
ROAMING_AGGRESSIVENESS_STR	="로밍의 주동성"
MIXED_MODE_PROTECTION_STR   	="혼합 모드 보호"
WIRELESS_MODE_STR           	="802.11a/b/g 무선 모드"
WIRELESS_MODE_A                 ="5GHz 802.11a"
WIRELESS_MODE_B                 ="2.4GHz 802.11b"
WIRELESS_MODE_G                 ="2.4GHz 802.11g"
WIRELESS_MODE_BG                ="2.4GHz 802.11b/g"
WIRELESS_MODE_AG                ="듀얼 밴드 802.11a/g"
WIRELESS_MODE_ABG               ="듀얼 밴드 802.11a/b/g"
PREFERRED_BAND_STR          	="기본 설정 밴드"
CHANNELWIDTH52              	="5GHz 채널 폭"
CHANNELWIDTH24              	="2.4GHz 채널 폭"
TGnMode                     	="802.11n/ac 무선 모드"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="과부하 채널 비지원"
LOWEST_STR			="최하"
MEDIUM_LOW_STR			="보통-낮음"
MEDIUM_STR			="보통"
MEDIUM_HIGH_STR			="보통-높음"
HIGHEST_STR			="최고"
DISABLED_STR			="비활성화함"
ENABLED_STR 			="활성화함"
CTS_TO_SELF_ENABLED_STR     	="자체 CTS 활성화함"
RTS_CTS_ENABLED_STR         	="RTS/CTS 활성화함"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="자동"
NO_PREFERECE_STR            	="기본 설정 없음"
PREFER_24_BAND_STR          	="2.4 GHz 밴드 선택"
PREFER_52_BAND_STR          	="5GHz 밴드 기본 설정"
WAKE_ON_MAGIC_PACKET        	="Wake on 매직 패킷"
WAKE_ON_PATTERN_MATCH       	="Wake on 패턴 일치"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN에 대한 GTK 키 재입력"
PM_ARP_OFFLOAD			="WoWLAN에 대한 ARP 오프로드"
PM_NS_OFFLOAD			="WoWLAN에 대한 NS 오프로드"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 연결 해제 시 절전 상태"
PACKET_COALESCING               ="패킷 통합"
U_APSD_SUPPORT			="U-APSD 지원"
THROUGHPUTBOOSTER_STR   	="처리량 부스터"
MIMO_POWER_SAVE_MODE_STR        ="MIMO 절전 모드" 
MIMO_AUTO_STR                   ="자동 SMPS" 
NO_MIMO_STR                     ="정적 SMPS" 
RTS_BEFORE_MIMO_STR             ="동적 SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="SMPS 안 함" 

SOURCEDISK1                     ="Intel(R) Wireless 시리즈 설치 디스크"

[Strings.0413] ; Dutch (Netherlands)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless adapter stuurprogramma onder Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Verzendenergie"
ROAMING_AGGRESSIVENESS_STR	="Agressiviteit bij roamen"
MIXED_MODE_PROTECTION_STR   	="Beveiliging van gemengde modus"
WIRELESS_MODE_STR           	="802.11a/b/g draadloze modus"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual-band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual-band 802.11a/b/g"
PREFERRED_BAND_STR          	="Voorkeursband"
CHANNELWIDTH52              	="Kanaalbreedte voor 5 GHz"
CHANNELWIDTH24              	="Kanaalbreedte voor 2,4 GHz"
TGnMode                     	="802.11n/ac draadloze modus"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Niet compatibel met 40-Mhz kanaal"
LOWEST_STR			="Laagste"
MEDIUM_LOW_STR			="Laag"
MEDIUM_STR			="Normaal"
MEDIUM_HIGH_STR			="Hoog"
HIGHEST_STR			="Hoogste"
DISABLED_STR			="Uitgeschakeld"
ENABLED_STR 			="Ingeschakeld"
CTS_TO_SELF_ENABLED_STR     	="CTS-naar-zelf ingeschakeld"
RTS_CTS_ENABLED_STR         	="RTS/CTS ingeschakeld"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisch"
NO_PREFERECE_STR            	="Geen voorkeur"
PREFER_24_BAND_STR          	="Voorkeur voor 2,4-GHz band"
PREFER_52_BAND_STR          	="5 GHz band"
WAKE_ON_MAGIC_PACKET        	="Activeren na Magic-pakket"
WAKE_ON_PATTERN_MATCH       	="patroonovereenkomst"
PM_WIFI_REKEY_OFFLOAD	    	="GTK opnieuw versleutelen voor WoWLAN"
PM_ARP_OFFLOAD			="ARP-offload voor WoWLAN"
PM_NS_OFFLOAD			="NS-offload voor WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slapen bij verbroken WoWLAN-verbinding"
PACKET_COALESCING               ="Pakketsamenvoeging"
U_APSD_SUPPORT			="U-APSD ondersteuning"
THROUGHPUTBOOSTER_STR   	="Throughput booster"
MIMO_POWER_SAVE_MODE_STR        ="MIMO energiebesparende stand" 
MIMO_AUTO_STR                   ="Automatische SMPS" 
NO_MIMO_STR                     ="Statische SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamische SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Geen SMPS" 

SOURCEDISK1                     ="Installatieschijf voor Intel(R) Wireless"

[Strings.0414] ; Norwegian Bokmål (Norway)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Intel(R) Wireless kortdriver for Windows 10 64-bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Overføringsstrøm"
ROAMING_AGGRESSIVENESS_STR	="Streifingsaggresjon"
MIXED_MODE_PROTECTION_STR   	="Blandet modus-beskyttelse"
WIRELESS_MODE_STR           	="802.11a/b/g trådløsmodus"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Tobånds 802.11a/g"
WIRELESS_MODE_ABG               ="Tobånds 802.11a/b/g"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="Kanalbredde for 5 GHz"
CHANNELWIDTH24              	="Kanalbredde for 2,4 GHz"
TGnMode                     	="802.11n/ac trådløsmodus"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Intolerant for kanal"
LOWEST_STR			="Laveste"
MEDIUM_LOW_STR			="Middels-lav"
MEDIUM_STR			="Middels"
MEDIUM_HIGH_STR			="Middels-høy"
HIGHEST_STR			="Høyeste"
DISABLED_STR			="Deaktivert"
ENABLED_STR 			="Aktivert"
CTS_TO_SELF_ENABLED_STR     	="CTS-til-selv aktivert"
RTS_CTS_ENABLED_STR         	="RTS/CTS-aktivert"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisk"
NO_PREFERECE_STR            	="Ingen preferanser"
PREFER_24_BAND_STR          	="Foretrekk 2,4 GHz-bånd"
PREFER_52_BAND_STR          	="Foretrekke 5 GHz-bånd"
WAKE_ON_MAGIC_PACKET        	="Reaktivert etter magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Reaktivert etter samsvarende mønster"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-omnøkling for WoWLAN"
PM_ARP_OFFLOAD			="ARP-avlastning for WoWLAN"
PM_NS_OFFLOAD			="NS-avlastning for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Hvilemodus ved WoWLAN-frakobling"
PACKET_COALESCING               ="Pakkeoppsamling"
U_APSD_SUPPORT			="Støtte for U-APSD:"
THROUGHPUTBOOSTER_STR   	="Gjennomstrømmings-Booster"
MIMO_POWER_SAVE_MODE_STR        ="MIMO-strømsparingsmodus" 
MIMO_AUTO_STR                   ="Auto-SMPS" 
NO_MIMO_STR                     ="Statisk SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamisk SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Ingen SMPS" 

SOURCEDISK1                     ="Installasjonsplate for Intel(R) Wireless"

[Strings.0415] ; Polish (Poland)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Sterownik karty Intel(R) Wireless dla systemu Windows 10 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Moc transmisji"
ROAMING_AGGRESSIVENESS_STR	="Agresywność mobilności"
MIXED_MODE_PROTECTION_STR   	="Ochrona trybu mieszanego"
WIRELESS_MODE_STR           	="Tryb bezprzewodowy 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Pasmo preferowane"
CHANNELWIDTH52              	="Szerokość kanału dla 5 GHz"
CHANNELWIDTH24              	="Szerokość kanału dla 2,4 GHz"
TGnMode                     	="Tryb bezprzewodowy 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Brak tolerancji dla kanału 40 MHz"
LOWEST_STR			="Najniższa"
MEDIUM_LOW_STR			="Średnio-niska"
MEDIUM_STR			="Średnia"
MEDIUM_HIGH_STR			="Średnio-wysoka"
HIGHEST_STR			="Najwyższa"
DISABLED_STR			="Wyłączono"
ENABLED_STR 			="Włączono"
CTS_TO_SELF_ENABLED_STR     	="Włączony zwrotny CTS"
RTS_CTS_ENABLED_STR         	="Włączony RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatyczny"
NO_PREFERECE_STR            	="Bez preferencji"
PREFER_24_BAND_STR          	="Preferowany pasmo 2,4 GHz"
PREFER_52_BAND_STR          	="Preferuj Pasmo 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Wznawianie na podstawie pakietu Magic"
WAKE_ON_PATTERN_MATCH       	="Wznawianie na podstawie dopasowania do wzorca"
PM_WIFI_REKEY_OFFLOAD	    	="GTK tworzy klucze ponowne dla WoWLAN"
PM_ARP_OFFLOAD			="Odciążanie ARP dla WoWLAN"
PM_NS_OFFLOAD			="Odciążanie NS dla WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Uśpienie WoWLAN Disconnect"
PACKET_COALESCING               ="Łączenie pakietów"
U_APSD_SUPPORT			="Obsługa funkcji U-APSD"
THROUGHPUTBOOSTER_STR   	="Przyśpieszacz przepustowości"
MIMO_POWER_SAVE_MODE_STR        ="Tryb oszczędzania energii MIMO" 
MIMO_AUTO_STR                   ="Automatyczna funkcja SMPS" 
NO_MIMO_STR                     ="Statyczna funkcja SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamiczna funkcja SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Brak funkcji SMPS" 

SOURCEDISK1                     ="Dysk instalacyjny Intel(R) Wireless"

[Strings.0416] ; Portuguese (Brazil)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Driver do adaptador Intel(R) Wireless para Windows 10 64 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade de roaming"
MIXED_MODE_PROTECTION_STR   	="Proteção de modo misto"
WIRELESS_MODE_STR           	="Modo sem fio 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Banda Dupla 802.11a/g"
WIRELESS_MODE_ABG               ="Banda Dupla 802.11a/b/g"
PREFERRED_BAND_STR          	="Banda preferencial"
CHANNELWIDTH52              	="Largura do canal para 5 GHz"
CHANNELWIDTH24              	="Largura do canal para 2,4 GHz"
TGnMode                     	="Modo sem fio 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Sem tolerância a canal FAT"
LOWEST_STR			="Mais baixo"
MEDIUM_LOW_STR			="Média a baixa"
MEDIUM_STR			="Média"
MEDIUM_HIGH_STR			="Média a alta"
HIGHEST_STR			="Mais alto"
DISABLED_STR			="Desabilitado"
ENABLED_STR 			="Habilitado"
CTS_TO_SELF_ENABLED_STR     	="CTS auto-ativação ativado"
RTS_CTS_ENABLED_STR         	="RTS/CTS ativado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Sem preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Pacote Mágico do Wake on"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Nova geração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarregamento ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarregamento NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender desconexão de WoWLAN"
PACKET_COALESCING               ="União de pacote"
U_APSD_SUPPORT			="Suporte para U-APSD"
THROUGHPUTBOOSTER_STR   	="Impulsionador do throughput"
MIMO_POWER_SAVE_MODE_STR        ="MIMO - Modo de Economia de Energia" 
MIMO_AUTO_STR                   ="SMPS automático" 
NO_MIMO_STR                     ="Estático SMPS" 
RTS_BEFORE_MIMO_STR             ="SMPS dinâmico" 
NO_RTS_BEFORE_MIMO_STR          ="Sem SMPS" 

SOURCEDISK1                     ="Disco da instalação do Intel(R) Wireless"

[Strings.0816] ; Portuguese (Portugal)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Controlador da placa Intel(R) Wireless para Windows 10 64 Bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade do roaming"
MIXED_MODE_PROTECTION_STR   	="Protecção do modo misto"
WIRELESS_MODE_STR           	="Modo sem fios 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Banda dupla de 802.11a/g"
WIRELESS_MODE_ABG               ="Banda dupla de 802.11a/b/g"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Largura do canal para 5 GHz"
CHANNELWIDTH24              	="Largura do canal para 2,4 GHz"
TGnMode                     	="Modo sem fios 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Canal de grandes volumes incompatível"
LOWEST_STR			="Menor"
MEDIUM_LOW_STR			="Média-baixa"
MEDIUM_STR			="Média"
MEDIUM_HIGH_STR			="Média-Elevada"
HIGHEST_STR			="Maior"
DISABLED_STR			="Desactivado"
ENABLED_STR 			="Activado"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS Activado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Sem Preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Reactivação por Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Regeração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender quando a WoWLAN estiver desligada"
PACKET_COALESCING               ="União de pacote"
U_APSD_SUPPORT			="Suporte de U-APSD"
THROUGHPUTBOOSTER_STR   	="Otimizador do rendimento"
MIMO_POWER_SAVE_MODE_STR        ="Modo de poupança de energia MIMO" 
MIMO_AUTO_STR                   ="SMPS automático" 
NO_MIMO_STR                     ="SMPS estático" 
RTS_BEFORE_MIMO_STR             ="SMPS dinâmico" 
NO_RTS_BEFORE_MIMO_STR          ="Sem SMPS" 

SOURCEDISK1                     ="Disco de Instalação da Intel(R) Wireless"

[Strings.0419] ; Russian (Russia)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Драйвер адаптера Intel(R) Wireless для Windows 10 64 Bit "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Мощность передачи"
ROAMING_AGGRESSIVENESS_STR	="Агрессивность роуминга"
MIXED_MODE_PROTECTION_STR   	="Защита в смешанном режиме"
WIRELESS_MODE_STR           	="Режим беспроводной связи 802.11a/b/g"
WIRELESS_MODE_A                 ="5 ГГц 802.11a"
WIRELESS_MODE_B                 ="2,4 ГГц 802.11b"
WIRELESS_MODE_G                 ="2,4 ГГц 802.11g"
WIRELESS_MODE_BG                ="2,4 ГГц 802.11b/g"
WIRELESS_MODE_AG                ="Двухдиапазонная сеть 802.11a/g"
WIRELESS_MODE_ABG               ="Двухдиапазонная сеть 802.11a/b/g"
PREFERRED_BAND_STR          	="Предпочитаемая частота"
CHANNELWIDTH52              	="Ширина канала для 5 ГГц"
CHANNELWIDTH24              	="Ширина канала для 2,4 ГГц"
TGnMode                     	="Режим беспроводной связи 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Несовместимость с каналом"
LOWEST_STR			="Мин."
MEDIUM_LOW_STR			="Средн.-мин."
MEDIUM_STR			="Средн."
MEDIUM_HIGH_STR			="Средн.-макс."
HIGHEST_STR			="Макс."
DISABLED_STR			="Выключено"
ENABLED_STR 			="Включено"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self включено"
RTS_CTS_ENABLED_STR         	="RTS/CTS включено"
CHANNELWIDTH20ONLY          	="20 МГц"
CHANNELWIDTHAUTO            	="Авто"
NO_PREFERECE_STR            	="Нет предпочтений"
PREFER_24_BAND_STR          	="Предпочитать частоту 2,4 ГГц"
PREFER_52_BAND_STR          	="диапазон 5 ГГц предпочтительней."
WAKE_ON_MAGIC_PACKET        	="Пробуждение пакетом Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Пробуждение при соответствии шаблону"
PM_WIFI_REKEY_OFFLOAD	    	="Повторный ввод ключа GTK для режима пробуждения Wake on Wireless LAN"
PM_ARP_OFFLOAD			="Выгрузка ARP для режима пробуждения Wake on Wireless LAN"
PM_NS_OFFLOAD			="Выгрузка NS для режима пробуждения Wake on Wireless LAN"
DEVICE_SLEEP_ON_DISCONNECT	="Переход в состояние сна при отключении режима пробуждения Wake on Wireless LAN"
PACKET_COALESCING               ="Объединение пакетов"
U_APSD_SUPPORT			="Поддержка U-APSD"
THROUGHPUTBOOSTER_STR   	="Увеличение пропускной способности"
MIMO_POWER_SAVE_MODE_STR        ="Режим энергосбережения MIMO" 
MIMO_AUTO_STR                   ="Авто SMPS" 
NO_MIMO_STR                     ="Статический SMPS" 
RTS_BEFORE_MIMO_STR             ="Динамический SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Нет SMPS" 

SOURCEDISK1                     ="Установочный диск адаптера Intel(R) Wireless"

[Strings.041D] ; Swedish (Sweden)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Kortdrivrutin för Windows 10 64-bitars Intel(R) Wireless"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Överföringsenergi"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
MIXED_MODE_PROTECTION_STR   	="Skydd för blandat läge"
WIRELESS_MODE_STR           	="802.11a/b/g Trådlöst läge"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="Förvalt band"
CHANNELWIDTH52              	="Kanalbredd för 5 GHz"
CHANNELWIDTH24              	="Kanalbredd för 2,4 GHz"
TGnMode                     	="802.11n/ac Trådlöst läge"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Inkompatibel med 40 MHz-kanal"
LOWEST_STR			="Lägsta"
MEDIUM_LOW_STR			="Medel-låg"
MEDIUM_STR			="Medel"
MEDIUM_HIGH_STR			="Medel-hög"
HIGHEST_STR			="Högsta"
DISABLED_STR			="Inaktiverad"
ENABLED_STR 			="Aktiverad"
CTS_TO_SELF_ENABLED_STR     	="CTS-till-själv aktiverat"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiverat"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
NO_PREFERECE_STR            	="Ingen inställning"
PREFER_24_BAND_STR          	="Föredra 2,4 GHz-bandet"
PREFER_52_BAND_STR          	="Föredrar 5 GHz-bandet"
WAKE_ON_MAGIC_PACKET        	="Aktivera vid Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivering vid mönstermatchning"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nyckeluppdatering för WoWLAN"
PM_ARP_OFFLOAD			="ARP-avbelastning för WoWLAN"
PM_NS_OFFLOAD			="NS-avbelastning för WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Viloläge vid WoWLAN-frånkoppling"
PACKET_COALESCING               ="Paketsammanslagning"
U_APSD_SUPPORT			="Support för U-APSD"
THROUGHPUTBOOSTER_STR   	="Genomflödesbooster"
MIMO_POWER_SAVE_MODE_STR        ="MIMO - Energisparläge" 
MIMO_AUTO_STR                   ="Auto SMPS" 
NO_MIMO_STR                     ="Statisk SMPS" 
RTS_BEFORE_MIMO_STR             ="Dynamisk SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Ingen SMPS" 

SOURCEDISK1                     ="Installationsdisk Intel(R) Wireless"

[Strings.041E] ; Thai (Thailand)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="ไดรเวอร์อแด็ปเตอร์ Intel(R) Wireless สำหรับ Windows 10 64 บิต"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="การส่งผ่านพลังงาน"
ROAMING_AGGRESSIVENESS_STR	="ความแรงในการใช้งานข้ามเขต"
MIXED_MODE_PROTECTION_STR   	="การป้องกันโหมดผสม"
WIRELESS_MODE_STR           	="โหมดไร้สาย 802.11a/b/g"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2.4 GHz 802.11b"
WIRELESS_MODE_G                 ="2.4 GHz 802.11g"
WIRELESS_MODE_BG                ="2.4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Dual Band 802.11a/g"
WIRELESS_MODE_ABG               ="Dual Band 802.11a/b/g"
PREFERRED_BAND_STR          	="แบนด์ที่ต้องการ"
CHANNELWIDTH52              	="ความกว้างช่องสัญญาณสำหรับ 5GHz"
CHANNELWIDTH24              	="ความกว้างช่องสัญญาณสำหรับ 2.4GHz"
TGnMode                     	="โหมดไร้สาย 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="ไม่สามารถใช้กับแชนแนลขนาดใหญ่"
LOWEST_STR			="ต่ำสุด"
MEDIUM_LOW_STR			="ปานกลาง-ต่ำ"
MEDIUM_STR			="ปานกลาง"
MEDIUM_HIGH_STR			="ปานกลาง-สูง"
HIGHEST_STR			="สูงสุด"
DISABLED_STR			="ยกเลิกใช้งาน"
ENABLED_STR 			="เปิดการใช้งาน"
CTS_TO_SELF_ENABLED_STR     	="ใช้งาน CTS-to-self แล้ว"
RTS_CTS_ENABLED_STR         	="ใช้งาน RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="อัตโนมัติ"
NO_PREFERECE_STR            	="ไม่มีการกำหนด"
PREFER_24_BAND_STR          	="แบนด์ 2.4 GHz"
PREFER_52_BAND_STR          	="ชอบแบนด์ 5 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="GTK กำลังกำหนดคีย์ใหม่สำหรับ WoWLAN"
PM_ARP_OFFLOAD			="ARP ออฟโหลดสำหรับ WoWLAN"
PM_NS_OFFLOAD			="NS ออฟโหลดสำหรับ WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="ยกเลิกการเชื่อมต่อสลีปบน WoWLAN"
PACKET_COALESCING               ="การรวมแพคเก็ต"
U_APSD_SUPPORT			="การสนับสนุน U-APSD"
THROUGHPUTBOOSTER_STR   	="ตัวเพิ่มอัตรารับส่ง"
MIMO_POWER_SAVE_MODE_STR        ="โหมดประหยัดพลังงานMIMO" 
MIMO_AUTO_STR                   ="SMPSอัตโนมัติ" 
NO_MIMO_STR                     ="SMPSค่าคงที่" 
RTS_BEFORE_MIMO_STR             ="SMPSความเคลื่อนไหว" 
NO_RTS_BEFORE_MIMO_STR          ="ไม่มีSMPS" 

SOURCEDISK1                     ="ดิสก์ติดตั้ง Intel(R) Wireless"

[Strings.041F] ; Turkish (Turkey)
NIC_7265_2x2_AC       = "Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    = "Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    = "Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     = "Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       = "Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     = "Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Windows 10 64 Bit için Intel(R) Wireless Bağdaştırıcı Sürücüsü "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Yayın gücü"
ROAMING_AGGRESSIVENESS_STR	="Gezinme Zorlaması"
MIXED_MODE_PROTECTION_STR   	="Karışık mod koruması"
WIRELESS_MODE_STR           	="802.11a/b/g Kablosuz Ağ Modu"
WIRELESS_MODE_A                 ="5 GHz 802.11a"
WIRELESS_MODE_B                 ="2,4 GHz 802.11b"
WIRELESS_MODE_G                 ="2,4 GHz 802.11g"
WIRELESS_MODE_BG                ="2,4 GHz 802.11b/g"
WIRELESS_MODE_AG                ="Çift Bant 802.11a/g"
WIRELESS_MODE_ABG               ="Çift Bant 802.11a/b/g"
PREFERRED_BAND_STR          	="Yeğlenen Bant"
CHANNELWIDTH52              	="5 GHz İçin Kanal Genişliği"
CHANNELWIDTH24              	="2,4 GHz İçin Kanal Genişliği"
TGnMode                     	="802.11n/ac Kablosuz Ağ Modu"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Geniş Kanal için Uyumsuz"
LOWEST_STR			="En düşük"
MEDIUM_LOW_STR			="Düşük"
MEDIUM_STR			="Orta"
MEDIUM_HIGH_STR			="Yüksek"
HIGHEST_STR			="En yüksek"
DISABLED_STR			="Devre dışı"
ENABLED_STR 			="Etkin"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self etkin"
RTS_CTS_ENABLED_STR         	="RTS/CTS etkin"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Otomatik"
NO_PREFERECE_STR            	="Tercih yok"
PREFER_24_BAND_STR          	="2,4 GHz bant Tercih Et"
PREFER_52_BAND_STR          	="5 GHz bant Tercih Et"
WAKE_ON_MAGIC_PACKET        	="Sihirli Paket Uyanması"
WAKE_ON_PATTERN_MATCH       	="Desen eşleştirme uyanması"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN için GTK yeniden anahtarlama"
PM_ARP_OFFLOAD			="WoWLAN için ARP yük boşaltma"
PM_NS_OFFLOAD			="WoWLAN için NS yük boşaltma"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN Bağlantı Kesintisinde uyku durumuna geç"
PACKET_COALESCING               ="Paket Birleştirme"
U_APSD_SUPPORT			="U-APSD Desteği"
THROUGHPUTBOOSTER_STR   	="Verimlilik Arttırıcı"
MIMO_POWER_SAVE_MODE_STR        ="MIMO Güç Tasarrufu Modu" 
MIMO_AUTO_STR                   ="Otomatik SMPS" 
NO_MIMO_STR                     ="Statik SMPS" 
RTS_BEFORE_MIMO_STR             ="Dinamik SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="SMPS Yok" 

SOURCEDISK1                     ="Intel(R) Wireless Yükleme Diski"

[Strings.0422] ; Ukrainian (Ukraine)
NIC_7265_2x2_AC       ="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265_2x2_AGN      ="Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_BGN15    ="Intel(R) Wireless-N 7265"
NIC_7265_2x2_AGN15    ="Intel(R) Dual Band Wireless-N 7265"
NIC_7265_2x2_AC15     ="Intel(R) Dual Band Wireless-AC 7265"

NIC_3168_1x1_AC       ="Intel(R) Dual Band Wireless-AC 3168"

NIC_3165_1x1_AC       ="Intel(R) Dual Band Wireless-AC 3165"
NIC_3165_1x1_AC15     ="Intel(R) Dual Band Wireless-AC 3165"

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_Service_DispName_WINT_64	     	="Драйвер адаптера бездротового зв’язку Intel(R) для ОС Windows 10 (64-розрядна версія)"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
IBSS_TX_POWER_STR           	="Потужність передачі сигналу"
ROAMING_AGGRESSIVENESS_STR	="Агресивність роумінгу"
MIXED_MODE_PROTECTION_STR   	="Захист у змішаному режимі"
WIRELESS_MODE_STR           	="Бездротовий режим 802.11a/b/g"
WIRELESS_MODE_A                 ="5 ГГц 802.11a"
WIRELESS_MODE_B                 ="2,4 ГГц 802.11b"
WIRELESS_MODE_G                 ="2,4 ГГц 802.11g"
WIRELESS_MODE_BG                ="2,4 ГГц 802.11b/g"
WIRELESS_MODE_AG                ="Дводіапазонний зв’язок 802.11a/g"
WIRELESS_MODE_ABG               ="Дводіапазонний зв’язок 802.11a/b/g"
PREFERRED_BAND_STR          	="Бажаний діапазон"
CHANNELWIDTH52              	="Ширина каналу для 5 ГГц"
CHANNELWIDTH24              	="Ширина каналу для 2,4 ГГц"
TGnMode                     	="Бездротовий режим 802.11n/ac"
VHT_ENABLED_STR			="802.11ac"
HT_ENABLED_STR			="802.11n"
FAT_CHANNEL_TOLERANT		="Без переваги широкого каналу"
LOWEST_STR			="Найнижч."
MEDIUM_LOW_STR			="Середньо-низьк."
MEDIUM_STR			="Середн."
MEDIUM_HIGH_STR			="Середньо-висок."
HIGHEST_STR			="Найвищ."
DISABLED_STR			="Вимкнуто"
ENABLED_STR 			="Увімкнено"
CTS_TO_SELF_ENABLED_STR     	="Функцію CTS-to-self увімкнуто"
RTS_CTS_ENABLED_STR         	="Функцію RTS/CTS увімкнуто"
CHANNELWIDTH20ONLY          	="Тільки 20 МГц"
CHANNELWIDTHAUTO            	="Автоматично"
NO_PREFERECE_STR            	="Без пріоритету"
PREFER_24_BAND_STR          	="У пріоритеті діапазон 2,4 ГГц"
PREFER_52_BAND_STR          	="У пріоритеті діапазон 5 ГГц"
WAKE_ON_MAGIC_PACKET        	="Пробудження за сигналом з локальної мережі"
WAKE_ON_PATTERN_MATCH       	="Пробудження після отримання особливого шаблону"
PM_WIFI_REKEY_OFFLOAD	    	="Зміна ключа GTK для WoWLAN"
PM_ARP_OFFLOAD			="Вивантаження ARP для WoWLAN"
PM_NS_OFFLOAD			="Вивантаження NS для WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Перехід у режим сну у разі вимкнення WoWLAN"
PACKET_COALESCING               ="Об’єднання пакетів"
U_APSD_SUPPORT			="Підтримка U-APSD"
THROUGHPUTBOOSTER_STR   	="Підсилювач пропускної здатності"
MIMO_POWER_SAVE_MODE_STR        ="Режим збереження енергії MIMO" 
MIMO_AUTO_STR                   ="Автоматичний SMPS" 
NO_MIMO_STR                     ="Статичний SMPS" 
RTS_BEFORE_MIMO_STR             ="Динамічний SMPS" 
NO_RTS_BEFORE_MIMO_STR          ="Без SMPS" 

SOURCEDISK1                     ="Інсталяційний диск безпровідного адаптера Intel(R)"
