; ************************************************************
; ************************************************************
; **  Filename: GeminilakeSystemLPSS.inf                    **
; **  Abstract: Assigns the null driver to devices          **
; **            for yellow-bang removal and                 **
; **            brands Intel(R) devices                     ** 
; ************************************************************
; ************************************************************

[Version]
Signature=$WINDOWS NT$
Class=System
ClassGUID={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
CatalogFile=Geminilake.cat
DriverVer=07/18/1968, 10.1.13.4
PnpLockDown=1

[SourceDisksNames]

[SourceDisksFiles]

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL,NTx86,NTamd64

[INTEL.NTx86]
%ACPI\INT3196Desc%=Needs_NO_DRV,ACPI\INT3196
%PCI\VEN_8086&DEV_31ACDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31AC
%PCI\VEN_8086&DEV_31AEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31AE
%PCI\VEN_8086&DEV_31B0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B0
%PCI\VEN_8086&DEV_31B2Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B2
%PCI\VEN_8086&DEV_31B4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B4
%PCI\VEN_8086&DEV_31B6Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B6
%PCI\VEN_8086&DEV_31B8Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B8
%PCI\VEN_8086&DEV_31BADesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BA
%PCI\VEN_8086&DEV_31BCDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BC
%PCI\VEN_8086&DEV_31BEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BE
%PCI\VEN_8086&DEV_31C0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C0
%PCI\VEN_8086&DEV_31C2Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C2
%PCI\VEN_8086&DEV_31C4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C4
%PCI\VEN_8086&DEV_31C6Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C6
%PCI\VEN_8086&DEV_31EEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31EE

[INTEL.NTamd64]
%ACPI\INT3196Desc%=Needs_NO_DRV,ACPI\INT3196
%PCI\VEN_8086&DEV_31ACDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31AC
%PCI\VEN_8086&DEV_31AEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31AE
%PCI\VEN_8086&DEV_31B0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B0
%PCI\VEN_8086&DEV_31B2Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B2
%PCI\VEN_8086&DEV_31B4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B4
%PCI\VEN_8086&DEV_31B6Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B6
%PCI\VEN_8086&DEV_31B8Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31B8
%PCI\VEN_8086&DEV_31BADesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BA
%PCI\VEN_8086&DEV_31BCDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BC
%PCI\VEN_8086&DEV_31BEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31BE
%PCI\VEN_8086&DEV_31C0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C0
%PCI\VEN_8086&DEV_31C2Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C2
%PCI\VEN_8086&DEV_31C4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C4
%PCI\VEN_8086&DEV_31C6Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31C6
%PCI\VEN_8086&DEV_31EEDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_31EE

[Needs_NO_DRV]
Include=machine.inf
Needs=NO_DRV

[Needs_NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[Strings]
INTEL="INTEL"
ACPI\INT3196Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor SPI - 3196"
PCI\VEN_8086&DEV_31ACDesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 0 - 31AC"
PCI\VEN_8086&DEV_31AEDesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 1 - 31AE"
PCI\VEN_8086&DEV_31B0Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 2 - 31B0"
PCI\VEN_8086&DEV_31B2Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 3 - 31B2"
PCI\VEN_8086&DEV_31B4Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 4 - 31B4"
PCI\VEN_8086&DEV_31B6Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 5 - 31B6"
PCI\VEN_8086&DEV_31B8Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 6 - 31B8"
PCI\VEN_8086&DEV_31BADesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor I2C 7 - 31BA"
PCI\VEN_8086&DEV_31BCDesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor UART 0 - 31BC"
PCI\VEN_8086&DEV_31BEDesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor UART 1 - 31BE"
PCI\VEN_8086&DEV_31C0Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor UART 2 - 31C0"
PCI\VEN_8086&DEV_31C2Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor SPI 0 - 31C2"
PCI\VEN_8086&DEV_31C4Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor SPI 1 - 31C4"
PCI\VEN_8086&DEV_31C6Desc="Intel(R) Celeron(R)/Pentium(R) Silver Processor SPI 2 - 31C6"
PCI\VEN_8086&DEV_31EEDesc="Intel(R) Celeron(R)/Pentium(R) Silver Processor UART 3 - 31EE"




; Copyright (c) 2003-2019 Intel Corporation
; 
; ********************************************************************************
; Intel is making no claims of usability, efficacy or warranty.
; ********************************************************************************
; Information in this document is provided in connection with Intel products. No
; license, express or implied, by estoppel or otherwise, to any intellectual
; property rights is granted by this document. Intel assumes no liability
; whatsoever, and Intel disclaims any express or implied warranty, relating to
; sale and/or use of Intel products including liability or warranties relating to
; fitness for a particular purpose, merchantability, or infringement of any
; patent, copyright or other intellectual property right. Intel products are not
; intended for use in medical, life saving, or life sustaining applications.
; ********************************************************************************
; Intel Corporation disclaims all warranties and liabilities for the use of this
; document and the information contained herein, and assumes no responsibility for
; any errors which may appear in this document, nor does Intel make a commitment
; to update the information contained herein. Intel reserves the right to make
; changes to this document at any time, without notice.
; ********************************************************************************
; ********************************************************************************
; 
; * Third-party brands and names are the property of their respective owners.
