SUMMARY: NESTED | FIELD | | METHOD
DETAIL: FIELD | METHOD

## Class OOB_Service

Used in features: Intel(R) ME defined Classes

    CIM_ManagedElement
       CIM_ManagedSystemElement
          CIM_LogicalElement
             CIM_EnabledLogicalElement
                CIM_Service
                   OOB_Service

    class OOB_Service

extends CIM_Service

General Information:
A class for handling Intel(R) ME's OOB activation(aka Intel(R) AMT provisioning) and forreporting the OOB configuration
Qualifiers:
-------------
Version=0.0.4
LOCALE=0x409
dynamic
provider=IntelMEProv

Supported Fields Summary
`string` | `Name` The Name property uniquely identifies the Service and provides an indication of the functionality that is managed . . .
`string` | `CreationClassName` CreationClassName indicates the name of the class or the subclass that is used in the creation of an instance . . .
`string` | `SystemName` The Name of the scoping System.
`string` | `SystemCreationClassName` The CreationClassName of the scoping System.

Methods Summary
`uint32` | `GetAMTProvisioningMode(mode)` Returns the current provisioning (activation) mode of the device
`uint32` | `isRemoteConfigEnabled(enabled)` Indicates if Remote Configuration is enabled in the MEBx
`uint32` | `GetActivationTLSMode(mode)` Indicates whether the device is using TLS-PSK or TLS-PKI activation mode
`uint32` | `GetPID(PID)` When the device is configured in TLS-PSK mode, this functions returns the PID value of the device, this can be used by Provisioning servers to associate a PSK value
`uint32` | `GetHelloPacketDestInfo(Address, ConfigServerListeningPort)` Returns the information about the server which Intel(R) AMT will send Hello packets to . . .
`uint32` | `GetAMTFQDN(FQDN)` Intel(R) AMT's configured Fully Qualified Domain Name
`uint32` | `Activate(OTP, PKIDNSSuffix, provTLSMode)` Activate Intel(R) AMT using Remote Configuration
`uint32` | `CancelActivation()` Stops Intel(R) AMT Activation if it is currently enabled, this will prevent Intel(R) AMT from being present on the Network for Bare-Metal activation
`uint32` | `GetProvisioningState(state)` GetProvisioningState
`uint32` | `GetProvisioningInfo(PKIDNSSuffix, ConfigServerFQDN)` GetProvisioningInfo returns the FQDN of configuration server and the PKI FQDN suffix
`uint32` | `isTLSEnabled(enabled)` Specifies whether Intel(R) AMT TLS port is enabled
`uint32` | `OpenUserInitiatedConnection()` CIRA: User request to initiate a CIRA connection
`uint32` | `CloseUserInitiatedConnection()` CIRA: Request Intel(R) ME to close an existing CIRA connection
`uint32` | `GetRemoteAccessConnectionStatus(NetworkConStatus, ConnectionTrigger, MPshostName, RemoteAccessConStatus)` CIRA: Retrieves information of an active CIRA connection
`uint32` | `GetLocalAdminCredentials(Username, Password)` Get the AMT local Administrator credentials . . .
`` | `Get(Instance)` Gets the representation of the instance
`` | `Enumerate()` Enumerates the instances of this class
`uint32` | `Unconfigure()` Un-configure the AMT system . . .

Field Detail

### Name

    public string Name

  General Information:
  The Name property uniquely identifies the Service and provides an indication of the functionality that is managed. This functionality is described in more detail in the Description property of the object.
  Qualifiers:
  -------------
  Key
  Override=Name
  MaxLen=256

### CreationClassName

    public string CreationClassName

  General Information:
  CreationClassName indicates the name of the class or the subclass that is used in the creation of an instance. When used with the other key properties of this class, this property allows all instances of this class and its subclasses to be uniquely identified.
  Qualifiers:
  -------------
  Key
  MaxLen=256

### SystemName

    public string SystemName

  General Information:
  The Name of the scoping System.
  Qualifiers:
  -------------
  Key
  MaxLen=256
  Propagated=CIM_System.Name

### SystemCreationClassName

    public string SystemCreationClassName

  General Information:
  The CreationClassName of the scoping System.
  Qualifiers:
  -------------
  Key
  MaxLen=256
  Propagated=CIM_System.CreationClassName

Method Detail

### GetAMTProvisioningMode

    public uint32 GetAMTProvisioningMode([OUT]uint8 mode)

  Permission Information:
  No permissions defined
  General Information:
  Returns the current provisioning (activation) mode of the device
  Qualifiers:
  -------------
  InternalOnly=Check Intel(R) AMT 6.0 support
  static
  implemented
  Parameters:
  --------------
  mode
    General Information:
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2, 3}
    Values={None, Enterprise, Small-Business, Remote Connectivity_Service}

### isRemoteConfigEnabled

    public uint32 isRemoteConfigEnabled([OUT]boolean enabled)

  Permission Information:
  No permissions defined
  General Information:
  Indicates if Remote Configuration is enabled in the MEBx
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  enabled
    General Information:
    Qualifiers:
    -------------
    OUT

### GetActivationTLSMode

    public uint32 GetActivationTLSMode([OUT]uint8 mode)

  Permission Information:
  No permissions defined
  General Information:
  Indicates whether the device is using TLS-PSK or TLS-PKI activation mode
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  mode
    General Information:
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2}
    Values={NOT READY, PSK, PKI}

### GetPID

    public uint32 GetPID([OUT]string PID)

  Permission Information:
  No permissions defined
  General Information:
  When the device is configured in TLS-PSK mode, this functions returns the PID value of the device, this can be used by Provisioning servers to associate a PSK value
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  PID
    General Information:
    Qualifiers:
    -------------
    OUT

### GetHelloPacketDestInfo

    public uint32 GetHelloPacketDestInfo([OUT]string Address, [OUT]uint16 ConfigServerListeningPort)

  Permission Information:
  No permissions defined
  General Information:
  Returns the information about the server which Intel(R) AMT will send Hello packets to. The OOB server (aka Intel(R) AMT) sends 'Hello packet' messages to this address as a mean to trigger remote configuration
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  Address
    General Information:
    returns the address information (IPv4, IPv6 or FQDN) of the configurationserver
    Qualifiers:
    -------------
    OUT
    InternalOnly=if not configured return 'provisionserver'
  ConfigServerListeningPort
    General Information:
    TCP Port of the configuration server to send Hello packets to
    Qualifiers:
    -------------
    OUT
    InternalOnly=if not configured return '9971'

### GetAMTFQDN

    public uint32 GetAMTFQDN([OUT]string FQDN)

  Permission Information:
  No permissions defined
  General Information:
  Intel(R) AMT's configured Fully Qualified Domain Name
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  FQDN
    General Information:
    Qualifiers:
    -------------
    OUT

### Activate

    public uint32 Activate([IN]string OTP, [IN]string PKIDNSSuffix, [OUT]uint8 provTLSMode)

  Permission Information:
  Permitted realms: Administrators
  General Information:
  Activate Intel(R) AMT using Remote Configuration
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  OTP
    General Information:
    Optional One-Time-Password value the remote configuration service can use to authenticate the device
    Qualifiers:
    -------------
    IN
  PKIDNSSuffix
    General Information:
    Optional DNSSuffix to match
    Qualifiers:
    -------------
    IN
  provTLSMode
    General Information:
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2}
    Values={NOT READY, PSK, PKI}

### CancelActivation

    public uint32 CancelActivation()

  Permission Information:
  Permitted realms: Administrators
  General Information:
  Stops Intel(R) AMT Activation if it is currently enabled, this will prevent Intel(R) AMT from being present on the Network for Bare-Metal activation
  Qualifiers:
  -------------
  static
  implemented

### GetProvisioningState

    public uint32 GetProvisioningState([OUT]uint8 state)

  Permission Information:
  No permissions defined
  General Information:
  GetProvisioningState
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  state
    General Information:
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2}
    Values={PRE-Provisioning, IN-Provisioning, POST-Provisioning}

### GetProvisioningInfo

    public uint32 GetProvisioningInfo([OUT]string PKIDNSSuffix, [OUT]string ConfigServerFQDN)

  Permission Information:
  No permissions defined
  General Information:
  GetProvisioningInfo returns the FQDN of configuration server and the PKI FQDN suffix
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  PKIDNSSuffix
    General Information:
    PKIDNSSuffix Specified
    Qualifiers:
    -------------
    OUT
  ConfigServerFQDN
    General Information:
    The ConfigurationServerFQDN, set to null if not specified
    Qualifiers:
    -------------
    OUT

### isTLSEnabled

    public uint32 isTLSEnabled([OUT]boolean enabled)

  Permission Information:
  No permissions defined
  General Information:
  Specifies whether Intel(R) AMT TLS port is enabled
  Qualifiers:
  -------------
  InternalOnly=consider modifying the API to specify all open ports
  static
  implemented
  Parameters:
  --------------
  enabled
    General Information:
    Qualifiers:
    -------------
    OUT

### OpenUserInitiatedConnection

    public uint32 OpenUserInitiatedConnection()

  Permission Information:
  No permissions defined
  General Information:
  CIRA: User request to initiate a CIRA connection
  Qualifiers:
  -------------
  static
  implemented

### CloseUserInitiatedConnection

    public uint32 CloseUserInitiatedConnection()

  Permission Information:
  No permissions defined
  General Information:
  CIRA: Request Intel(R) ME to close an existing CIRA connection
  Qualifiers:
  -------------
  static
  implemented

### GetRemoteAccessConnectionStatus

    public uint32 GetRemoteAccessConnectionStatus([OUT]uint32 NetworkConStatus, [OUT]uint32 ConnectionTrigger, [OUT]string MPshostName, [OUT]uint32 RemoteAccessConStatus)

  Permission Information:
  No permissions defined
  General Information:
  CIRA: Retrieves information of an active CIRA connection
  Qualifiers:
  -------------
  static
  implemented
  Parameters:
  --------------
  NetworkConStatus
    General Information:
    Indicates the network connection status from Intel(R) AMT standpoint
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2, 3}
    Values={Direct, VPN, Outside Enterprise, Unknown}
  ConnectionTrigger
    General Information:
    Indicates the trigger for the remote access establishment in case a connection status is connected/connecting
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2, 3}
    Values={User Initiated, Alert, Periodic, Provisioning}
  MPshostName
    General Information:
    The MPS hostname that Intel(R) AMT is connected or trying to connect to
    Qualifiers:
    -------------
    OUT
  RemoteAccessConStatus
    General Information:
    the status of the connection (not connected, connecting, connected)
    Qualifiers:
    -------------
    OUT
    ValueMap={0, 1, 2}
    Values={not connected, connecting, connected}

### GetLocalAdminCredentials

    public uint32 GetLocalAdminCredentials([OUT]string Username, [OUT]string Password)

  Permission Information:
  Permitted realms: Administrators
  General Information:
  Get the AMT local Administrator credentials. A local application or a service running as a Windows local administrator, can use this method to retrieve credentials from AMT. This application can use these credentials to authenticate to AMT during WSMAN commands.
  Qualifiers:
  -------------
  Amended
  Static
  Implemented
  Parameters:
  --------------
  Username
    General Information:
    Qualifiers:
    -------------
    OUT
  Password
    General Information:
    Qualifiers:
    -------------
    OUT

### Get

    public  Get([OUT]OOB_Service Instance)

  Permission Information:
  No permissions defined
  General Information:
  Gets the representation of the instance

### Enumerate

    public  Enumerate()

  Permission Information:
  All users permitted to use method
  General Information:
  Enumerates the instances of this class

### Unconfigure

    public  Unconfigure()

  Permission Information:
  Permitted realms: Administrators
  General Information:
  Un-configure the AMT system

SUMMARY: NESTED | FIELD | METHOD
DETAIL: FIELD | METHOD