;;
;; Copyright 2014, Broadcom Corporation.
;; All Rights Reserved.
;;


[version]
Signature       = "$Windows NT$"                ; Combined win7/win8/win8.1/win10
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_BCM%

DriverVer=07/30/2015, 1.480.0.0
CatalogFile     = bcmpciedhd63.cat

[Manufacturer]
	%V_BCM% = BROADCOM, NTamd64.6.2

[ControlFlags]
	ExcludeFromSelect = *

;	Display Name		Section			DeviceID
;	------------		-------			--------

;-----------------------------------------------------------------
; x86, x64 (AMD64, Intel EM64T)
;

[BROADCOM.NTamd64.6.2]
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4350, PCI\VEN_14E4&DEV_43A3
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4356, PCI\VEN_14E4&DEV_43EC
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4371, PCI\VEN_14E4&DEV_440D
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_43570, PCI\VEN_14E4&DEV_AA31
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_43602, PCI\VEN_14E4&DEV_43BA
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4359, PCI\VEN_14E4&DEV_43EF
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4364, PCI\VEN_14E4&DEV_4364
	%BCM43XXPCIE_DeviceDesc% = BCM43XAC_NT62_4366, PCI\VEN_14E4&DEV_43C3


[BCM43XAC_NT62_4350]
	Include         = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_4350.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4356]
	Include		= netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_4356.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4371]
	Include		= netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_4371.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_43570]
	Include = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_43570.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_43602]
	Include         = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_43602.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4359]
	Include         = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_4359.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4364]
	Include         = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.enabled.reg, wowl.std_keywords.reg, cs.std_keywords.reg
	CopyFiles       = BCM43XAC_NT62_4364.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4366]
	Include         = netvwifibus.inf
	Needs           = VWiFiBus.CopyFiles
	*IfType         = 71    ; IF_TYPE_IEEE80211
	*MediaType      = 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
	BusType         = 5	; PCI bus
 	AddReg          = BCM43XX_NT.reg, BCMPCIE43XX.brcm.reg, common.reg, gn.options.reg, BCMIHV.reg, wowl.capabilities.disabled.reg 
	CopyFiles       = BCM43XAC_NT62_4366.files, BCMIHV.files
	RegisterDlls    = BCMIHVUI.regsrv

[BCM43XAC_NT62_4350.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4350.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg


[BCM43XAC_NT62_4356.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4356.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XAC_NT62_4371.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4371.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XAC_NT62_43570.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_43570.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg


[BCM43XAC_NT62_43602.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_43602.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XAC_NT62_4359.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4359.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XAC_NT62_4364.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4364.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XAC_NT62_4366.Services]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.Services
	AddService = BCMPCIEDHD63, 2, BCMPCIE43XX_NT62.Service, common.EventLog

[BCM43XAC_NT62_4366.HW]
	Include = netvwifibus.inf
	Needs   = VWiFiBus.PnPFilterRegistration
	AddReg  = MSI.reg

[BCM43XX_NT.reg]
	; Ndis Info
	; Interfaces
	HKR,    Ndi\Interfaces, UpperRange,     ,       "ndis5"
	HKR,    Ndi\Interfaces, LowerRange,     ,       "ethernet,wlan,vwifi"

[BCMPCIE43XX.brcm.reg]
	HKR,    Ndi,    HelpText,               ,       %BCM43XX_HELP%
	HKR,    Ndi,    Service,                0,      "BCMPCIEDHD63"

[common.EventLog]
	AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
	HKR,    ,       EventMessageFile,       0x00020000,     "%%SystemRoot%%\System32\netevent.dll"
	HKR,    ,       TypesSupported,         0x00010001,     7

[BCMPCIE43XX_NT62.Service]
	DisplayName     = %BCM43XXPCIE_Service_DispName%
	ServiceType     = 1                     ; %SERVICE_KERNEL_DRIVER%
	StartType       = 3                     ; %SERVICE_DEMAND_START%
	ErrorControl    = 1                     ; %SERVICE_ERROR_NORMAL%
	ServiceBinary   = %12%\bcmpciedhd63.sys
	LoadOrderGroup  = NDIS

[BCM43XAC_NT62_4350.files]
	bcmpciedhd63.sys,,,6
	4350r8rtecdc.bin,4350c5rtecdc.bin,,6

[BCM43XAC_NT62_4356.files]
	bcmpciedhd63.sys,,,6
	4356r2rtecdc.bin,4356a2rtecdc.bin,,6

[BCM43XAC_NT62_4371.files]
	bcmpciedhd63.sys,,,6
	4371r2rtecdc.bin,4371c2rtecdc.bin,,6

[BCM43XAC_NT62_43570.files]
	bcmpciedhd63.sys,,,6
	43570r2rtecdc.bin,43570a2rtecdc.bin,,6
	43570r2nvram.txt,bcm943570pcieir_p156.txt,,6

[BCM43XAC_NT62_43602.files]
	bcmpciedhd63.sys,,,6
	43602r1rtecdc.bin,43602a1rtecdc.bin,,6

[BCM43XAC_NT62_4359.files]
	bcmpciedhd63.sys,,,6
	4359r5rtecdc.bin,4359b1rtecdc.bin,,6
	4359r5nvram.txt,bcm94359fcpagbss_2.txt,,6

[BCM43XAC_NT62_4364.files]
	bcmpciedhd63.sys,,,6
	4364r0rtecdc.bin,4364a0rtecdc.bin,,6
	4364r0nvram.txt,bcm94364fcpagb.txt,,6

[BCM43XAC_NT62_4366.files]
	bcmpciedhd63.sys,,,6
	4365r3rtecdc.bin,4365b1rtecdc.bin,,6

; 11 == %windir%/system32
; 12 == %windir%/system32/drivers

[BCMIHV.files]
	bcmihvsrv64.dll,,,6
	bcmihvui64.dll,,,6
;
; IHV UI registration
;
[BCMIHVUI.regsrv]
	11,,bcmihvui64.dll,1

[DestinationDirs]
	DefaultDestDir					= 11
	BCM43XAC_NT62_4350.files		= 12
	BCM43XAC_NT62_4356.files		= 12
	BCM43XAC_NT62_4371.files		= 12
	BCM43XAC_NT62_43570.files		= 12
	BCM43XAC_NT62_43602.files		= 12
	BCM43XAC_NT62_4359.files		= 12
	BCM43XAC_NT62_4364.files		= 12
	BCM43XAC_NT62_4366.files		= 12
	BCMIHV.files					= 11

[SourceDisksNames]
	1=%BCM43XX_DiskName%,,

[SourceDisksFiles]
	bcmpciedhd63.sys=1
	bcmihvsrv64.dll=1
	bcmihvui64.dll=1
	4356a2rtecdc.bin=1
	4350c5rtecdc.bin=1
	4371c2rtecdc.bin=1
	43570a2rtecdc.bin=1
	bcm943570pcieir_p156.txt=1
	43602a1rtecdc.bin=1
	4359b1rtecdc.bin=1
	bcm94359fcpagbss_2.txt=1
	4364a0rtecdc.bin=1
	bcm94364fcpagb.txt=1
	4365b1rtecdc.bin=1

;Uninstall

[BCMIHV.reg]
	HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%%SystemRoot%%\System32\bcmihvsrv64.dll"
	HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{AAA6DEE9-31B9-4f18-AB39-82EF9B06EB73}"
	HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x001018

;Message Signalled Interrupt
[MSI.reg]
	HKR,Interrupt Management,,0x00000010
	HKR,Interrupt Management\MessageSignaledInterruptProperties,,0x00000010
	HKR,Interrupt Management\MessageSignaledInterruptProperties,MSISupported,0x00010001,1

;common for all platform
[common.reg]

	HKR,    Ndi\params\*PriorityVLANTag, ParamDesc, 0,      %PriorityVLANTag%
	HKR,    Ndi\params\*PriorityVLANTag, type,      0,      "enum"
	HKR,    Ndi\params\*PriorityVLANTag\enum, "0",  0,      %PriorityAndVLANDisabled%
	HKR,    Ndi\params\*PriorityVLANTag\enum, "1",  0,      %PriorityEnabled%
	HKR,    Ndi\params\*PriorityVLANTag\enum, "2",  0,      %VLANEnabled%
	HKR,    Ndi\params\*PriorityVLANTag\enum, "3",  0,      %PriorityAndVLANEnabled%
	HKR,    Ndi\params\*PriorityVLANTag,default,,"0"
	HKR,    Ndi\params\*PriorityVLANTag,optional,,"0"

	HKLM,system\CurrentControlSet\Services\NativeWiFiP\Parameters,EnableWoWLAN,0x00010001,1

	HKR,    Ndi\params\RoamDelta, ParamDesc,        0,      %RoamingTendency%
	HKR,    Ndi\params\RoamDelta, type,             0,      "enum"
	HKR,    Ndi\params\RoamDelta\enum, "0",         0,      %Aggressive%
	HKR,    Ndi\params\RoamDelta\enum, "1",         0,      %Moderate%
	HKR,    Ndi\params\RoamDelta\enum, "2",         0,      %Conservative%
	HKR,    Ndi\params\RoamDelta\enum, "3",         0,      %Auto%
	HKR,    Ndi\params\RoamDelta,default,,"3"

	HKR,    Ndi\params\MPC, ParamDesc,              0,      %MinimumPowerConsumption%
	HKR,    Ndi\params\MPC, type,                   0,      "enum"
	HKR,    Ndi\params\MPC\enum, "0",               0,      %Disabled%
	HKR,    Ndi\params\MPC\enum, "1",               0,      %Enabled%
	HKR,    Ndi\params\MPC,default,,"1"

	HKR,    Ndi\params\frag, ParamDesc,     0,      %FragmentationThreshold%
	HKR,    Ndi\params\frag,type,0,"dword"
	HKR,    Ndi\params\frag,min,,"256"
	HKR,    Ndi\params\frag,max,,"2346"
	HKR,    Ndi\params\frag,default,,"2346"

	HKR,    Ndi\params\rts, ParamDesc,      0,      %RTSThreshold%
	HKR,    Ndi\params\rts,type,0,"dword"
	HKR,    Ndi\params\rts,min,,"0"
	HKR,    Ndi\params\rts,max,,"2347"
	HKR,    Ndi\params\rts,default,,"2347"

	HKR,    Ndi\params\NetworkAddress, ParamDesc,   0, %LocallyAdministeredMACAddress%
	HKR,    Ndi\params\NetworkAddress, type,        0, "edit"
	HKR,    Ndi\params\NetworkAddress, LimitText,   0, "12"
	HKR,    Ndi\params\NetworkAddress, UpperCase,   0, "1"
	HKR,    Ndi\params\NetworkAddress, default,     0, ""
	HKR,    Ndi\params\NetworkAddress, optional,    0, "1"

	HKR,    Ndi\params\PwrOut, ParamDesc,   0,      %PowerOutput%
	HKR,    Ndi\params\PwrOut, type,                0,      "enum"
	HKR,    Ndi\params\PwrOut\enum, "100",  0,      "100%%"
	HKR,    Ndi\params\PwrOut\enum, "75",   0,      "75%%"
	HKR,    Ndi\params\PwrOut\enum, "50",   0,      "50%%"
	HKR,    Ndi\params\PwrOut\enum, "25",   0,      "25%%"
	HKR,    Ndi\params\PwrOut,default,,"100"

	HKR,    Ndi\params\FrameBursting, ParamDesc,    0,      %XPress_Technology%
	HKR,    Ndi\params\FrameBursting, type,         0,      "enum"
	HKR,    Ndi\params\FrameBursting\enum, "0",             0,      %Disabled%
	HKR,    Ndi\params\FrameBursting\enum, "1",             0,      %Enabled%
	HKR,    Ndi\params\FrameBursting,default,,"0"

	HKR,    Ndi\params\BTCoexist, ParamDesc,        0,      %BlueToothCollaboration%
	HKR,    Ndi\params\BTCoexist, type,             0,      "enum"
	HKR,    Ndi\params\BTCoexist\enum, "0", 0,      %Disable%
	HKR,    Ndi\params\BTCoexist\enum, "1", 0,      %Enable%
	HKR,    Ndi\params\BTCoexist\enum, "3", 0,      %Auto%
	HKR,    Ndi\params\BTCoexist,default,,"3"

	HKR,    Ndi\params\antdiv, ParamDesc,   0,      %AntennaDiversity%
	HKR,    Ndi\params\antdiv, type,        0,      "enum"
	HKR,    Ndi\params\antdiv\enum, "-1",   0,      %Auto%
	HKR,    Ndi\params\antdiv\enum, "0",    0,      %Main%
	HKR,    Ndi\params\antdiv\enum, "1",    0,      %Aux%
	HKR,    Ndi\params\antdiv,default,,"-1"

	HKR,    Ndi\params\WME, ParamDesc,      0,      %WME%
	HKR,    Ndi\params\WME, type,           0,      "enum"
	HKR,    Ndi\params\WME\enum, "-1",      0,      %Auto%
	HKR,    Ndi\params\WME\enum, "1",       0,      %Enabled%
	HKR,    Ndi\params\WME\enum, "0",       0,      %Disabled%
	HKR,    Ndi\params\WME,default,,"-1"

	HKR,    Ndi\params\ListenInterval, ParamDesc,     0,      %ListenInterval%
	HKR,    Ndi\params\ListenInterval,type,0,"dword"
	HKR,    Ndi\params\ListenInterval,min,,"1"
	HKR,    Ndi\params\ListenInterval,max,,"100"
	HKR,    Ndi\params\ListenInterval,default,,"1"

	HKR,    Ndi\params\D2ListenInterval, ParamDesc,     0,      %D2ListenInterval%
	HKR,    Ndi\params\D2ListenInterval,type,0,"dword"
	HKR,    Ndi\params\D2ListenInterval,min,,"1"
	HKR,    Ndi\params\D2ListenInterval,max,,"100"
	HKR,    Ndi\params\D2ListenInterval,default,,"5"

	HKR,    Ndi\params\WFDChannelNumber, ParamDesc,     0,      %WFDChannelNumber%
	HKR,    Ndi\params\WFDChannelNumber,type,0,"dword"
	HKR,    Ndi\params\WFDChannelNumber,min,,"1"
	HKR,    Ndi\params\WFDChannelNumber,max,,"11"
	HKR,    Ndi\params\WFDChannelNumber,default,,"11"

	HKR,    Ndi\params\EnableLTR, ParamDesc,0, %EnableLTR%
	HKR,    Ndi\params\EnableLTR, type,     0,         "enum"
	HKR,    Ndi\params\EnableLTR\enum, "0", 0, %Disabled%
	HKR,    Ndi\params\EnableLTR\enum, "1", 0, %Enabled%
	HKR,    Ndi\params\EnableLTR,default,,"1"

	HKR,    Ndi\params\LTR_ActiveValue, ParamDesc,     0,      %LTR_ActiveValue%
	HKR,    Ndi\params\LTR_ActiveValue,type,0,"dword"
	HKR,    Ndi\params\LTR_ActiveValue,min,,"0"
	HKR,    Ndi\params\LTR_ActiveValue,max,,"1023"
	HKR,    Ndi\params\LTR_ActiveValue,default,,"60"

	HKR,                                    ,"mchan_algo_wfd",                0,      "1"
	HKR,                                    ,"mchan_bw_wfd",                0,      "40"

	HKR, Ndi\params\BWCap2G, ParamDesc, 0, %BandwidthCapability2G%
	HKR, Ndi\params\BWCap2G, type, 0, "enum"
	HKR, Ndi\params\BWCap2G\enum, "0", 0, "2.4G: 20MHz"
	HKR, Ndi\params\BWCap2G\enum, "1", 0, "2.4G: 20/40MHz"
	HKR, Ndi\params\BWCap2G,default,,"0"

	HKR, Ndi\params\autoCountryDiscovery, ParamDesc, 0, %autoCountryDiscovery%
	HKR, Ndi\params\autoCountryDiscovery, type, 0, "enum"
	HKR, Ndi\params\autoCountryDiscovery\enum, "0", 0, "Disabled"
	HKR, Ndi\params\autoCountryDiscovery\enum, "1", 0, "Enabled"
	HKR, Ndi\params\autoCountryDiscovery,default,,"0"

[gn.options.reg]
	HKR,    Ndi\params\RoamTrigger, ParamDesc,      0,      %RoamingDecision%
	HKR,    Ndi\params\RoamTrigger, type,           0,      "enum"
	HKR,    Ndi\params\RoamTrigger\enum, "3",       0,      %Auto%
	HKR,    Ndi\params\RoamTrigger\enum, "1",       0,      %OptimizeBandwidth%
	HKR,    Ndi\params\RoamTrigger\enum, "0",       0,      %Default%
	HKR,    Ndi\params\RoamTrigger\enum, "2",       0,      %OptimizeDistance%
	HKR,    Ndi\params\RoamTrigger,default,,"3"

	HKR,    Ndi\params\PLCPHeader, ParamDesc,       0,      %BSSPLCPHeader%
	HKR,    Ndi\params\PLCPHeader, type,            0,      "enum"
	HKR,    Ndi\params\PLCPHeader\enum, "-1",       0,      %Long%
	HKR,    Ndi\params\PLCPHeader\enum, "0",        0,      %AutoShortLong%
	HKR,    Ndi\params\PLCPHeader,default,,"0"

	HKR,    Ndi\params\Intolerant, ParamDesc,       0,      %Intolerant%
	HKR,    Ndi\params\Intolerant, type,         0,      "enum"
	HKR,    Ndi\params\Intolerant\enum, "0",     0,      %Disabled%
	HKR,    Ndi\params\Intolerant\enum, "1",     0,      %Enabled%
	HKR,    Ndi\params\Intolerant,default,,"0"

	HKR,    Ndi\params\OBSSCoex, ParamDesc, 0,      %OBSSCoex%
	HKR,    Ndi\params\OBSSCoex, type,      0,      "enum"
	HKR,    Ndi\params\OBSSCoex\enum, "0",  0,      %Disabled%
	HKR,    Ndi\params\OBSSCoex\enum, "1",  0,      %Enabled%
	HKR,    Ndi\params\OBSSCoex\enum, "-1", 0,      %Auto%
	HKR,    Ndi\params\OBSSCoex,default,,"-1"

	; option to override antenna selection, -1: no override, 0: no selection
	HKR,                                    ,"mimo_antsel", 0,      "-1"

[wowl.capabilities.enabled.reg]
        HKR,,   "WakeUpCapabilities", 0x00010001, "0xffffffff"

[wowl.capabilities.disabled.reg]
        HKR,,   "WakeUpCapabilities", 0x00010001, "0x00000000"

[wowl.std_keywords.reg]
        HKR, Ndi\params\*WakeOnMagicPacket, ParamDesc,  0, %WakeOnMagicPacket%
        HKR, Ndi\params\*WakeOnMagicPacket, type,       0, "enum"
        HKR, Ndi\params\*WakeOnMagicPacket\enum,        "0", 0, %Disabled%
        HKR, Ndi\params\*WakeOnMagicPacket\enum,        "1", 0, %Enabled%
        HKR, Ndi\params\*WakeOnMagicPacket,default,,    "1"
        HKR, Ndi\params\*WakeOnMagicPacket,optional,,   "0"

        HKR, Ndi\params\*WakeOnPattern, ParamDesc,      0, %WakeOnPatternMatch%
        HKR, Ndi\params\*WakeOnPattern, type,           0, "enum"
        HKR, Ndi\params\*WakeOnPattern\enum,            "0", 0, %Disabled%
        HKR, Ndi\params\*WakeOnPattern\enum,            "1", 0, %Enabled%
        HKR, Ndi\params\*WakeOnPattern,default,,        "1"
        HKR, Ndi\params\*WakeOnPattern,optional,,       "0"

        HKR, Ndi\params\*PMARPOffload, ParamDesc,       0, %ARPOffload%
        HKR, Ndi\params\*PMARPOffload, type,            0, "enum"
        HKR, Ndi\params\*PMARPOffload\enum,             "0", 0, %Disabled%
        HKR, Ndi\params\*PMARPOffload\enum,             "1", 0, %Enabled%
        HKR, Ndi\params\*PMARPOffload,default,,         "1"
        HKR, Ndi\params\*PMARPOffload,optional,,        "0"

        HKR, Ndi\params\*PMNSOffload, ParamDesc,        0, %NSOffload%
        HKR, Ndi\params\*PMNSOffload, type,             0, "enum"
        HKR, Ndi\params\*PMNSOffload\enum,              "0", 0, %Disabled%
        HKR, Ndi\params\*PMNSOffload\enum,              "1", 0, %Enabled%
        HKR, Ndi\params\*PMNSOffload,default,,          "1"
        HKR, Ndi\params\*PMNSOffload,optional,,         "0"

        HKR, Ndi\params\*PMWiFiRekeyOffload, ParamDesc, 0, %WiFiRekeyingOffload%
        HKR, Ndi\params\*PMWiFiRekeyOffload, type,      0, "enum"
        HKR, Ndi\params\*PMWiFiRekeyOffload\enum,       "0", 0, %Disabled%
        HKR, Ndi\params\*PMWiFiRekeyOffload\enum,       "1", 0, %Enabled%
        HKR, Ndi\params\*PMWiFiRekeyOffload,default,,   "1"
        HKR, Ndi\params\*PMWiFiRekeyOffload,optional,,  "0"

[cs.std_keywords.reg]
        HKR, Ndi\Params\*PacketCoalescing,  ParamDesc,  0, %PacketCoalescing%
        HKR, Ndi\params\*PacketCoalescing, type,      0, "enum"
        HKR, Ndi\params\*PacketCoalescing\enum,       "0", 0, %Disabled%
        HKR, Ndi\params\*PacketCoalescing\enum,       "1", 0, %Enabled%
        HKR, Ndi\params\*PacketCoalescing,default,,   "1"
        HKR, Ndi\params\*PacketCoalescing,optional,,  "0"

[strings]
	V_BCM="Broadcom"
	BCM43XX_HELP="The Broadcom 802.11 Network Adapter provides wireless local area networking."
	BCM43XX_Service_DispName="Broadcom 802.11 Network Adapter Driver"
	BCM43XX_DiskName="802.11 Network Adapter Install Disk"
	BCM43XXPCIE_DeviceDesc="Broadcom 802.11ac Wireless PCIE Full Dongle Adapter"
	BCM43XXPCIE_Service_DispName="Broadcom 802.11 PCIE Network Adapter Driver"

	54gAuto="54g - Auto"
	54gPerformance="54g - Performance"
	80211bOnly="802.11b Only"
	AntennaDiversity="Antenna Diversity"
	Auto="Auto"
	AutoShortLong="Auto (Short/Long)"
	BSSPLCPHeader="BSS PLCP Header"
	BlueToothCollaboration="Bluetooth Collaboration"
	Default="Default"
	Disable="Disable"
	Disable80211a="Disable 802.11a"
	Disable80211gb="Disable 802.11g/b"
	DisableBands="Disable Bands"
	Disabled="Disabled"
	Enable="Enable"
	Enabled="Enabled"
	FragmentationThreshold="Fragmentation Threshold"
	LocallyAdministeredMACAddress="Locally Administered MAC Address"
	Long="Long"
	None="None"
	OptimizeBandwidth="Optimize Bandwidth"
	OptimizeDistance="Optimize Distance"
	PLCPHeader="PLCP Header"
	PowerOutput="Power Output"
	PowerSaveMode="Power Save Mode"
	Prefer80211a="Prefer 802.11a"
	Prefer80211gb="Prefer 802.11g/b"
	RTSThreshold="RTS Threshold"
	RadioEnableDisable="Radio Enable/Disable"
	Rate="Rate"
	RoamingDecision="Roaming Decision"
	XPress_Technology="XPress (TM) Technology"
	Fast="Fast"
	MinimumPowerConsumption="Minimum Power Consumption"
	AssociationRoamPreference="Association Roam Preference"
	BandPreference="Band Preference"
	RoamingTendency="Roam Tendency"
	Aggressive="Aggressive"
	Moderate="Moderate"
	Conservative="Conservative"
	Aux="Aux"
	Main="Main"
	ApCompatibilityMode="AP Compatibility Mode"
	BroaderCompat="Broader Compatibility"
	HigherPerf="Higher Performance"
	WME="WMM"
	Rate_802_11a="Rate (802.11a)"
	Rate_802_11bg="Rate (802.11b/g)"
	WZC_Managed_Ethernet="WZC Managed Ethernet"
	Legacy="Legacy"
	Manage_Wireless_Settings="Manage Wireless Settings"
	DisableRadioUponWiredConnection="Disable Upon Wired Connect"
	SSIDAutoPromote="SSID Autopromote"
	Loose_11h="Loose 11h"
	Strict_11h="Strict 11h"
	vlan_mode="VLAN Priority Support"
	PriorityVLANTag="Priority & VLAN"
	PriorityAndVLANDisabled="Priority & VLAN Disabled"
	PriorityAndVLANEnabled="Priority & VLAN Enabled"
	PriorityEnabled="Priority Enabled"
	VLANEnabled="VLAN Enabled"
	Lock_Wireless_Settings="Lock Wireless Settings"
	Usebestrate="Best Rate"
	NetPattern="Wake Up Frame"
	Intolerant="40MHz Intolerant"
	All="All"
	LossofAP="LossOfLink"
	Mixed_Mode="Mixed Mode"
	LossNet="WakeUpPkt & LinkLoss"
	OBSSCoex="20/40 Coexistance"
	BandwidthCapability2G="2G Bandwidth Capability"
	autoCountryDiscovery="802.11d Support (Auto-Country)"
	BTAMP="BT-AMP"
	ListenInterval="Assoc Listen Interval"
	D2ListenInterval="D2 Listen Interval"
	WFDChannelNumber="WFD Channel Number"
	EnableLTR="Enable/Disable LTR"
	LTR_ActiveValue="LTR Active value in microseconds"
	WakeOnMagicPacket="Wake On Magic Packet"
	WakeOnPatternMatch="Wake On Pattern Match"
	ARPOffload="ARP Offload"
	NSOffload="NS Offload"
	WiFiRekeyingOffload="WiFi Rekeying Offload"
	PacketCoalescing="Packet Coalescing"
