# Release Notes for
Intel® PROSet/Wireless Advanced Enterprise Software

## Version 18.30 for Windows*

## Note: PROSet Enterprise support has been removed for Windows* 10.

Supported Adapters
Operating Systems
Intel® Centrino® Wireless Bluetooth® High Speed Protocol
Intel® My WiFi Dashboard Software
Viewing User Documentation
Upgrading Drivers and Utilities from Previous Versions
Notes and Recommendations
Customer Support

### Supported Adapters

This version of Intel® PROSet/Wireless WiFi Software is compatible with the adapters listed below. Note that newer features provided in this software release are generally not supported for older, legacy adapters.

The following adapters are supported on this release for Windows* 8 and Windows* 8.1 with Windows* 7 drivers from Intel®:

- Intel® Centrino® Wireless-N 100
- Intel® Centrino® Wireless-N 130
- Intel® Centrino® Wireless-N 1000
- Intel® Centrino® Wireless-N 1030
- Intel® Centrino® Advanced-N 6200
- Intel® Centrino® Advanced-N 6230

The following adapters are supported on this release for Windows* 8 with Windows* 8 drivers from Intel®.

- Intel® Centrino® Wireless-N 105
- Intel® Centrino® Wireless-N 135
- Intel® Centrino® Wireless-N 2200
- Intel® Centrino® Wireless-N 2230
- Intel® Centrino® Wireless-N + WiMAX 6150
- Intel® Centrino® Advanced-N 6205
- Intel® Centrino® Advanced-N 6235
- Intel® Centrino® Advanced-N + WiMAX 6250
- Intel® Centrino® Ultimate-N 6300
- Intel® Dual Band Wireless-AC 7260
- Intel® Dual Band Wireless-N 7260
- Intel® Wireless-N 7260
- Intel® Dual Band Wireless-AC 3160
- Intel® Dual Band Wireless-AC 7265
- Intel® Dual Band Wireless-N 7265
- Intel® Wireless-N 7265
- Intel® Dual Band Wireless-AC 8260

The following adapters are supported on this release for Windows* 8.1 with Windows* 8 drivers from Intel®.

- Intel® Centrino® Wireless-N 105
- Intel® Centrino® Wireless-N 135
- Intel® Centrino® Wireless-N 2200
- Intel® Centrino® Wireless-N 2230
- Intel® Centrino® Wireless-N + WiMAX 6150
- Intel® Centrino® Advanced-N 6205
- Intel® Centrino® Advanced-N 6235
- Intel® Centrino® Advanced-N + WiMAX 6250
- Intel® Centrino® Ultimate-N 6300

The following adapters are supported on this release for Windows* 8.1 with Windows* 8.1 drivers from Intel®.

- Intel® Dual Band Wireless-AC 7260
- Intel® Dual Band Wireless-N 7260
- Intel® Wireless-N 7260
- Intel® Dual Band Wireless-AC 3160
- Intel® Dual Band Wireless-AC 7265
- Intel® Dual Band Wireless-N 7265
- Intel® Wireless-N 7265
- Intel® Dual Band Wireless-AC 8260

The CCX SDK version number for this release is 1.1.13.

### Operating Systems

This version of Intel® PROSet/Wireless WiFi Software runs on Microsoft Windows* 7, Windows* 8, and Windows* 8.1.

### Support for 802.11ac draft specification

This release of Intel® PROSet/Wireless WiFi Software, with the Intel® Dual Band Wireless-AC 7260 adapter, supports the 802.11ac draft specification.

### Intel® Centrino® Wireless Bluetooth® High Speed Protocol

This release of Intel® PROSet/Wireless WiFi Software includes support for Intel® Centrino® Wireless Bluetooth® High Speed Protocol. Bluetooth High Speed Protocol supports theoretical data transfer speeds of up to 24 Mbit/s, using the Bluetooth link for negotiation and establishment and 802.11 link for the high data rate traffic.

### Intel® My WiFi Technology Software

This release of Intel® PROSet/Wireless WiFi Software includes the Intel® My WiFi Technology application. The Intel® My WiFi Technology application uses your Intel wireless WiFi adapter to connect to other devices with Wi-Fi Direct*. You can connect up to eight other devices to your laptop computer, all while maintaining your WiFi wireless connection to the Internet. You can choose to install the Intel® My WiFi Technology application at the Intel® PROSet/Wireless WiFi Software Installer screen. See Known Issues and Limitations in this document for related information.

### Viewing User Documentation

To access user documentation, load the Intel® PROSet/Wireless WiFi Software CD. Click View User Guide on the Intel PROSet/Wireless WiFi Installer screen.

### Upgrading Drivers and Utilities from Previous Versions

When you run the Intel® PROSet/Wireless WiFi Installer program, it replaces all previous versions of 13.x, 14.x, and 15.x of Intel® PROSet/Wireless WiFi Connection Utility with the current version. If you have a version previous to 13.0, you should remove the old version of Intel® PROSet/Wireless WiFi Connection Utility before installing this version. Please visit this site for more information:

- http://www.intel.com/support/go/wireless/w7wirelessinfo.htm

### Notes and Recommendations

#### Recommended Power Save Settings

To optimize power settings, follow the instructions provided at the following support site:

- http://www.intel.com/support/wireless/wlan/sb/CS-024509.htm

#### Recommended Power Configuration

A client disassociates upon moving from hibernation mode when the following conditions are met:

- A client is connected to an 802.1X profile.
- The Power Management setting in the Adapter Settings is configured to "Allow the device to bring the computer out of standby".
- In Windows, the system is configured to move automatically from standby to hibernation in the Power Option Properties.

The recommendation is to set the system hibernate power option to “Never” when the computer is on AC power.

#### Operating in 802.11n Mode

Intel recommends using security with your WiFi network. The 802.11n specification indicates that a compliant adapter can achieve transfer rates greater than 54 Mbps on 802.11n connections only when using AES security or no security. You should only use no security when setting up or troubleshooting the network.

To enable AES for Personal Security, select WPA-Personal (AES-CCMP) or WPA2-Personal (AES-CCMP) in the Security Settings pulldown menu. To enable AES for Enterprise Security, select AES-CCMP in the Data Encryption pulldown menu.

#### Linksys* Access Point Association Timeout

After the association flow completes, the adapter stays awake (as in CAM mode) for 10 seconds, and then acts according to the PowerIndex (PI) regkey. PI should not be change during this period. The association timeout is 10 seconds. Using the Linksys access point, association occurs every 60 seconds, resulting in deauthentication and disconnection from the Linksys access point.

#### Intel® My WiFi Technology Supported Channels

Intel® My WiFi Technology can operate as a hotspot on channels 1-11 of the 2.4GHz band, channels 36, 40, 44, and 48 in the low 5GHz range, and channels 149, 153, 157, 161, and 165 in the high 5GHz range.

#### Intel® My WiFi Dashboard failed to enable due to an unsupported channel

The following message may display: Unable to Connect Invalid Channel.

The computer is currently connected to wireless LAN using a channel that is incompatible with Intel My WiFi Dashboard. To correct this, it is recommended that you change the channel at the access point to match a supported channel listed above.

Another reason for this message may be that this computer and the remote device that you are attempting to connect are both connected to wireless LAN on different channels. You should disconnect your wireless connection and try again.

#### Intel® My WiFi Technology Device Reconnection After Profile Security Changes

In some instances a PDA may fail to immediately reconnect to the My WiFi Technology network after the profile security is changed from one security setting to another.

#### NCPA Platform Wake Configuration for NetDetect

Intel® Smart Connect Technology (iSCT) / NetDetect feature requires the checkboxes on the NCPA Power management tab “Allow this device to wake the computer” and “Only allow a magic packet to wake the computer” to be enabled due to the way that Microsoft implemented the wake function. (To access this tab, open the Device Manager and open Properties for the Intel® wireless adapter. Select the Power Management tab.) Intel® has not implemented support for WoWLAN (Wake over WLAN) in v15.0/15.1 nor is wake via magic packet supported.

#### Wake Enable vs. WoWLAN

This checkboxes on the Power Management tab (described above) do not mean the adapter supports WoWLAN or the platform is able to be configured for WoWLAN feature. Rather the adapter supports Wake Enable. However, the OS enables this check box and allows checking only if the WiFi driver reports it supports WoWLAN.

### Customer Support

Intel web support site: www.intel.com/support/go/wireless/wlan/software/index.htm.

Network products information: http://www.intel.com/network/connectivity/products/wireless/index.htm.

Worldwide access: Intel has technical support centers worldwide. Many of the centers are staffed by technicians who speak the local languages. For a list of all Intel support centers, the telephone numbers, and the times they are open, visit http://www.intel.com/support/feedback.htm.

Information in this document is subject to change without notice.
(c) 2000–2014 Intel Corporation. All rights reserved. Intel Corporation, 5200 N.E. Elam Young Parkway, Hillsboro, OR 97124-6497

Trademark and Disclaimers information: Intel® is a trademark or registered trademark of Intel Corporation or its subsidiaries in the United States and other countries. * Other trademarks and trade names may be used in this document to refer to either the entities claiming the marks and names or their products. Intel disclaims any proprietary interest in trademarks and trade names other than its own.

* Microsoft and Windows are registered trademarks of Microsoft Corporation. Other names and brands may be claimed as the property of others. Intel Corporation assumes no responsibility for errors or omissions in this document, nor does Intel make any commitment to update the information contained herein.

August 19, 2015