**************************************************
* Intel(R) Management Engine Installation Readme
**************************************************

This Readme explains how to choose the appropriate installation package for a platform SKU.

Intel AMT driver for AMT11.6 for Win10 & Win7 operating systems .Supporting Intel(R) ME firmware version: 8 and above

Version:
MEI: 11.6.0.1042
SOL: 11.6.0.1009

Installer Packages:
-------------------
 MEI_SOL Installer
-----------------------
This package installs the Intel(R) ME components without the Intel(R) Management and Security Status Application. Following is a list of the installed components:
* Intel(R) Management Engine Interface (Intel(R) ME Interface)
* Serial Over LAN (SOL) Driver
* Intel(R) Management and Security Status
* Local Manageability Service (LMS)
* User Notification Service (UNS)
* Intel(R) Identity Protection Technology (Intel(R) IPT)
* Intel(R) Dynamic Application Loader (Intel(R) DAL)
==================================================
The required certificates are contained in:
? x86: Update for Root Certificates for Windows 7 [November 2013] (KB931125)
? x64: Update for Root Certificates for Windows 7 for x64-based Systems [November 2013] (KB931125)
? Certificates can be found in http://catalog.update.microsoft.com/v7/site/Search.aspx?q=root%20certificate%20update
=============================================================================
Error code	Error String				Description
0		ERROR_SUCCESS				Operation was successful and a reboot is not needed. Use of the ¨Cb switch will not cause a reboot in this case.
1602		ERROR_INSTALL_USEREXIT			One of:? The user canceled the operation? Setup was run silently but a downgrade was detected and the ¨Coverwrite switch was not used.
1603		ERROR_INSTALL_FAILURE			General failure code. The error could have been an unanticipated error or one of the expected errors such as:? Not admin? No device matches? OS requirement not met? .NET requirement not met
1633		ERROR_INSTALL_PLATFORM_UNSUPPORTED	A device check revealed no matching devices to INF¡¯s in the setup.
1641		ERROR_SUCCESS_REBOOT_INITIATED		A system reboot has been initiated either by the user choosing to ¡°reboot now¡± or the ¨Cb switch was used in silent mode and setup requires a reboot.Note that depending on the OS and platform speed, the calling process may never get this code due to it being terminated as part of the shutdown procedure.
3010		ERROR_SUCCESS_REBOOT_REQUIRED		Successful, but a reboot is required to complete the process.
==============================================================================

Install the Drivers in Microsoft Windows

This will update the drivers for all supported Intel AMT in your system. 
 
Before installing or updating the drivers, insert your adapter(s) in the computer. When Windows discovers the new adapter, it attempts to find an acceptable Windows driver already installed with the operating system.  

If found, the driver is installed without any user intervention. If Windows cannot find the driver, the Found New Hardware Wizard window is displayed.

Regardless of whether or not Windows finds the driver, it is recommended that you follow the procedure below to install the driver. Drivers for all Intel adapters supported by this software release are installed.

If you are installing drivers from the Product CD, insert the CD. If you do not have the Product CD, download drivers from the support website and transfer them to the system.

If the Found New Hardware Wizard screen is displayed, click Cancel.

Start the autorun located on the CD. If you downloaded the software package from the support website, the autorun automatically runs after you have extracted the files.

Click Install Drivers and Software.

Follow the instructions in the install wizard.

===============================================================================
Uninstalling the Driver
These instructions uninstall the drivers for all Intel AMT in a system.

From the Control Panel, double-click Add/Remove Programs.  

Select Intel(R) Management Engine Components

Click Add/Remove.  

When the confirmation dialog displays, click OK.  

===============================================================================
Update the driver
1.  On the desktop, right-click on MY COMPUTER.
2.  Select MANAGE.
3.  In the "Device Manager", double-click Intel(R) Management Engine Interface 
4.  Select DRIVER.
5.  Click UPDATE DRIVER...
6.  Follow the instructions given by the operating system to locate the 
    driver.
7.  If the driver which is found to be the latest is not the one you want to 
    install, select the check box "Install one of the other drivers".
8.  Click NEXT. 
9.  From the driver list, select the driver to be installed.
10. Click NEXT.
11. Click FINISH to complete the installation.

===============================================================================

Silent install:
SetupME.exe /s


After install, please open cdrun folder. Double click cdrun.exe.       

THIS DOCUMENT IS PROVIDED "AS IS" WITHOUT WARRANTY OF ANY KIND. LENOVO
DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS OR IMPLIED, INCLUDING WITHOUT
LIMITATION, THE IMPLIED WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN THIS DOCUMENT.
BY FURNISHING THIS DOCUMENT, LENOVO GRANTS NO LICENSES TO ANY PATENTS OR
COPYRIGHTS.

Copyright (c) Lenovo 2010, all rights reserved
